<template #introduction>

:::info
The CTCISZ 2K0300 ForeverPi is a development board based on Loongson 2K0300.

ForeverPi ships in "TF Card" and "Wi-Fi" versions - as both the Wi-Fi module amd microSD (TF) card slot uses the SDIO bus, only one may be equipped at a time. The Wi-Fi version comes additionally with 4GB of eMMC storage and an LCD interface, and the onboard NOR Flash capacity is larger (8Mbit on the "Wi-Fi" version and "256Mbit" on the "TF Card" version).
:::

</template>

<template #spec>

### Wi-Fi Version

| Category | Specification |
| ---- | ---- |
| Manufacturer | CTCISZ |
| Form Factor | 88×56mm |
| Processor | 2K0300 @ 1.0GHz |
| Memory | 512MiB DDR4 @ 2666MT/s (onboard) |
| Interfaces (USB) | 2 × USB 2.0 |
| Interfaces (Storage) | 4GB eMMC (onboard), 8Mbit NOR Flash |
| Interfaces (Network) | 1 × GbE, onboard Wi-Fi + Bluetooth module (single antenna) |
| Interfaces (Video) | 1 × LCD output |
| Interfaces (Other) | 8 × 12-bit ADC, 1 × JTAG, 40-pin GPIO |

### TF Card Version

| Category | Specification |
| ---- | ---- |
| Manufacturer | CTCISZ |
| Form Factor | 88×56mm |
| Processor | 2K0300 @ 1.0GHz |
| Memory | 512MiB DDR4 @ 2666MT/s (onboard) |
| Interfaces (USB) | 2 × USB 2.0 |
| Interfaces (Storage) | 256Mbit NOR Flash |
| Interfaces (Network) | 1 × GbE |
| Interfaces (Video) | None |
| Interfaces (Other) | 8 × 12-bit ADC, 1 × JTAG, 40-pin GPIO |

</template>

<template #known-issues>

None noted.

</template>

<template #image>

(Coming Soon)

</template>
