<template #introduction>

:::info
The OrangePi Nova v1.1 is a Nano-ITX (120×120mm) motherboard based on Loongson 2K3000.
:::

</template>

<template #spec>

| Category | Specification |
| ---- | ---- |
| Manufacturer | Xunlong Software (OrangePi) |
| Form Factor | Nano-ITX (120×120mm) |
| Processor | 2K3000 @ 2.2GHz |
| Memory | DDR4 @ 3200MT/s (onboard) |
| Interfaces (USB) | 4 × USB 3.0, 2 × USB 2.0 |
| Interfaces (Storage) | 1 × NVMe (PCIe 3.0 x4), 1 × microSD card slot, 32GB eMMC (onboard) |
| Interfaces (Network) | 1 × 2.5GbE (Realtek RTL8125), 1 × GbE |
| Interfaces (Video) | 1 × HDMI, 1 × MIPI (30-pin), 1 × eDP |
| Interfaces (Other) | 1 × m.2 Key E interface (PCIe + USB), 1 × 3.5mm headphone/microphone jack, 1 × CPU UART, 1 × SE UART, 40-pin GPIO |

</template>

<template #known-issues>

None noted.

</template>

<template #image>

[![Front-side photo of an OrangePi Nova v1.1](/images/devices/opi-nova-v1.1-front.thumbnail.webp)](/images/devices/opi-nova-v1.1-front.webp)
Source: [深圳市迅龙软件有限公司](http://www.orangepi.cn/)

[![Back-side photo of an OrangePi Nova v1.1](/images/devices/opi-nova-v1.1-back.thumbnail.webp)](/images/devices/opi-nova-v1.1-back.webp)
Source: [深圳市迅龙软件有限公司](http://www.orangepi.cn/)

</template>

<template #download-notes>

:::tip
Daily firmware updates provided by the community: https://fw.loongfans.cn/opi-nova-v1.1/
:::

</template>
