# Partial audio pipeline with custom read callback registered by the application.

The demo plays a MP3 stored on the SD card using an application specified custom callback. 

To run this example you need ESP32 LyraT or compatible board:

- Connect speakers or headphones to the board. 
- Insert a microSD card loaded with a MP3 file 'test.mp3' into board's slot.
