# Page 341–344 of 434

> **Source:** ASD-STE100 Issue 9, January 2025
> **Pages:** 341–344 of 434

# Page 341 of 434

| **Word**<br>**(part of speech)** | **Approved meaning/**<br>**ALTERNATIVES** | **STE EXAMPLE** | **Non-STE example** |
|---|---|---|---|
| re- (prefix) — UNNAPPROVED | In general, use<br>the word AGAIN<br>(adv) or BACK<br>(adv) with the<br>basic word to<br>replace words<br>that have "re-" as<br>a prefix. |  |  |
| reach (v) — UNNAPPROVED | GET (v)<br><br>TOUCH (v)<br><br>BE (v) | WHEN YOU GET THE<br>CORRECT PRESSURE,<br>CLOSE THE VALVE.<br><br>MAKE SURE THAT THE<br>EXTENSION BAR<br>TOUCHES THE<br>TARGET PLATE.<br><br>WHEN THE FLAPS ARE<br>AT THE 30 DEGREE<br>POSITION, INSTALL<br>THE RIGGING PIN. | When the correct<br>pressure is reached,<br>close the valve.<br><br>Make sure that the<br>extension bar reaches<br>the target plate.<br><br>When the flaps reach the<br>30 degree position,<br>install the rigging pin. |
| reactivate (v) — UNNAPPROVED | ACTIVATE (v) | ACTIVATE THE MODE<br>AGAIN. | Reactivate the mode. |
| READ (v),<br>READS,<br>READ,<br>READ | To come to know<br>information with the eyes<br>or electronically | READ THE<br>INDICATORS ON THE<br>CONTROL PANEL. |  |
| reading (n) — UNNAPPROVED | INDICATION (n) | MAKE SURE THAT THE<br>EXHAUST FROM THE<br>GROUND CART DOES<br>NOT CAUSE AN<br>INCORRECT<br>INDICATION. | Avoid an erroneous<br>reading caused by<br>exhaust from ground<br>cart. |
| readjust (v) — UNNAPPROVED | ADJUST (v) | AFTER THE<br>INSPECTION, ADJUST<br>THE LINKAGE AGAIN. | Readjust the linkage<br>after the inspection. |
| ready (adj) — UNNAPPROVED | PREPARE (v) | MAKE SURE THAT THE<br>CONTROL SYSTEM IS<br>PREPARED FOR<br>OPERATION. | Make sure that the<br>control system is in an<br>operational ready state. |
| ready (v) — UNNAPPROVED | PREPARE (v) | PREPARE THE<br>REMOVAL KIT FOR<br>THE REMOVAL OF THE<br>STRUT. | Ready the removal kit for<br>the removal of the strut. |

# Page 342 of 434

| **Word**<br>**(part of speech)** | **Approved meaning/**<br>**ALTERNATIVES** | **STE EXAMPLE** | **Non-STE example** |
|---|---|---|---|
| real (adj) — UNNAPPROVED | AGREE (v) | MAKE SURE THAT THE<br>INDICATION ON THE<br>GAUGE AGREES WITH<br>THE QUANTITY OF<br>FUEL THAT IS IN THE<br>TANK. | Make sure that the<br>gauge shows the real<br>quantity of fuel that is in<br>the tank. |
| REAR (adj) | Away from the person<br>who looks or from a<br>reference point | INSTALL THE TWO<br>BOLTS IN THE REAR<br>FITTINGS. |  |
| REAR (n) | The rear part or rear<br>surface | THE CIRCUIT<br>BREAKERS ARE<br>INSTALLED ON THE<br>REAR OF THE UNIT. |  |
| rear of (prep) — UNNAPPROVED | AFT OF<br><br>BEHIND (prep) | THE PUMP IS<br>INSTALLED ON RIB 3,<br>AFT OF THE FRONT<br>SPAR.<br><br>THE PUMP IS<br>INSTALLED ON RIB 3,<br>BEHIND THE FRONT<br>SPAR. | The pump is located on<br>rib 3, rear of the front<br>spar.<br><br>The pump is located on<br>rib 3, rear of the front<br>spar. |
| rearmost (adj) — UNNAPPROVED | REAR (n) | YOU CANNOT<br>REMOVE THE HALF<br>CLAMP NEAREST TO<br>THE REAR. | The rearmost half clamp<br>is not removable. |
| REARWARD (adv) | In the direction of the<br>rear | PULL THE LEVER<br>REARWARD. |  |
| reason (n) — UNNAPPROVED | CAUSE (n)<br><br>BECAUSE OF (prep) | FIND THE CAUSE OF<br>THE INCORRECT<br>INDICATION.<br><br>BECAUSE OF THE<br>POSSIBLE EFFECTS<br>ON YOUR HEALTH,<br>USE ONLY POTABLE<br>WATER. | Find the reason for the<br>wrong indication.<br><br>For health reasons, only<br>use potable water. |
| reassemble (v) — UNNAPPROVED | ASSEMBLE (v) | ASSEMBLE THE<br>ACTUATOR AGAIN. | Reassemble the<br>actuator. |
| rebuild (v) — UNNAPPROVED | ASSEMBLE (v) | ASSEMBLE THE UNIT<br>AGAIN. | Rebuild the unit. |

# Page 343 of 434

| **Word**<br>**(part of speech)** | **Approved meaning/**<br>**ALTERNATIVES** | **STE EXAMPLE** | **Non-STE example** |
|---|---|---|---|
| RECEIVE (v),<br>RECEIVES,<br>RECEIVED,<br>RECEIVED | To get energy, material,<br>or a signal from a<br>different source | MAKE SURE THAT THE<br>CAPTAIN'S BOOMSET<br>RECEIVES THE<br>SIGNALS CORRECTLY. |  |
| RECESS (n) | An indentation in a<br>surface | WHEN YOU CLEAN<br>THE SURFACES,<br>REMOVE THE STAINS<br>FROM THE<br>RECESSES. |  |
| recess (v) — UNNAPPROVED | RECESS (n) | DO NOT MAKE A<br>RECESS OF MORE<br>THAN 5 mm FOR THE<br>STUDS.<br><br>THE FLANGE IS IN A<br>RECESS IN THE<br>FUSELAGE. | Do not recess studs<br>more than 5 mm.<br><br>The flange is recessed<br>into the fuselage. |
| recharge (v) — UNNAPPROVED | CHARGE (v)<br><br>FILL (v)<br><br>PRESSURIZE (v) | CHARGE THE<br>BATTERY AGAIN.<br><br>FILL THE FLUID<br>RESERVOIR.<br><br>PRESSURIZE THE<br>ACCUMULATOR. | Recharge the battery.<br><br>Recharge the fluid<br>reservoir.<br><br>Recharge the<br>accumulator. |
| recheck (v) — UNNAPPROVED | MEASURE (v)<br><br>EXAMINE (v)<br><br>CHECK (n) | MEASURE THE<br>DISTANCE BETWEEN<br>THE FACES AGAIN.<br><br>EXAMINE THE<br>CASTING FOR<br>CORROSION AGAIN.<br><br>DO A LEAKAGE<br>CHECK OF THE<br>FILTER ASSEMBLY<br>AGAIN. | Recheck the distance<br>between the faces.<br><br>Recheck the casting for<br>corrosion.<br><br>Recheck the filter<br>assembly for leakage. |
| reclaim (v) — UNNAPPROVED | REPAIR (v) | REPAIR THE<br>DAMAGED FABRIC<br>AREA. | Reclaim the damaged<br>fabric area. |
| recleat (v) — UNNAPPROVED | ATTACH (v)<br>(TO A CLEAT [TN]) | ATTACH THE<br>TIEDOWN CORD TO A<br>CLEAT. | Recleat the tiedown<br>cord. |
| reclose (v) — UNNAPPROVED | CLOSE (v) | AFTER SERVICING,<br>CLOSE THE<br>COMPARTMENT<br>AGAIN. | Reclose the<br>compartment after<br>servicing. |

# Page 344 of 434

| **Word**<br>**(part of speech)** | **Approved meaning/**<br>**ALTERNATIVES** | **STE EXAMPLE** | **Non-STE example** |
|---|---|---|---|
| recoil (v) — UNNAPPROVED | MOVE BACK<br><br>WIND (v)<br><br>RECOIL (TN) | BE CAREFUL WHEN<br>THE SLIDE MOVES<br>BACK.<br><br>WIND THE PROBE<br>WIRE BACK ON THE<br>SPOOL.<br><br>THE GUN BARREL HAS<br>A QUICK RECOIL. | Be careful when the<br>slide recoils.<br><br>Recoil the probe wire<br>back on the spool.<br><br>The gun barrel recoils<br>quickly. |
| RECOMMEND (v),<br>RECOMMENDS,<br>RECOMMENDED,<br>RECOMMENDED | To advise that which is<br>best | THE MANUFACTURER<br>RECOMMENDS THAT<br>YOU KEEP THE UNIT<br>IN A DEDICATED<br>AREA. |  |
| recondition (v) — UNNAPPROVED | REPAIR (v)<br><br>OVERHAUL (TN) | REPAIR THE SEATS.<br><br>DO AN OVERHAUL OF<br>THE ENGINE. | Recondition the seats.<br><br>Recondition the engine. |
| reconstruction (n) — UNNAPPROVED | REPAIR (n)<br><br>REPAIR (v) | RECORD ALL REPAIRS<br>TO THE SKIN<br>SURFACE.<br><br>THIS PROCEDURE<br>TELLS YOU HOW TO<br>REPAIR THE<br>SURFACE. | Record all reconstruction<br>of the skin surface.<br><br>This procedure is for the<br>reconstruction of the<br>surface. |
| RECORD (v),<br>RECORDS,<br>RECORDED,<br>RECORDED | 1.<br>To make notes of<br>and keep data to<br>use subsequently<br><br>2.<br>To put data on a<br>storage medium | RECORD THE<br>RESULTS.<br><br>THE COCKPIT VOICE<br>RECORDER RECORDS<br>SIGNALS FROM FOUR<br>AUDIO INPUTS<br>DURING THE FLIGHT. |  |
| recover (v) — UNNAPPROVED | COLLECT (v) | REMOVE THE NUT<br>AND THE BOLT. THEN,<br>COLLECT THE<br>WASHER. | Remove the nut and the<br>bolt. Then, recover the<br>washer. |
| rectify (v) — UNNAPPROVED | CORRECT (v) | BEFORE YOU START<br>THE PROCEDURE<br>AGAIN, CORRECT THE<br>DEFECT. | Rectify the defect before<br>you restart the<br>procedure. |
| recur (v) — UNNAPPROVED | OCCUR (v) | IF THE SYMPTOMS<br>OCCUR AGAIN, DO A<br>SYSTEM TEST. | If the symptoms recur,<br>do a system test. |
