# Page 361 of 434

**Page 2-1-S3**

**Issue 9 2025-01-15**

**Part 2 - Dictionary**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
|---|---|---|---|---|
|**secure (adj) — UNNAPPROVED**|TIGHT (adj)|MAKE SURE THAT THE<br>BOLTS ARE TIGHT.|Make sure that the bolts<br>are secure.|
|||SAFE (adj)|BEFORE YOU LIFT<br>THE PLATFORM, MAKE<br>SURE THAT IT IS<br>SAFE.|Make sure that the<br>platform is secure before<br>you lift it.|
|||CORRECTLY (adv)|MAKE SURE THAT THE<br>BRACKETS ARE<br>CORRECTLY<br>ATTACHED.|Check the brackets for<br>secure attachment.|
|**secure (v) — UNNAPPROVED**|ATTACH (v)|REMOVE THE BOLTS<br>THAT ATTACH THE<br>UNIT.|Remove the bolts that<br>secure the unit.|
|||SAFETY (v)|SAFETY THE PULLEY<br>GUARD PINS WITH<br>SPLIT PINS.|Secure the pulley guard<br>pins with split pins.|
|**securely (adv) — UNNAPPROVED**|CORRECTLY (adv)|MAKE SURE THAT THE<br>BRACKETS ARE<br>CORRECTLY<br>ATTACHED.|Make sure that the<br>brackets are securely<br>attached.|
|||SAFELY (adv)|MAKE SURE THAT THE<br>LADDER IS SAFELY<br>ATTACHED.|Make sure the ladder is<br>securely attached.|
|||TIGHT (adj)|MAKE SURE THAT THE<br>BOLTS ARE TIGHT.|Make sure that the bolts<br>are securely installed.|
|**security (n) — UNNAPPROVED**|CORRECTLY (adv)|MAKE SURE THAT THE<br>COMPONENTS ARE<br>CORRECTLY<br>ATTACHED.|Check the security of the<br>components.|

# Page 362 of 434

**Page 2-1-S4**

**Part 2 - Dictionary**

**Issue 9 2025-01-15**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
|---|---|---|---|---|
|**SEE (v),**<br>**SEES,**<br>**SAW,**<br>**SEEN**|To know with the eyes|MAKE SURE THAT<br>YOU CAN SEE THE<br>CABLE THROUGH THE<br>INSPECTION HOLE.||
|||For other<br>meanings, use:<br>REFER (v)|REFER TO TABLE 8001<br>FOR THE APPLICABLE<br>TORQUE VALUES.|See Table 8001 for the<br>applicable torque values.|
|||EXAMINE (v)|EXAMINE THE<br>MEMBRANE FOR<br>HOLES.|Check the membrane to<br>see if there are holes.|
|||MAKE SURE (v)|MOVE THE TUBE TO<br>MAKE SURE THAT ITS<br>INNER CONNECTION<br>IS TIGHT.|Move the tube to see if<br>its inner connection is<br>tight.|
|**seek (v) — UNNAPPROVED**|GET (v)|GET MEDICAL AID<br>IMMEDIATELY.|Seek medical attention<br>immediately.|
|**seepage (n) — UNNAPPROVED**|LEAKAGE (n)|CLEAN THE AREAS<br>WHERE THERE IS<br>HYDRAULIC FLUID<br>LEAKAGE.|Clean the areas where<br>there is hydraulic fluid<br>seepage.|
|**seized (adj) — UNNAPPROVED**|CATCH (v)|IF THE CONTROL<br>CABLE IS CAUGHT IN<br>THE PULLEY,<br>RELEASE THE CABLE<br>TENSION.|If the control cable is<br>seized in the pulley,<br>release the cable<br>tension.|
|||MOVE (v)|IF YOU CANNOT MOVE<br>THE BOLTS, APPLY<br>SOME PENETRATING<br>OIL.|If the bolts are seized,<br>apply some penetrating<br>oil.|
|||TURN (v)|IF THE FLAP CONTROL<br>MOTOR CANNOT<br>TURN, USE THE<br>ALTERNATIVE MODE.|If the flap control motor<br>is seized, use the<br>alternate mode.|

# Page 363 of 434

**Page 2-1-S5**

**Issue 9 2025-01-15**

**Part 2 - Dictionary**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
|---|---|---|---|---|
|**SELECT (v),**<br>**SELECTS,**<br>**SELECTED,**<br>**SELECTED**|To make a choice|SELECT THE<br>HYDRAULIC SYSTEM<br>THAT YOU WILL<br>PRESSURIZE.||
|||SELECT A LANGUAGE<br>FROM THE MENU.||
|||Do not use this<br>word as a<br>synonym for<br>SET (v).|SET THE SWITCH TO<br>"TEST."|Select the switch to<br>TEST.|
|**SELECTION (n)**|The action or result of<br>choosing|THE OPERATION OF<br>THE INDICATOR DOES<br>NOT PREVENT THE<br>SELECTION OF<br>SYSTEM 1.||
|**SEMICIRCULAR**<br>**(adj)**|That has the shape of<br>half a circle|THE VALVE FLAPS<br>ARE SEMICIRCULAR.||
|**SEND (v),**<br>**SENDS,**<br>**SENT,**<br>**SENT**|To cause to go|SEND THE FILTER<br>ELEMENT TO THE<br>MAINTENANCE SHOP<br>FOR THE NECESSARY<br>INSPECTION.||
|**SENSE (v),**<br>**SENSES,**<br>**SENSED,**<br>**SENSED**|To get an input<br>automatically|THE TEMPERATURE<br>BULB SENSES THE<br>EXTERNAL AIR<br>TEMPERATURE.||
|**SENSITIVE (adj)**|That can sense small<br>changes|THE CAPSULE IS<br>SENSITIVE TO<br>PRESSURE CHANGES.||
|**separable (adj) — UNNAPPROVED**|DISASSEMBLE (v)|YOU CAN<br>DISASSEMBLE THIS<br>UNIT INTO TWO<br>PARTS.|This unit is separable<br>into two parts.|
|||DISCONNECT (v)|YOU CAN<br>DISCONNECT THESE<br>LINE FITTINGS.|These line fittings are<br>separable.|

# Page 364 of 434

**Page 2-1-S6 Part 2 - Dictionary**

**Issue 9 2025-01-15**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
|---|---|---|---|---|
|**separate (adj) — UNNAPPROVED**|ISOLATED (adj)|EACH HYDRAULIC<br>SYSTEM IS FULLY<br>ISOLATED.|All hydraulic systems are<br>completely separate.|
|||DIFFERENT (adj)|PUT THE REMAINING<br>PARTS IN A<br>DIFFERENT<br>CONTAINER.|Put the remaining parts<br>in a separate container.|
|||NOT CONNECTED|THESE TWO TRACKS<br>ARE NOT CONNECTED<br>TO THE OTHER TWO.|These two tracks are<br>separate from the other<br>two.|
|||NOT ATTACHED|THE CAP IS NOT<br>ATTACHED TO THE<br>COUPLING.|The cap is separate from<br>the coupling.|
|**separate (v) — UNNAPPROVED**|DISCONNECT (v)|DISCONNECT THE<br>LINE FITTINGS.|Separate the line fittings.|
|||DIVIDE (v)|YOU CAN DIVIDE THE<br>DRAINS INTO THREE<br>GROUPS.|You can separate the<br>drains into three groups.|
|**separately (adv) — UNNAPPROVED**|INDEPENDENTLY (adv)|THE SYSTEM<br>MONITORS THE<br>CONDITION OF THE<br>PARTS<br>INDEPENDENTLY.|The system monitors the<br>condition of the parts<br>separately.|
|**SEPARATION (n)**|The action or result of<br>separating|SEPARATION OF<br>THESE PARTS IS NOT<br>EASY.||
|**SEQUENCE (n)**|The relation of items that<br>follow one after the other<br>in a list or the relation of<br>steps or events that<br>occur one after the other<br>in time|TIGHTEN THE BOLTS<br>IN THE SEQUENCE<br>THAT IS GIVEN IN<br>FIGURE 3.||
|**serious (adj) — UNNAPPROVED**|IMPORTANT (adj)|VIRUS<br>CONTAMINATION IS<br>AN IMPORTANT<br>PROBLEM.|Virus contamination is a<br>serious problem.|
|||DANGEROUS (adj)|HYDRAULIC FLUID IS<br>DANGEROUS FOR<br>YOUR EYES.|Hydraulic fluid can cause<br>serious eye injury.|
