# Page 317 of 434

**Page 2-1-O7**

**Page 2-1-O7**

**Issue 9 2025-01-15**

**Part 2 - Dictionary**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**||---|---||**outside (adv) — UNNAPPROVED**|OUTDOORS (adv)|DO THIS PROCEDURE<br>OUTDOORS.|Do this procedure<br>outside.||**outside (n) — UNNAPPROVED**|EXTERNAL (adj)|FOLD THE EDGING<br>AGAINST THE<br>EXTERNAL SIDE OF<br>THE INSULATION<br>BLANKET.|Fold the edging against<br>the outside of the<br>insulation blankets.||
|OUTER (adj)|FOLD THE EDGING<br>AGAINST THE OUTER<br>SIDE OF THE<br>INSULATION BLANKET.|
|Fold the edging against<br>the outside of the<br>insulation blankets.||**outside (prep) — UNNAPPROVED**|NEAR (prep)|WHEN YOU DO WORK<br>IN A FUEL TANK, A<br>SECOND PERSON<br>MUST BE NEAR THE<br>TANK AT ALL TIMES.|When you do work in a<br>fuel tank, a second<br>person must be outside<br>the tank at all times.||**outwards (adv) — UNNAPPROVED**|OUT (adv)|MOVE THE DOOR OUT<br>AND FORWARD.|Move the door outwards<br>and forwards.||**over (prep) — UNNAPPROVED**|ABOVE (prep)|MAKE SURE THAT THE<br>HYDRAULIC FLUID<BR>LEVEL IS NOT ABOVE<BR>THE "FULL" MARK.|
|Make sure the hydraulic<br>fluid level is not over the<br>FULL mark.||
|ALONG (prep)|APPLY THE WEIGHT<BR>EQUALLY ALONG THE<BR>STABILIZER SPAN.|The weight must be<BR>evenly spread over the<BR>stabilizer span.|||ON (prep)|INSTALL THE STOP<BR>SLEEVE ON THE<BR>SLIDING MEMBER.|Install the stop sleeve<BR>over the sliding member.||
|MORE THAN|DO NOT INSTALL<BR>SHIMS WITH A<BR>THICKNESS OF MORE<BR>THAN 0.1 mm.|Do not install shims over<BR>0.1 mm thick.||
|For movement<br>above land or<br>water, use a<br>technical noun.|BEFORE OVER-<BR>WATER OPER_A_TION<BR>AT LOW ALTITUDES,<BR>APPLY CORROSION-<BR>PREVENTIVE FLUID<BR>TO THE DOOR HINGES<BR>OF THE LANDING<BR>GEAR.||

# Page 318 of 434

**Page 2-1-O8**

**Page 2-1-O8 Part 2 - Dictionary**

**Issue 9 2025-01-15**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**||---|---||**OVERBOARD**<br>**(adv)**|Out of a vessel|RELEASE THE AIR<BR>OVERBOARD.|||**overfill (v) — UNNAPPROVED**|TOO MUCH|DO NOT PUT TOO<BR>MUCH FLUID IN THE<BR>LUBRICATION HOLE.|Do not overfill the<BR>lubrication hole.||**overfull (adj) — UNNAPPROVED**|TOO FULL|IF THE TANK IS TOO<BR>FULL, YOU CANNOT<BR>PRESSURIZE IT<BR>CORRECTLY.|If the tank is overfull, you<BR>cannot pressurize it<BR>correctly.||**overhaul (v) — UNNAPPROVED**|OVERHAUL (TN)|DO AN OVERHAUL OF<BR>THE No. 2 ENGINE.|Overhaul the No. 2<BR>engine.||**overheat (v) — UNNAPPROVED**|TOO HOT|IF YOU PRESSURIZE<BR>THE OXYGEN BOTTLE<BR>QUICKLY, IT WILL<BR>BECOME TOO HOT.|Rapid charging<BR>overheats the oxygen<BR>bottle.||**OVERLAP (n)**|The area in which a part<BR>of one surface is on a<BR>part of a second surface|IF THE OVERLAP IS<BR>MORE THAN 0,01 mm,<BR>REPLACE THE PART.|||**overlap (v) — UNNAPPROVED**|OVERLAP (n)|MAKE AN OVERLAP<BR>OF 10 mm.|Overlap the surfaces by<BR>10 mm.||**OVERRIDE (v),**<br>**OVERRIDES,**<br>**OVERRODE,**<br>**OVERRIDDEN**|To prevent the automatic<BR>operation of a part or<BR>system|MANUALLY OVERRIDE<BR>THE START<BR>SEQUENCE.|||**overtighten (v) — UNNAPPROVED**|TIGHTEN TOO MUCH|DO NOT TIGHTEN THE<BR>FITTINGS TOO MUCH.|Do not overtighten the<BR>fittings.||
|TOO TIGHT|DO NOT MAKE THE<BR>FITTINGS TOO TIGHT.|
|Do not overtighten the<BR>fittings.|||TOO TIGHTLY|DO NOT INSTALL THE<BR>FITTINGS TOO<BR>TIGHTLY.|
|Do not overtighten the<BR>fittings.||

# Page 319 of 434

**Page 2-1-O9**

**Page 2-1-O9**

**Issue 9 2025-01-15**

**Part 2 - Dictionary**

**ASD-STE100 Simplified Technical English**

**Word** **Approved meaning/ (part of speech) ALTERNATIVES STE EXAMPLE**

**Non-STE example**

Blank Page

# Page 320 of 434

**Page 2-1-O10**

**Page 2-1-O10**

**Part 2 - Dictionary**

**Issue 9 2025-01-15**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**||---|---||**pack (v) — UNNAPPROVED**|PUT (v)|PUT THE ASSEMBLY<BR>INTO THE BOX.|Pack the assembly into<BR>the box.|||
|FILL (v)|FILL THE GROOVE<BR>WITH GREASE.|
|Pack grease into the<BR>groove.|||**PAINT (v),**<br>**PAINTS,**<br>**PAINTED,**<br>**PAINTED**|To apply paint to<BR>something|PAINT ALL THE<BR>SURFACES.|||**PAIR (n)**|Two objects that are the<BR>same or almost the<BR>same, and/or that you<BR>use together|MEASURE THE<BR>DISTANCE BETWEEN<BR>EACH PAIR OF AXLES.|||**PARALLEL (adj)**|Along lines that stay a<BR>constant distance apart<BR>at all points|MAKE SURE THAT THE<BR>SURFACE IS<BR>PARALLEL TO THE<BR>AXIS OF THE SHAFT.|||**PARK (v),**<br>**PARKS,**<br>**PARKED,**<br>**PARKED**|To stop a vehicle and to<BR>let it stay in one position<BR>on the ground|PARK THE CAR IN THE<BR>PERMITTED AREA.|||**PART (n)**|1.<br>A constituent of an<BR>object, machine,<BR>component,<BR>assembly, or<BR>equipment|REPLACE THE<BR>DEFECTIVE PARTS.|||
|2.<br>A piece or section of<BR>a whole|REFER TO PART 2<BR>FOR THE APPLICABLE<BR>PROCEDURE.|||**part (v) — UNNAPPROVED**|DISCONNECT (v)|DISCONNECT THE<BR>PIPES.|Part the pipes.||**partial (adj) — UNNAPPROVED**|NOT FULLY|IF THE RODS DO NOT<BR>FULLY EXTEND,<BR>ADJUST THEM AGAIN.|If only partial extension<BR>of the rods occurs, do<BR>the adjustment again.||**partially (adv) — UNNAPPROVED**|NOT FULLY|IF THE FLAPS DO NOT<BR>FULLY EXTEND, DO<BR>THE TEST AGAIN.|If the flaps only partially<BR>extend, do the test<BR>again.||**PARTICLE (n)**|A very small piece of<BR>material|IF THERE ARE METAL<BR>PARTICLES IN THE<BR>DISASSEMBLED<BR>PUMP, FIND THE<BR>SOURCE OF<BR>CONTAMINATION.|

**Issue 9 2025-01-15**

**Part 2 - Dictionary**
