# Page 305–308 of 434

> **Source:** ASD-STE100 Issue 9, January 2025
> **Pages:** 305–308 of 434

# Page 305 of 434

| **Word**<br>**(part of speech)** | **Approved meaning/**<br>**ALTERNATIVES** | **STE EXAMPLE** | **Non-STE example** |
|---|---|---|---|
| **MOVE (v),**<br>**MOVES,**<br>**MOVED,**<br>**MOVED** | To change or cause to<br>change position or<br>location | MAKE SURE THAT THE<br>POINTER MOVES<br>FREELY.<br>MOVE THE VALVE<br>UNTIL IT ALIGNS WITH<br>THE ACTUATOR<br>SHAFT. |  |
| **MOVEMENT (n)** | A change of position or<br>location | SUDDEN OPERATION<br>OF THE GYRO CAN<br>CAUSE UNWANTED<br>MOVEMENT OF THE<br>HORIZONTAL<br>STABILIZER. |  |
| **MUCH (adj)**<br>**(MORE, MOST)** | Of relatively large<br>dimension, value,<br>quantity, or volume | DO NOT APPLY TOO<br>MUCH PRESSURE. |  |
| **MUCH (adv)** | To a great degree or<br>extent | BE CAREFUL THAT<br>YOU DO NOT TURN<br>THE INNER RACES<br>TOO MUCH. |  |
| **MULTIPLY (v),**<br>**MULTIPLIES,**<br>**MULTIPLIED,**<br>**MULTIPLIED** | To use multiplication to<br>get a result<br>For other<br>meanings, use:<br>INCREASE (v) —<br>THE NUMBER OF<br>CRACKS CAN<br>INCREASE. | MULTIPLY THE<br>INDICATOR VALUE BY<br>THE SCALE VALUE. | Cracks can multiply. |
| **MUST (v)** | Auxiliary modal verb that<br>shows obligation | THE BAT 1 SWITCH<br>MUST BE IN THE ON<br>POSITION. |  |

# Page 306 of 434

| **Word**<br>**(part of speech)** | **Approved meaning/**<br>**ALTERNATIVES** | **STE EXAMPLE** | **Non-STE example** |
|---|---|---|---|
| **NAME (n)** | The identification you<br>give to a person or an<br>object | PUSH THE BUTTON<br>ADJACENT TO THE<br>NAME OF THE<br>SYSTEM.<br>WRITE YOUR NAME<br>ON THE<br>REGISTRATION FORM. |  |
| **NEAR (adj)**<br>**(NEARER,**<br>**(NEAREST)** | At or to a relatively short<br>distance | PUT THE SYRINGE ON<br>THE NEAREST<br>SURFACE OF THE<br>EXAMINATION TABLE. |  |
| **NEAR (prep)** | Approaching in space or<br>condition | BALANCE THE<br>ELEVATOR NEAR ITS<br>MAXIMUM LIMIT.<br>MAKE SURE THAT THE<br>COMPUTER SCREEN<br>IS NOT NEAR THE<br>WINDOW. |  |
| **nearly (adv) — UNNAPPROVED** | ALMOST (adv) | MOVE THE POINTER<br>UNTIL IT IS ALMOST IN<br>THE GREEN BAND. | Move the pointer until<br>nearly in the green band. |
| **NECESSARY (adj)** | That must be | TWO HOURS ARE<br>NECESSARY TO<br>COMPLETE THE<br>EXAM. |  |
| **need (v) — UNNAPPROVED** | NECESSARY (adj) | DURING THIS<br>PROCEDURE, IT IS<br>NOT NECESSARY TO<br>REPLACE THE<br>BACKING RINGS. | The backing rings do not<br>need to be replaced<br>during this procedure. |
| **neither (adj) — UNNAPPROVED** | TWO (TN) … NOT | THE TWO UNITS MUST<br>NOT OPERATE. | Neither unit must<br>operate. |
| **neither (pron) — UNNAPPROVED** | TWO (TN) … NOT | THE TWO UNITS MUST<br>NOT OPERATE. | Neither of the units must<br>operate. |
| **NEUTRAL (adj)** | 1.<br>That has no effect<br>2.<br>That is not acid or<br>alkaline | MAKE SURE THAT THE<br>CONTROLS ARE IN<br>THE NEUTRAL<br>POSITION.<br>CLEAN THE SCREEN<br>WITH A NEUTRAL<br>SOLUTION. |  |

# Page 307 of 434

| **Word**<br>**(part of speech)** | **Approved meaning/**<br>**ALTERNATIVES** | **STE EXAMPLE** | **Non-STE example** |
|---|---|---|---|
| **neutralize (v) — UNNAPPROVED** | NEUTRAL (adj) | MAKE THE BASIC<br>ELECTROLYTE<br>NEUTRAL WITH<br>VINEGAR OR BORIC<br>ACID. | Neutralize the basic<br>electrolyte with vinegar<br>or boric acid. |
| **never (adv) — UNNAPPROVED** | DO NOT | DO NOT LET THE<br>LEVEL IN THE TANK<br>DECREASE TO LESS<br>THAN HALF. | Never allow the level in<br>the tank to drop below<br>half. |
| **NEW (adj)**<br>**(NEWER,**<br>**(NEWEST)** | Not used before | INSTALL A NEW<br>GASKET ON THE<br>FLANGE. |  |
| **NEXT (adj)** | The first occurrence that<br>follows immediately after<br>in time or sequence. | REMOVE THE UNIT<br>BEFORE THE NEXT<br>OPERATING CYCLE. |  |
| **next (adv) — UNNAPPROVED** | THEN (adv) | HOLD THE FLANGE IN<br>ITS POSITION. THEN,<br>INSTALL THE BOLT. | Hold the flange in its<br>position. Next, install the<br>bolt. |
| **next to (prep) — UNNAPPROVED** | ADJACENT TO (prep) | THE PUMP IS<br>ADJACENT TO THE<br>CENTRAL RIB. | The pump is next to the<br>central rib. |
| **NO (adj)** | Not any | MAKE SURE THAT<br>THERE IS NO FUEL<br>LEAKAGE. |  |
| **NO (adv)** | Function word that<br>shows the negative<br>answer to a question | DOES THE LIGHT<br>COME ON?<br>YES OR NO? |  |
| **NOISE (n)** | An unwanted sound | WHILE THE ENGINE<br>CONTINUES TO TURN,<br>LISTEN FOR UNUSUAL<br>NOISES. |  |
| **noisy (adj) — UNNAPPROVED** | NOISE (n) | IF THERE IS NOISE<br>WHEN THE PUMP<br>OPERATES, EXAMINE<br>THE FILTER FOR<br>UNWANTED<br>PARTICLES. | If pump operation is<br>noisy, check the pump<br>filter for unwanted<br>particles. |
| **NONE (pron)** | Not one, not anyone | IF NONE OF THE<br>BRACKETS ARE<br>DAMAGED, CONTINUE<br>THE INSPECTION. |  |

# Page 308 of 434

| **Word**<br>**(part of speech)** | **Approved meaning/**<br>**ALTERNATIVES** | **STE EXAMPLE** | **Non-STE example** |
|---|---|---|---|
| **nor (conj) — UNNAPPROVED** | NOT (adv) | IN THESE<br>CONDITIONS, THE<br>MECHANICAL AND<br>ELECTRICAL PITCH<br>TRIM SYSTEMS WILL<br>NOT OPERATE. | In these conditions,<br>neither the mechanical<br>nor the electrical pitch<br>trim systems will<br>operate. |
| **normal (adj) — UNNAPPROVED** | USUAL (adj)<br>CORRECT (adj) | THE "ARMED"<br>POSITION IS THE<br>USUAL POSITION OF<br>THE SWITCH.<br>THE CORRECT<br>PRESSURE FOR<br>OPERATION IS<br>3000 psi. | The ARMED position is<br>the normal position of<br>the switch.<br>Normal operating<br>pressure is 3000 psi. |
| **normally (adv) — UNNAPPROVED** | USUALLY (adv)<br>CORRECTLY (adv) | THE SWITCH IS<br>USUALLY IN THE<br>"STANDBY" POSITION.<br>IF THE SYSTEM DOES<br>NOT OPERATE<br>CORRECTLY, REFER<br>TO THE FAULT<br>ISOLATION<br>PROCEDURE. | The switch is normally in<br>the STANDBY position.<br>If the system does not<br>operate normally, refer<br>to the fault isolation<br>procedure. |
| **NOSE (n)** | The front end or part, a<br>part that protrudes | PULL THE<br>TRANSPARENT<br>PLASTIC COLLAR<br>AWAY FROM THE<br>NOSE OF THE<br>ELECTRICAL LATCH. |  |
| **NOT (adv)** | Adverb of negation | DO NOT LET THE<br>PRESSURE INCREASE<br>TO MORE THAN<br>3000 psi. |  |
| **NOTCH (n)** | An area in the shape of<br>a "V" | MAKE SURE THAT THE<br>BOGIE ROLLERS ARE<br>ALIGNED WITH THE<br>NOTCHES IN THE<br>TRACK. |  |
