# Page 265 of 434

**Page 2-1-H7**

**ASD-STE100 Simplified Technical English**

**Word Approved meaning/** **<u>(part of speech) ALTERNATIVES</u>**

**<u>STE EXAMPLE</u>**

**<u>Non-STE example</u>**

Blank Page

# Page 266 of 434

**Page 2-1-H8**

**Part 2 - Dictionary**

**Issue 9 2025-01-15**

##### **ASD-STE100 Simplified Technical English**

|**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
|---|---|---|---|
|**identical (adj) — UNNAPPROVED**|SAME (adj)|THE SAME<br>PROCEDURE IS<br>APPLICABLE TO THE<br>TWO VHF SETS.|The procedure is<br>identical for both VHF<br>sets.|
|**IDENTIFICATION**<br>**(n)**|Something that identifies<br>an object|MAKE SURE THAT THE<br>NAMEPLATE SHOWS<br>THE CORRECT<br>IDENTIFICATION OF<br>THE UNIT.|
|**IDENTIFY (v),**<br>**IDENTIFIES,**<br>**IDENTIFIED,**<br>**IDENTIFIED**|1. To use a specified<br>code or marking to<br>supply with an<br>identity|IDENTIFY THE WIRES<br>WITH SLEEVES OF<br>DIFFERENT COLORS.|

| |2. To show an identity<br>For other<br>meanings, use:|A 406 MHz DIGITAL<br>SIGNAL IDENTIFIES<br>THE EMERGENCY<br>LOCATOR<br>TRANSMITTER AND<br>ITS LOCATION.|	FIND (v)|FIND THE DAMAGED<br>AREAS.|Identify the damaged<br>areas.
|**idle (v) — UNNAPPROVED**|IDLE (TN)|OPERATE THE<br>ENGINE AT IDLE FOR<br>20 MINUTES.|Idle the engine for<br>20 minutes.

|**IF (conj)**|In the event that, on the<br>condition that, in case of|IF YOU USE A<br>REPLACEMENT<br>FAIRING PLATE, CUT<br>IT UNTIL YOU GET THE<br>CORRECT MATING<br>DIMENSION.|

|**ignite (v) — UNNAPPROVED**|IGNITION (TN)|FUEL GOES THROUGH<br>THE ATOMIZERS INTO<br>THE COMBUSTION<br>CHAMBER, WHERE<br>IGNITION OCCURS.|Fuel passes through the<br>atomizers to the<br>combustion chamber,<br>where it is ignited.

|**IGNORE (v),**<br>**IGNORES,**<br>**IGNORED,**<br>**IGNORED**|Not to think about<br>something, not to do<br>something about|IGNORE THE<br>VIBRATION<br>INDICATIONS.|
| |SELECT "CANCEL" TO<br>IGNORE ALL<br>CHANGES.|

|

**Issue 9 2025-01-15**

**Part 2 - Dictionary**

# Page 267 of 434

**Page 2-1-I1**

**ASD-STE100 Simplified Technical English**

|**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
|---|---|---|---|---|
|**ILLUMINATE (v),**<br>**ILLUMINATES,**<br>**ILLUMINATED,**<br>**ILLUMINATED**|To make something<br>visible with an external<br>light source<br>For lights or<br>lamps, use:|THE EMERGENCY<br>LIGHTS COME ON TO<br>ILLUMINATE THE<br>EVACUATION PATH.|

| |COME ON|WHEN THE PRESSURE<br>LIGHT COMES ON,<br>READ THE VALUE ON<br>THE PRESSURE<br>GAUGE.|	<br>When the pressure light<br>illuminates, read the<br>value on the pressure<br>gauge.
| |MAKE SURE THAT THE<br>LAMP COMES ON.|Ensure the lamp<br>illuminates.
| |BE ON|MAKE SURE THAT THE<br>LAMP IS ON.|Ensure the lamp is<br>illuminated.
|**immediate (adj) — UNNAPPROVED**|IMMEDIATELY (adv)|MAKE SURE THAT THE<br>SPEEDBRAKE<br>RETRACTS<br>IMMEDIATELY.|Check the speedbrake<br>for immediate retraction.

|**IMMEDIATELY**<br>**(adv)**|Without a gap of time or<br>space|MAKE SURE THAT THE<br>EMERGENCY LIGHT<br>IMMEDIATELY GOES<br>BACK TO "OFF."|

|**immerse (v) — UNNAPPROVED**|SOAK (v)|SOAK THE FILTER IN<br>THE CLEANING<br>SOLUTION FOR<br>4 HOURS.|Immerse the filter in the<br>cleaning solution for<br>4 hours.
| |PUT FULLY INTO|PUT THE FILTER<br>FULLY INTO THE<br>SOLVENT.|Immerse the filter in<br>solvent.
|**immobilize (v) — UNNAPPROVED**|LOCK (v)|LOCK THE PULLEY<br>WITH THE RIGGING<br>PIN.|Immobilize the pulley<br>with the rigging pin.
| |PREVENT MOVEMENT|WHEN YOU REPAIR<br>THE UNIT, PREVENT<br>MOVEMENT OF THE<br>ASSEMBLIES.|Immobilize the<br>assemblies when<br>repairing the unit.
|**impact (n) — UNNAPPROVED**|HIT (v)|MAKE SURE THAT<br>METAL OBJECTS DO<br>NOT HIT THE MATING<br>SURFACE.|Avoid impact between<br>metal objects and the<br>mating surface.

# Page 268 of 434

**Page 2-1-I2**

**Part 2 - Dictionary**

**Issue 9 2025-01-15**

##### **ASD-STE100 Simplified Technical English**

|**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
|---|---|---|---|

|**impact (v) — UNNAPPROVED**|HIT (v)|DO NOT LET THE<br>VIBRATOR TOOL HIT<br>THE SURFACE OF THE<br>SEAL.|Do not allow the vibrator<br>tool to impact the seal<br>surface.
| |EFFECT (n)|THESE REPAIRS HAVE<br>AN EFFECT ON THE<br>PERFORMANCE OF<br>THE ENGINE.|These repairs impact<br>engine performance.
|**impair (v) — UNNAPPROVED**|DECREASE (v)|THE LIFE OF THE UNIT<br>WILL DECREASE IF<br>YOU LET THE UNIT<br>BECOME DIRTY.|The life of the unit is<br>impaired if the unit is<br>allowed to get dirty.
| |OPERATE<br>INCORRECTLY|DAMAGE WILL CAUSE<br>THE INSTRUMENT TO<br>OPERATE<br>INCORRECTLY.|Damage will impair<br>operation of the<br>instrument.
| |CAUSE DAMAGE|CONTAMINATION OF<br>THE GREASE CAN<br>CAUSE DAMAGE TO<br>THE BEARING.|Contaminants in the<br>grease may impair the<br>bearing.
|**implement (v) — UNNAPPROVED**|DO (v)|IF THE TEST DOES<br>NOT GIVE<br>SATISFACTORY<br>RESULTS, DO THE<br>FAULT ISOLATION<br>PROCEDURE.|If the test does not give<br>satisfactory results,<br>implement the fault<br>isolation procedure.
|**implementation (n) — UNNAPPROVED**|DO (v)|IT IS MANDATORY TO<br>DO THE PROCEDURE<br>IN THIS SERVICE<br>BULLETIN.|The implementation of<br>the procedure in this<br>Service Bulletin is<br>mandatory.

|**IMPORTANT (adj)**|That has a significant<br>effect|THESE PROCEDURES<br>ARE VERY<br>IMPORTANT.|

**Issue 9 2025-01-15**

**Part 2 - Dictionary**
