# Page 265–268 of 434

> **Source:** ASD-STE100 Issue 9, January 2025
> **Pages:** 265–268 of 434

# Page 265 of 434

Blank Page

# Page 266 of 434

| Word (POS) | Approved meaning / ALTERNATIVES | STE example | Non-STE example |
|------------|--------------------------------|-------------|-----------------|
| identical (adj) — UNNAPPROVED | SAME (adj) | THE SAME PROCEDURE IS APPLICABLE TO THE TWO VHF SETS. | The procedure is identical for both VHF sets. |
| IDENTIFICATION (n) | Something that identifies an object | MAKE SURE THAT THE NAMEPLATE SHOWS THE CORRECT IDENTIFICATION OF THE UNIT. | |
| IDENTIFY (v), IDENTIFIES, IDENTIFIED, IDENTIFIED | 1. To use a specified code or marking to supply with an identity | IDENTIFY THE WIRES WITH SLEEVES OF DIFFERENT COLORS. | |
| IDENTIFY (v), IDENTIFIES, IDENTIFIED, IDENTIFIED | 2. To show an identity For other meanings, use: | A 406 MHz DIGITAL SIGNAL IDENTIFIES THE EMERGENCY LOCATOR TRANSMITTER AND ITS LOCATION. | |
| FIND (v) | | FIND THE DAMAGED AREAS. | Identify the damaged areas. |
| idle (v) — UNNAPPROVED | IDLE (TN) | OPERATE THE ENGINE AT IDLE FOR 20 MINUTES. | Idle the engine for 20 minutes. |
| IF (conj) | In the event that, on the condition that, in case of | IF YOU USE A REPLACEMENT FAIRING PLATE, CUT IT UNTIL YOU GET THE CORRECT MATING DIMENSION. | |
| ignite (v) — UNNAPPROVED | IGNITION (TN) | FUEL GOES THROUGH THE ATOMIZERS INTO THE COMBUSTION CHAMBER, WHERE IGNITION OCCURS. | Fuel passes through the atomizers to the combustion chamber, where it is ignited. |
| IGNORE (v), IGNORES, IGNORED, IGNORED | Not to think about something, not to do something about | IGNORE THE VIBRATION INDICATIONS. | |
| IGNORE (v), IGNORES, IGNORED, IGNORED | | SELECT "CANCEL" TO IGNORE ALL CHANGES. | |

# Page 267 of 434

| Word (POS) | Approved meaning / ALTERNATIVES | STE example | Non-STE example |
|------------|--------------------------------|-------------|-----------------|
| ILLUMINATE (v), ILLUMINATES, ILLUMINATED, ILLUMINATED | To make something visible with an external light source For lights or lamps, use: | THE EMERGENCY LIGHTS COME ON TO ILLUMINATE THE EVACUATION PATH. | |
| ILLUMINATE (v), ILLUMINATES, ILLUMINATED, ILLUMINATED | COME ON | WHEN THE PRESSURE LIGHT COMES ON, READ THE VALUE ON THE PRESSURE GAUGE. | When the pressure light illuminates, read the value on the pressure gauge. |
| ILLUMINATE (v), ILLUMINATES, ILLUMINATED, ILLUMINATED | COME ON | MAKE SURE THAT THE LAMP COMES ON. | Ensure the lamp illuminates. |
| ILLUMINATE (v), ILLUMINATES, ILLUMINATED, ILLUMINATED | BE ON | MAKE SURE THAT THE LAMP IS ON. | Ensure the lamp is illuminated. |
| immediate (adj) — UNNAPPROVED | IMMEDIATELY (adv) | MAKE SURE THAT THE SPEEDBRAKE RETRACTS IMMEDIATELY. | Check the speedbrake for immediate retraction. |
| IMMEDIATELY (adv) | Without a gap of time or space | MAKE SURE THAT THE EMERGENCY LIGHT IMMEDIATELY GOES BACK TO "OFF." | |
| immerse (v) — UNNAPPROVED | SOAK (v) | SOAK THE FILTER IN THE CLEANING SOLUTION FOR 4 HOURS. | Immerse the filter in the cleaning solution for 4 hours. |
| immerse (v) — UNNAPPROVED | PUT FULLY INTO | PUT THE FILTER FULLY INTO THE SOLVENT. | Immerse the filter in solvent. |
| immobilize (v) — UNNAPPROVED | LOCK (v) | LOCK THE PULLEY WITH THE RIGGING PIN. | Immobilize the pulley with the rigging pin. |
| immobilize (v) — UNNAPPROVED | PREVENT MOVEMENT | WHEN YOU REPAIR THE UNIT, PREVENT MOVEMENT OF THE ASSEMBLIES. | Immobilize the assemblies when repairing the unit. |
| impact (n) — UNNAPPROVED | HIT (v) | MAKE SURE THAT METAL OBJECTS DO NOT HIT THE MATING SURFACE. | Avoid impact between metal objects and the mating surface. |

# Page 268 of 434

| Word (POS) | Approved meaning / ALTERNATIVES | STE example | Non-STE example |
|------------|--------------------------------|-------------|-----------------|
| impact (v) — UNNAPPROVED | HIT (v) | DO NOT LET THE VIBRATOR TOOL HIT THE SURFACE OF THE SEAL. | Do not allow the vibrator tool to impact the seal surface. |
| impact (v) — UNNAPPROVED | EFFECT (n) | THESE REPAIRS HAVE AN EFFECT ON THE PERFORMANCE OF THE ENGINE. | These repairs impact engine performance. |
| impair (v) — UNNAPPROVED | DECREASE (v) | THE LIFE OF THE UNIT WILL DECREASE IF YOU LET THE UNIT BECOME DIRTY. | The life of the unit is impaired if the unit is allowed to get dirty. |
| impair (v) — UNNAPPROVED | OPERATE INCORRECTLY | DAMAGE WILL CAUSE THE INSTRUMENT TO OPERATE INCORRECTLY. | Damage will impair operation of the instrument. |
| impair (v) — UNNAPPROVED | CAUSE DAMAGE | CONTAMINATION OF THE GREASE CAN CAUSE DAMAGE TO THE BEARING. | Contaminants in the grease may impair the bearing. |
| implement (v) — UNNAPPROVED | DO (v) | IF THE TEST DOES NOT GIVE SATISFACTORY RESULTS, DO THE FAULT ISOLATION PROCEDURE. | If the test does not give satisfactory results, implement the fault isolation procedure. |
| implementation (n) — UNNAPPROVED | DO (v) | IT IS MANDATORY TO DO THE PROCEDURE IN THIS SERVICE BULLETIN. | The implementation of the procedure in this Service Bulletin is mandatory. |
| IMPORTANT (adj) | That has a significant effect | THESE PROCEDURES ARE VERY IMPORTANT. | |
