# Page 229 of 434

**Page 2-1-E11**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
||---|---|---|---|---|
||**exactly (adv) — UNNAPPROVED**|ACCURATELY (adv)|PUT THE REPAIR<BR>SHEET ACCURATELY<BR>ON THE DAMAGED<BR>AREA.|Put the repair sheet<br>exactly on the damaged<br>area.|
|||FULLY (adv)|FIND THE BOLT HOLE<br>THAT ALIGNS FULLY<BR>WITH ONE OF THE<br>OUTER SLOTS.|Find the bolt hole that<br>aligns exactly with one<br>of the outer slots.|
|||CORRECT (adj)|THE SEAL MUST BE<BR>OF THE CORRECT<br>DIMENSION FOR THE<br>GROOVE.|The seal must fit the<br>groove exactly.|
||**examination (n) — UNNAPPROVED**|EXAMINE (v)|EXAMINE THE BLADE<BR>FOR CRACKS.|Do an examination of<br>the blades for cracks.|
|||FIND (v)|IF YOU FIND<br>CORROSION,<br>REMOVE IT WITH THE<BR>SPECIFIED MATERIAL.|<br>If the examination<br>reveals corrosion, it<br>must be removed with<br>the specified material.|
||**EXAMINE (v),**<br>**EXAMINES,**<br>**EXAMINED,**<br>**EXAMINED**|To look carefully at|EXAMINE THE<br>COMPUTER FOR<br>DAMAGE.|
||**EXAMPLE (n)**|Something from a group<br>which has the same<br>qualities as the group|FIGURE 2 IS AN<br>EXAMPLE OF A<br>REPAIR PROCEDURE<br>FOR A DAMAGED<br>WEB.|
||**exceed (v) — UNNAPPROVED**|MORE THAN|MAKE SURE THAT<br>THE INDICATION IS<br>NOT MORE THAN<br>400 KNOTS.|Ensure that the<br>indication does not<br>exceed 400 knots.|
||**except (prep) — UNNAPPROVED**|To replace this<br>word, use a<br>different<br>construction.<br>Be accurate.|KEEP ALL THE PARTS<br>THAT ARE<br>SERVICEABLE AND<br>DISCARD THOSE<br>THAT ARE BROKEN.|Keep all parts except<br>those that are broken.|
|||||REMOVE ALL<br>SCREWS, BUT NOT<br>THE ONE ON THE<br>LEFT SIDE OF THE<br>FLANGE.|Remove all screws<br>except the one on the<br>left side of the flange.|

# Page 230 of 434

**Page 2-1-E12**

**Part 2 - Dictionary**

**Issue 9 2025-01-15**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
||---|---|---|---|---|
||**exception (n) — UNNAPPROVED**|To replace this<br>word, use a<br>different<br>construction.<br>Be accurate.|KEEP ALL THE PARTS<br>THAT ARE<br>SERVICEABLE AND<br>DISCARD THOSE<br>THAT ARE BROKEN.|Keep all parts with the<br>exception of those that<br>are broken.|
|||||REMOVE ALL<br>SCREWS, BUT NOT<br>THE ONE ON THE<br>LEFT SIDE OF THE<br>FLANGE.|Remove all screws with<br>the exception of the one<br>on the left side of the<br>flange.|
||**exceptional (adj) — UNNAPPROVED**|UNUSUAL (adj)|IF IT IS NECESSARY<br>TO APPLY UNUSUAL<br>FORCE TO OPEN THE<br>UNIT, EXAMINE THE<br>CONTROL LINKAGE.|If exceptional force is<br>needed to open the unit,<br>examine the control<br>linkage.|
||**exceptionally (adv) — UNNAPPROVED**|UNUSUALLY (adv)|IF THE TIRE<br>PRESSURE IS<br>UNUSUALLY HIGH,<br>OPEN THE VALVE.|If the tire pressure is<br>exceptionally high, open<br>the valve.|
||**excess (adj) — UNNAPPROVED**|TOO MUCH|DO NOT APPLY TOO<br>MUCH ADHESIVE ON<br>THE GASKET.|Do not apply excess<br>adhesive on the gasket.|
|||MORE THAN|DO NOT PUT MORE<br>THAN THE<br>PERMITTED WEIGHT<br>ON THE TROLLEY.|Do not put excess<br>weight on the trolley.|
|||UNWANTED (adj)|REMOVE UNWANTED<br>COMPOUND FROM<br>THE GASKET.|Wipe excess compound<br>from the gasket.|
|||NOT NECESSARY|REMOVE ALL<br>REMAINING SEALANT<br>THAT IS NOT<br>NECESSARY.|Remove all the excess<br>sealant.|
||**excess (n) — UNNAPPROVED**|TOO MUCH|IF YOU USE TOO<br>MUCH PAINT, THE<br>FINISH WILL BE<br>UNSATISFACTORY.|An excess of paint will<br>give a poor finish.|
|||MORE THAN|THE HYDRAULIC<br>PRESSURE MUST NOT<br>BE MORE THAN<br>200 bar.|The hydraulic pressure<br>must not be in excess of<br>200 bar.|

**Issue 9 2025-01-15**

**Part 2 - Dictionary**

# Page 231 of 434

**Page 2-1-E13**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
||---|---|---|---|---|
||**excessive (adj) — UNNAPPROVED**|TOO MUCH|TOO MUCH FORCE<br>CAN CAUSE DAMAGE<br>TO THE SEAL.|Excessive force can<br>damage the seal.|
|||MORE THAN|IF THE PRESSURE IS<br>MORE THAN 1000 kPa,<br>STOP THE TEST.|<br>If the pressure is<br>excessive, stop the test.|
||**excessively (adv) — UNNAPPROVED**|TOO MUCH|BE CAREFUL NOT TO<br>TURN THE INNER<br>RACES TOO MUCH.|Be careful not to<br>excessively rotate the<br>inner races.|
|||MORE THAN|IF THE OIL LEAKAGE<br>IS MORE THAN FIVE<br>DROPS A MINUTE,<br>REJECT THE UNIT.|If oil leaks excessively,<br>reject the unit.|
||**exchange (v) — UNNAPPROVED**|INTERCHANGE (v)|INTERCHANGE THE<br>No. 1 AND No. 2<br>COMPUTERS. THEN<br>DO THE TEST AGAIN.|Exchange the No. 1 and<br>No. 2 computers. Then<br>do the test again.|
|||REPLACE (v)|REPLACE THE<br>O-RINGS.|Exchange the O-rings.|
||**exclude (v) — UNNAPPROVED**|NOT INCLUDE|THIS PROCEDURE<br>DOES NOT INCLUDE<br>THE REMOVAL OF<br>THE PISTON.|This procedure excludes<br>the removal of the<br>piston.|
|||NOT USE|DO NOT USE<br>OXYGEN.|Exclude the use of<br>oxygen.|
||**excluding (prep) — UNNAPPROVED**|WITHOUT (prep)|THE WEIGHT OF THE<br>UNIT, WITHOUT THE<br>MOTOR, IS 10 kg.|The weight of the unit,<br>excluding the motor, is<br>10 kg.|
||**execute (v) — UNNAPPROVED**|DO (v)|DO THESE STEPS.|Execute the following<br>operations.|
||**exempt (adj) — UNNAPPROVED**|NO (adj)|MAKE SURE THAT<br>THERE ARE NO<br>METAL PARTICLES IN<br>THE OIL.|Ensure the oil is exempt<br>from metal particles.|
|||NOT SHOW|MAKE SURE THAT<br>THE SEALS DO NOT<br>SHOW SIGNS OF<br>DETERIORATION.|Ensure the seals are<br>exempt from signs of<br>deterioration.|

# Page 232 of 434

**Page 2-1-E14**

**Part 2 - Dictionary**

**Issue 9 2025-01-15**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
||---|---|---|---|---|
||**exercise (v) — UNNAPPROVED**|MAKE SURE (v)|MAKE SURE THAT<br>YOU DO NOT GET<br>ACID ON YOUR SKIN.|Exercise caution not to<br>allow acid to contact<br>skin.|
|||CAREFUL (adj)|BE CAREFUL THAT<br>YOU DO NOT GET<br>ACID ON YOUR SKIN.|Exercise caution not to<br>allow acid to contact<br>skin.|
||**exert (v) — UNNAPPROVED**|APPLY (v)|APPLY A LIGHT<br>FORCE TO THE<br>PEDALS.|Exert a light force on the<br>pedals.|
|||PUT (v)|PUT PRESSURE ON<br>THE WOUND.|Exert pressure on the<br>wound.|
||**exhale (v) — UNNAPPROVED**|BREATHE (v)|BREATHE INTO THE<br>OXYGEN MASK.|Exhale into the oxygen<br>mask.|
||**EXHAUST (n)**|The gas from an engine|THE EXHAUST FROM<br>THE APU IS<br>DANGEROUS.|
||**exhaust (v) — UNNAPPROVED**|REMOVE (v)|USE A FAN TO<br>REMOVE THE GASES.|Exhaust the gases using<br>a fan.|
|||DECREASE (v)|DECREASE THE<br>NITROGEN<br>PRESSURE TO<br>120 psi.|Exhaust the nitrogen<br>pressure to 120 psi.|
|||RELEASE (v)|RELEASE THE<br>HYDRAULIC<br>PRESSURE IN THE<br>ACCUMULATOR.|Exhaust all the hydraulic<br>pressure in the<br>accumulator.|
||**exhaustive (adj) — UNNAPPROVED**|ALL (adj)|ALL THE TEST<br>CONDITIONS ARE<br>GIVEN IN<br>PARAGRAPH 2.0.|An exhaustive list of test<br>conditions is given at<br>paragraph 2.0.|
|||FULL (adj)|THIS IS NOT A FULL<br>LIST.|The list is not exhaustive.|
||**exist (v) — UNNAPPROVED**|BE (v)|THERE ARE TWO<br>DIFFERENT<br>PROCEDURES FOR<br>THIS REPAIR.|Two different procedures<br>exist for this repair.|
||**EXIT (n)**|An opening to go out of<br>a space|MAKE SURE THAT ALL<br>THE EMERGENCY<br>EXITS ARE CLEAR OF<br>UNWANTED OBJECTS.|

**Issue 9 2025-01-15**

**Part 2 - Dictionary**
