<!-- section: DICT_Q-Z | pages: 353-356 | verified: true -->

# Page 353 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **recoil (v) — UNNAPROVED** | MOVE BACK BE CAREFUL WHEN Be careful when the THE SLIDE MOVES slide recoils. BACK. |
| **WIND (v)** | WIND THE PROBE Recoil the probe wire WIRE BACK ON THE back on the spool. SPOOL. RECOIL (TN) THE GUN BARREL HAS The gun barrel recoils A QUICK RECOIL. quickly. |
| **RECOMMEND (v)** | , To advise that which is THE MANUFACTURER RECOMMENDS, best RECOMMENDS THAT RECOMMENDED, YOU KEEP THE UNIT RECOMMENDED IN A DEDICATED AREA. |
| **recondition (v) — UNNAPROVED** | REPAIR (v) REPAIR THE SEATS. Recondition the seats. OVERHAUL (TN) DO AN OVERHAUL OF Recondition the engine. THE ENGINE. |
| **reconstruction (n) — UNNAPROVED** | REPAIR (n) RECORD ALL REPAIRS Record all reconstruction TO THE SKIN of the skin surface. SURFACE. |
| **REPAIR (v)** | THIS PROCEDURE This procedure is for the TELLS YOU HOW TO reconstruction of the REPAIR THE surface. SURFACE. |
| **RECORD (v)** | , 1. To make notes of RECORD THE RECORDS, and keep data to RESULTS. RECORDED, use subsequently RECORDED 2. To put data on a THE COCKPIT VOICE storage medium RECORDER RECORDS SIGNALS FROM FOUR AUDIO INPUTS DURING THE FLIGHT. |
| **recover (v) — UNNAPROVED** | COLLECT (v) REMOVE THE NUT Remove the nut and the AND THE BOLT. THEN, bolt. Then, recover the COLLECT THE washer. WASHER. |
| **rectify (v) — UNNAPROVED** | CORRECT (v) BEFORE YOU START Rectify the defect before THE PROCEDURE you restart the AGAIN, CORRECT THE procedure. DEFECT. |
| **recur (v) — UNNAPROVED** | OCCUR (v) IF THE SYMPTOMS If the symptoms recur, OCCUR AGAIN, DO A do a system test. SYSTEM TEST. |

# Page 354 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **RECYCLE (v)** | , To put a used material MAKE SURE THAT RECYCLES, through a process to YOU RECYCLE THE RECYCLED, make it possible to use it REMOVED RECYCLED or its components again INSULATION MATERIAL. For other meanings, use: |
| **CYCLE (n)** | DO ONE MORE TEST Recycle the component CYCLE OF THE through a test. COMPONENT. |
| **reduce (v) — UNNAPROVED** | DECREASE (v) SLOWLY DECREASE Slowly reduce the THE SPEED. speed. |
| **REFER (v)** | , 1. To tell a person REFER TO CHAPTER REFERS, where to find 28 FOR THE REFERRED, information INSTALLATION REFERRED PROCEDURE. 2. To give information BEFORE YOU DO THIS PROCEDURE, ENGAGE THE RAMP SERVICE DOOR SAFETY CONNECTOR PIN (THE PIN THAT HOLDS THE RAMP SERVICE DOOR, REFERRED TO IN THIS PROCEDURE AS THE "SAFETY CONNECTOR PIN"). |
| **reference (n) — UNNAPROVED** | REFER (v) REFER TO Reference is made to CHAPTER 20 FOR THE Chapter 20 for the STANDARD TORQUE standard torque values. VALUES. |
| **referenced (adj) — UNNAPROVED** | SHOW (v) MAKE SURE THAT THE Make sure that this point GRAPH SHOWS THIS is referenced on the POINT. graph. |
| **refill (v) — UNNAPROVED** | FILL (v) FILL THE CONTAINER Refill the container. AGAIN. |
| **refit (v) — UNNAPROVED** | INSTALL (v) INSTALL THE LINKAGE Refit the linkage. AGAIN. |
| **REPAIR (v)** | ON THE SUBMARINE, Refit the submarine. REPAIR ALL DAMAGE AND REPLACE ALL WORN PARTS. |

# Page 355 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **reflect (v) — UNNAPROVED** | REFLECTION (n) THE RETICLE IMAGE The reticle image MAKES A REFLECTION reflects on the bottom ON THE BOTTOM surface of the glass. SURFACE OF THE GLASS. |
| **REFLECTION (n)** | Something that occurs A CLEAN SURFACE when energy comes GIVES A BETTER against a surface which REFLECTION. sends it back |
| **REFUEL (v)** | , To supply with fuel REFUEL THE VEHICLE. REFUELS, REFUELED, REFUELED |
| **register (v) — UNNAPROVED** | SHOW (v) ADJUST THE "SET +40" Adjust the "SET +40" CONTROL UNTIL THE control until the pointer POINTER SHOWS +40. registers +40. |
| **regrease (v) — UNNAPROVED** | APPLY (v) APPLY GREASE TO Regrease the rod. THE ROD AGAIN. |
| **MORE (adj)** | PUT MORE GREASE Regrease the joint until ON THE JOINT UNTIL you can move it. YOU CAN MOVE IT. |
| **REGULAR (adj)** | At specified or equal THE COMPUTER intervals GIVES REGULAR INPUTS TO THE CONTROL SYSTEM. |
| **REGULARLY (adv)** | In a regular manner IF THE FAILURE OCCURS REGULARLY, DO A SYSTEM TEST. |
| **regulate (v) — UNNAPROVED** | CONTROL (v) CONTROL THE Regulate the electrical ELECTRICAL current. CURRENT. |
| **ADJUST (v)** | ADJUST THE TIRE Regulate the tire PRESSURE AS pressure as necessary. NECESSARY. |

# Page 356 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **regulation (n) — UNNAPROVED** | ADJUSTMENT (n) THE TEMPERATURE The regulation of ADJUSTMENT IS temperature is AUTOMATIC. automatic. |
| **CONTROL (n)** | THE TEMPERATURE The regulation of CONTROL IS temperature is AUTOMATIC. automatic. |
| **CONTROL (v)** | A SENSOR CONTROLS The regulation of THE TEMPERATURE IN temperature in the THE COMPARTMENT. compartment is effected by a sensor. |
| **reinflate (v) — UNNAPROVED** | INFLATE (v) INFLATE THE TIRE Reinflate the tire. AGAIN. |
| **reinforce (v) — UNNAPROVED** | MAKE … STRONGER DOUBLERS MAKE THE Doublers reinforce the JOINT STRONGER. joint. |
| **reinstall (v) — UNNAPROVED** | INSTALL (v) AFTER YOU ADJUST Reinstall the cover after THE UNIT, INSTALL you adjust the unit. THE COVER AGAIN. |
| **reinstallation (n) — UNNAPROVED** | INSTALLATION (n) ONLY APPROVED This reinstallation must PERSONNEL CAN DO be performed by THE INSTALLATION qualified personnel. PROCEDURE. |
| **REJECT (v)** | , To make a decision that REJECT THE PARTS REJECTS, something is THAT ARE DAMAGED. REJECTED, unsatisfactory REJECTED |
| **rejection (n) — UNNAPROVED** | REJECT (v) IF THE TEST IS NOT Rejection is mandatory if SATISFACTORY, the test proves the REJECT THE component to be COMPONENT. defective. |
| **relate (v) — UNNAPROVED** | RELATED (adj) THE PROCEDURES The procedures relate to ARE RELATED TO THE the system test. SYSTEM TEST. |
| **RELATED (adj)** | That has a relation CLEAN THE BALLS OF THE ELECTRICAL LATCH AND ITS RELATED SOCKETS. |
| **RELATION (n)** | The connection between THE RELATION two or more things BETWEEN THE TWO caused by their CONTROL SYSTEMS functions, values, or KEEPS THE AIRCRAFT conditions STABLE. |
