# Page 189–192 of 434

> **Source:** ASD-STE100 Issue 9, January 2025
> **Pages:** 189–192 of 434

# Page 189 of 434

| Word (POS) | Approved meaning / ALTERNATIVES | STE example | Non-STE example |
|---|---|---|---|
| COMPONENT (n) | A part, subassembly, or unit that has a specified function | CLEAN THESE COMPONENTS WITH APPROVED SOLVENTS. |  |
| comprehensive (adj) | FULL (adj) | DO A FULL INSPECTION OF THE FAIRING. | Do a comprehensive inspection of the fairing. |
| COMPRESS (v), COMPRESSES, COMPRESSED, COMPRESSED | To decrease or cause to decrease in dimension or volume | COMPRESS THE SPRING AND CAREFULLY INSTALL THE COVER. WHEN THE SPRING COMPRESSES, THE VALVE OPENS. |  |
| comprise (v) — UNAPPROVED | HAVE (v) | THE VALVE ASSEMBLY HAS THESE PARTS: EACH SURVIVAL KIT CONTAINS THESE ITEMS. | The valve assembly comprises these parts: Each survival kit comprises these items. |
| compulsory (adj) — UNAPPROVED | MANDATORY (adj) | BEFORE YOU INSTALL A NEW COMPONENT, IT IS MANDATORY TO REPLACE THE FILTER. | Before you install a new component, it is compulsory to replace the filter. |
| compute (v) — UNAPPROVED | CALCULATE (v) | CALCULATE THE VOLTAGE IN THE CIRCUIT. | Compute the voltage in the circuit. |
| concentrate (v) — UNAPPROVED | ALL (adj) | ALL THE WEIGHT MUST BE ON THE SPAR TIP. | The weight must be concentrated on the spar tip. |
| CONCENTRATION (n) | The strength of something contained in a mixture | IN A HIGH CONCENTRATION, THIS MATERIAL IS POISONOUS. |  |
| CONCENTRIC (adj) | That has a common center | THE EXTERNAL DIAMETER MUST BE CONCENTRIC TO THE INTERNAL DIAMETER. |  |
| concern (v) — UNAPPROVED | APPLICABLE (adj) | THIS PROCEDURE IS APPLICABLE ONLY TO A TYPE B UNIT. | This procedure only concerns a Type B unit. |

# Page 190 of 434

| Word (POS) | Approved meaning / ALTERNATIVES | STE example | Non-STE example |
|---|---|---|---|
| conclusion (n) — UNAPPROVED | END (n) | AT THE END OF THE TEST, SET THE SWITCH TO "NORMAL." | At the conclusion of the test, you must switch to NORMAL. |
| conclusion (n) — UNAPPROVED | RESULT (n) | IF THE RESULTS OF THE TEST ARE UNSATISFACTORY, REPLACE THE UNIT. | If the conclusions of the test are unsatisfactory, replace the unit. |
| concurrently (adj) — UNAPPROVED | AT THE SAME TIME | DO THESE TWO PROCEDURES AT THE SAME TIME. | These two procedures must be applied concurrently. |
| CONDENSATION (n) | The result when a gas changes into a liquid | SET THE SWITCH TO THE "ON" POSITION TO REMOVE THE CONDENSATION. |  |
| CONDITION (n) | 1. Something that is necessary for what occurs<br>2. The state of an item<br>Use IF (conj) for "on the condition that." | THESE INITIAL CONDITIONS ARE NECESSARY TO GET CORRECT RESULTS.<br>DO A CHECK OF THE UNIT CONDITION.<br>IF THERE IS NO WIND, DO THE TEST OUTDOORS. | On the condition that there is no wind, do the test outdoors. |
| conduct (v) — UNAPPROVED | DO (v) | DO THE LEAK TEST. | Conduct the leak test. |
| confine to (v) — UNAPPROVED | ONLY (adv) | IF THE DAMAGE IS ONLY TO THE MIDDLE TREADS, THE TIRE IS SERVICEABLE. | If the damage is confined to the middle treads, the tire is serviceable. |
| confirm (v) — UNAPPROVED | MAKE SURE (v) | DO A GROUND RUN OF THE ENGINE TO MAKE SURE THAT YOU GET THE SAME INDICATIONS. | Do a ground run of the engine to confirm the indications. |
| conflict (n) — UNAPPROVED | DIFFERENT (adj) | IF THE TWO INDICATIONS ARE DIFFERENT, DO THE TEST AGAIN. | If there is a conflict between the two indicators, repeat the test. |
| conflict (n) — UNAPPROVED | AGREE (v) | IF THE TWO INDICATIONS DO NOT AGREE, DO THE TEST AGAIN. | If there is a conflict between the two indicators, repeat the test. |

# Page 191 of 434

| Word (POS) | Approved meaning / ALTERNATIVES | STE example | Non-STE example |
|---|---|---|---|
| conform (v) — UNAPPROVED | AGREE (v) | IF THE FLAP EXTENSION DOES NOT AGREE WITH THE POSITION OF THE FLAP CONTROL LEVER, DO THE RIGGING PROCEDURE AGAIN. | If the flap extension does not conform to the setting of the flap control lever, do the rigging procedure again. |
| conformance (n) — UNAPPROVED | AGREE (v) | THE INDICATIONS MUST AGREE WITH THOSE IN TABLE 2. | The indications must be in conformance with those in Table 2. |
| conformity (n) — UNAPPROVED | AGREE (v) | THE PRECISION OF THE GAUGES MUST AGREE WITH THE APPLICABLE QUALITY STANDARD. | The accuracy of the gauges must be in conformity with the applicable quality standard. |
| CONNECT (v), CONNECTS, CONNECTED, CONNECTED | To come together or cause to come together to make one unit or system | CONNECT THE ELECTRICAL CONNECTORS TO THE INSTRUMENT. PLUG "A" CONNECTS TO SOCKET "B". |  |
| CONNECTION (n) | That which connects or is connected | MAKE SURE THAT ALL THE FUEL AND AIR CONNECTIONS ARE INSTALLED. |  |
| consecutive (adj) — UNAPPROVED | ONE (TN) AFTER THE OTHER | DO NOT DO MORE THAN THREE STARTS, ONE AFTER THE OTHER. | Do not do more than three consecutive starts. |
| consecutively (adv) | ONE (TN) AFTER THE OTHER | DO THESE STEPS ONE AFTER THE OTHER. | These actions must be done consecutively. |
| consecutively (adv) | SEQUENCE (n) | DO THE WORK STEPS IN SEQUENCE. | Do the work steps consecutively. |
| consequence (n) — UNAPPROVED | BECAUSE OF (prep) | BECAUSE OF THIS DEFECT, THE UNIT WILL NOT OPERATE. | As a consequence of this defect, the unit will not operate. |

# Page 192 of 434

| Word (POS) | Approved meaning / ALTERNATIVES | STE example | Non-STE example |
|---|---|---|---|
| consider (v) — UNAPPROVED | THINK (v) | IF YOU THINK THAT THE INDICATION IS NOT CORRECT, DO THE TEST AGAIN. | If you consider that the indication is not correct, do the test again. |
| considerable (adj) — UNAPPROVED | LARGE (adj) | CLEAN YOUR SKIN WITH A LARGE QUANTITY OF WATER. | Clean your skin with a considerable quantity of water. |
| considerable (adj) — UNAPPROVED | IMPORTANT (adj) | CONTAMINATION OF CABIN AIR CAN BE AN IMPORTANT PROBLEM. | Contamination of cabin air can be a considerable problem. |
| considerable (adj) — UNAPPROVED | DANGEROUS (adj) | HYDRAULIC FLUID IS DANGEROUS FOR YOUR EYES. | Hydraulic fluid can cause considerable eye injury. |
| consist of (v) — UNAPPROVED | HAVE (v) | EACH ANTENNA HAS THREE PARTS. | Each antenna consists of three parts. |
| consistent (adj) — UNAPPROVED | AGREE (v) | MAKE SURE THAT THE INDICATIONS AGREE WITH THE POSITION OF THE FLAPS. | Check that the indications are consistent with the position of the flaps. |
| CONSTANT (adj) | That continues to be the same, without change | MAKE SURE THAT THE CABIN PRESSURE STAYS CONSTANT. |  |
| CONSTANTLY (adv) | Incessantly | THE INSTRUMENT WILL CONSTANTLY SHOW THIS VALUE. |  |
| construct (v) — UNAPPROVED | ASSEMBLE (v) | ASSEMBLE THE UNIT. | Construct the unit. |
| consult (v) — UNAPPROVED | REFER (v) | FOR MORE INFORMATION, REFER TO THE USER'S MANUAL. | For more information, consult the User's Manual. |
| CONTACT (v), CONTACTS, CONTACTED | To start communication. For other meanings, use: | CONTACT CUSTOMER SERVICES. |  |
| CONTACT (v), CONTACTS, CONTACTED | TOUCH (v) | TIGHTEN THE FIXTURE SCREW UNTIL IT TOUCHES THE SURFACE. | Tighten the fixture screw until it contacts the surface. |
