# Page 153 of 434

**Page 2-1-A12**

**Part 2 - Dictionary**

**Issue 9 2025-01-15**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
||---|---|---|---|
||**alter (v) — UNNAPPROVED**|CHANGE (v)|IT IS POSSIBLE THAT<br>THE INSTALLATION OF<br>THE CONNECTOR<BR>PINS CHANGED THE<BR>ROUTING OF THE<BR>CABLE LOOM.|It is possible that the<br>installation of the<br>connector pins altered<br>the routing of the cable<br>loom.|
||**alteration (n) — UNNAPPROVED**|CHANGE (v)|IF YOU CHANGE THIS<br>REPAIR PROCEDURE,<BR>GET APPROVAL OF<BR>THE DESIGN<BR>AUTHORITY.|The alteration to this<br>repair procedure must<br>get approval of the<br>Design Authority.|
||**alternate (adj) — UNNAPPROVED**|ALTERNATIVE (adj)|AN ALTERNATIVE<br>REPAIR IS AVAILABLE.|An alternate repair is<br>available.|
|||EACH SECOND|EACH SECOND<br>SQUARE IS RED.|Alternate squares are<br>red.|
||**alternate (v) — UNNAPPROVED**|THEN (adv)|DO THE PILOT'S<br>INSTRUMENT TEST<br>AND THEN THE<br>COPILOT'S TEST.|Alternate between pilot's<br>and copilot's instrument<br>test.|
||**alternately (adv) — UNNAPPROVED**|IN ONE (TN) … AND<br>THEN THE OTHER|TO MAKE PIN<BR>REMOVAL EASIER,<BR>MANUALLY TURN THE<BR>CANOPY IN ONE<BR>DIRECTION AND THEN<br>IN THE OTHER.|To make pin removal<br>easier, manually turn the<br>canopy alternately in the<br>two directions.|
||**ALTERNATIVE**<br>**(adj)**|That gives a choice|YOU CAN USE<br>ALTERNATIVE<br>MATERIALS.|
||**ALTERNATIVE (n)**|One of two or more<br>objects or processes that<br>have the same or almost<br>the same properties or<br>functions|A BIO-BASED FUEL<br>CAN BE AN<br>ALTERNATIVE TO<BR>FUELS JET-A1 AND<br>JET-A.|
||**alternatively (adv) — UNNAPPROVED**|ALTERNATIVE (n)|YOU CAN DO TEST B<br>AS AN ALTERNATIVE.|Alternatively, you can do<br>test B.|
||**ALTHOUGH (conj)**|In spite of the fact that|ALTHOUGH THE<br>PRESSURE<br>DECREASES, THE<br>VALVE MUST STAY<br>CLOSED.|
||**ALWAYS (adv)**|At all times|ALWAYS KEEP THE<BR>BRIGHTNESS<BR>CONTROL ON THE<BR>LCD DISPLAY AT<BR>MAXIMUM.|

**Issue 9 2025-01-15**

**Part 2 - Dictionary**

# Page 154 of 434

**Page 2-1-A13**

##### **ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
||---|---|---|---|
||**amend (v) — UNNAPPROVED**|CHANGE (v)|IF IT IS NECESSARY<br>TO CHANGE THE<br>REPAIR SCHEME, GET<br>THE APPROVAL OF<br>THE DESIGN<BR>AUTHORITY.|If it is necessary to<br>amend the Repair<br>Scheme, get the<br>approval of the Design<br>Authority.|
||**amendment (n) — UNNAPPROVED**|CHANGE (n)|THE DESIGN<br>AUTHORITY MUST<br>GIVE APPROVAL TO<br>THE CHANGES THAT<br>YOU MAKE TO THE<BR>REPAIR SCHEME.|The Design Authority<br>must approve the<br>amendments that you<br>make to the Repair<br>Scheme.|
|||CHANGE (v)|IF IT IS NECESSARY<br>TO CHANGE THE<br>REPAIR SCHEME, GET<br>THE APPROVAL OF<br>THE DESIGN<br>AUTHORITY.|If an amendment to the<br>Repair Scheme is<br>necessary, get the<br>approval of the Design<br>Authority.|
||**among (prep) — UNNAPPROVED**|IN (prep)|IF THERE ARE METAL<br>PARTICLES IN THE<br>SAMPLES, REPLACE<br>THE PUMP.|If there are metal<br>particles among the<br>samples, replace the<br>pump.|
||**amount (n) — UNNAPPROVED**|QUANTITY (n)|MAKE SURE THAT THE<br>QUANTITY OF FUEL IN<br>THE TANK IS NOT<BR>MORE THAN 500<br>LITERS.|<br>Make sure that the<br>amount of fuel in the<br>tank is not more than<br>500 liters.|
||**AN (art)**|Function word:<br>indefinite article|MAKE AN ENTRY IN<br>THE LOGBOOK.|
||**ANALOG (adj)**|Of data given by pointers<br>and dials|THE PRE-MOD UNIT<br>HAS ANALOG<br>INDICATORS.|
||**analyze (v) — UNNAPPROVED**|ANALYSIS (TN)|MAKE AN ANALYSIS<br>OF THE OIL.|Analyze the oil sample.|
||**anchor (v) — UNNAPPROVED**|ATTACH (v)|THE STRAPS ARE<br>ATTACHED TO A<br>FULL-LENGTH RAIL.|The straps are anchored<br>to a full-length rail.|

# Page 155 of 434

**Page 2-1-A14**

**Part 2 - Dictionary**

**Issue 9 2025-01-15**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
||---|---|---|---|
||**ancillary (adj) — UNNAPPROVED**|AUXILIARY (adj)|THE ENGINE AND ALL<br>AUXILIARY<BR>EQUIPMENT USE THE<BR>SAME LUBRICANT.|The engine and all<br>ancillary equipment use<br>the same lubricant.|
|||SECONDARY (adj)|DO AN OPERATIONAL<br>CHECK OF THE<br>SECONDARY<BR>CONTROLS.|Do an operational check<br>of the ancillary controls.|
||**AND (conj)**|Function word used to<br>connect words, phrases,<br>or clauses|MAKE SURE THAT THE<br>FLAPS ARE<br>RETRACTED AND THE<br>AILERON TRIM<BR>HANDWHEEL IS IN<br>THE ZERO POSITION.|
||**ANGULAR (adj)**|That has one or more<br>angles|MAKE SURE THAT THE<br>ANGULAR POSITION IS<br>CORRECT.|
||**annotation (n) — UNNAPPROVED**|WRITE (v)|WRITE THE<br>TEMPERATURE VALUE<BR>ON THE ENGINE LOG<br>CARD.|Make an annotation of<br>the temperature on the<br>Engine Log Card.|
|||RECORD (v)|RECORD THE<BR>TEMPERATURE VALUE<BR>ON THE ENGINE LOG<BR>CARD.|Make an annotation of<br>the temperature on the<br>Engine Log Card.|
||**annunciate (v) — UNNAPPROVED**|SHOW (v)|THE DISPLAY SHOWS<br>A FAULT MESSAGE.|The display annunciates<br>a fault message.|
||**another (adj) — UNNAPPROVED**|ONE (TN) MORE|INSTALL ONE MORE<br>WASHER BETWEEN<br>THE NUT AND THE<br>SURFACE.|Install another washer<br>between the nut and the<br>surface.|
|||DIFFERENT (adj)|REFER TO DETAIL C<br>ON FIG. 4 FOR A<br>DIFFERENT<br>PROCEDURE TO<BR>ATTACH THE CABLE.|Refer to detail C on Fig.<br>4 for another way of<br>attaching the cable.|
|||AGAIN (adv)|BEFORE YOU TRY TO<br>START THE ENGINE<br>AGAIN, MAKE SURE<br>THAT THE AREA IS<BR>SAFE.|Before you try another<br>engine start, make sure<br>that the area is safe.|
||**anticlockwise**<br>**(adv)**|COUNTERCLOCKWISE<br>(adv)|COUNTERCLOCKWISE.|<br>Turn the cap<br>anticlockwise.|

**Issue 9 2025-01-15**

**Part 2 - Dictionary**

# Page 156 of 434

**Page 2-1-A15**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
||---|---|---|---|
||**any (adj) — UNNAPPROVED**|Frequently, an<br>alternative for this<br>word is not<br>necessary.|<br>IF YOU HAVE<br>QUESTIONS ABOUT<br>THIS DOCUMENT,<br>SEND AN E-MAIL TO<br>THE ADDRESS THAT<br>FOLLOWS:|If you have any<br>questions about this<br>document, send an<br>e-mail to the address<br>that follows:|
||**any (pron) — UNNAPPROVED**|ONE (TN)|REMOVE ONE OF THE<br>FOUR BOLTS.|Remove any of the four<br>bolts.|
||**anytime (adv) — UNNAPPROVED**|WHEN (conj)|WHEN YOU USE THE<br>EMERGENCY PUMP,<br>RECORD THE TIME OF<br>OPERATION.|<br>Anytime you use the<br>emergency pump, record<br>the time of operation.|
||**APART (adv)**|At a distance (not<br>specified) from|MOVE THE CABLE<br>STRANDS APART.|
||**aperture (n) — UNNAPPROVED**|OPENING (n)|GET ACCESS TO THE<br>CONTROL UNIT<br>THROUGH THE<br>OPENING IN THE SIDE<br>OF THE TANK.|Get access to the control<br>unit through the aperture<br>in the side of the tank.|
||**apparent (adj) — UNNAPPROVED**|SEE (v)|IF YOU SEE<br>DISCOLORATION,<br>REPLACE THE PART.|If discoloration is<br>apparent, replace the<br>part.|
|||FIND (v)|IF YOU FIND A CRACK,<br>DO THE APPLICABLE<br>REPAIR PROCEDURE.|<br>If a crack is apparent, do<br>the applicable repair<br>procedure.|
||**appear (v) — UNNAPPROVED**|SHOW (v)|A WARNING FLAG<br>SHOWS IN THE<br>WINDOW.|A warning flag appears<br>in the window.|
||**(v)**|||THINK (v)|IF YOU THINK THAT<br>THE ENGINE IS TOO<br>HOT, TURN THE<br>SWITCH TO "OFF."|If the engine appears to<br>be too hot, turn the<br>switch to off.|
|||POSSIBLE (adj)|IF IT IS POSSIBLE<br>THAT THE<br>TEMPERATURE<br>VALUES ARE<br>INCORRECT,<br>DECREASE THE<br>POWER.|If it appears that the<br>temperature values are<br>incorrect, decrease the<br>power.|
