# Page 401–404 of 434

> **Source:** ASD-STE100 Issue 9, January 2025
> **Pages:** 401–404 of 434

# Page 401 of 434

| **Word**<br>**(part of speech)** | **Approved meaning/**<br>**ALTERNATIVES** | **STE EXAMPLE** | **Non-STE example** |
|---|---|---|---|
| **TRY (v),**<br>**TRIES,**<br>**TRIED,**<br>**TRIED** | To make an effort to do<br>something | TRY TO MOVE THE<br>CONTROL COLUMN. |  |
| **tuck (v) — UNNAPPROVED** | PUT (v) | PUT THE HEADSTRAP<br>INTO THE FACE<br>PIECE. | Tuck the headstrap into<br>the face piece. |
| **TUNE (v),**<br>**TUNES,**<br>**TUNED,**<br>**TUNED** | To adjust equipment to<br>the best performance | TUNE ADF 1 TO A<br>KNOWN FREQUENCY. |  |
| **TURN (n)** | One full cycle of<br>movement around an<br>axis | LET THE PRESSURE<br>BECOME STABLE<br>AFTER EACH TURN OF<br>THE ADJUSTMENT<br>SCREW. |  |
| **TURN (v),**<br>**TURNS,**<br>**TURNED,**<br>**TURNED** | To move or cause to<br>move around an axis or<br>a point | TURN THE CONTROL<br>CLOCKWISE.<br>THE BEARING TURNS<br>AT 1500 RPM. |  |
| **turn off (v) — UNNAPPROVED** | SET (v)<br>STOP (v)<br>DE-ENERGIZE (v) | SET THE COMPUTER<br>TO “OFF.”<br>STOP THE<br>COMPUTER.<br>DE-ENERGIZE THE<br>ELECTRICAL SYSTEM. | Turn off the computer.<br>Turn off the computer.<br>Turn the electrical<br>system off. |
| **turn on (v) — UNNAPPROVED** | SET (v)<br>START (v)<br>ENERGIZE (v) | SET THE POWER TO<br>“ON.”<br>START THE POWER.<br>ENERGIZE THE<br>ELECTRICAL SYSTEM. | Turn on the power.<br>Turn on the power.<br>Turn the electrical<br>system on. |
| **turn over (v) — UNNAPPROVED** | TURN (v) | TURN THE DISPLAY<br>PANEL UNTIL YOU<br>HAVE ACCESS TO THE<br>CABLE. | <br>Turn the display panel<br>over to access the cable. |
| **twice (adv) — UNNAPPROVED** | TWO (TN) | DO THIS PROCEDURE<br>TWO TIMES. | Do this procedure twice. |

# Page 402 of 434

| **Word**<br>**(part of speech)** | **Approved meaning/**<br>**ALTERNATIVES** | **STE EXAMPLE** | **Non-STE example** |
|---|---|---|---|
| **TWIST (v),**<br>**TWISTS,**<br>**TWISTED,**<br>**TWISTED** | 1. To use a force that<br>turns something and<br>causes a distortion<br>2. To turn or change<br>shape as a result of<br>torsion | DO NOT TWIST THE<br>CABLES.<br>IF THE CABLE TWISTS,<br>DISCONNECT THE<br>TWO CONNECTORS. |  |
| **TYPE (n)** | A specified group | FIND THE TYPE AND<br>DIMENSIONS OF THE<br>DAMAGE. |  |
| **TYPICAL (adj)** | That has the important<br>qualities of a group | THIS INSTALLATION<br>PROCEDURE IS<br>TYPICAL FOR THIS<br>TYPE OF FASTENER. |  |

# Page 403 of 434

Blank Page

# Page 404 of 434

| **Word**<br>**(part of speech)** | **Approved meaning/**<br>**ALTERNATIVES** | **STE EXAMPLE** | **Non-STE example** |
|---|---|---|---|
| **unable (adj) — UNNAPPROVED** | CANNOT (v) | IF YOU CANNOT TURN<br>THE PULLEY, MAKE<br>SURE THAT THE PIN IS<br>REMOVED. | If you are unable to turn<br>the pulley, make sure<br>that the pin is removed. |
| **unauthorized (adj) — UNNAPPROVED** | NOT APPROVED | IF YOU ARE NOT<br>APPROVED TO DO<br>THIS WORK, DO NOT<br>DO THIS ENGINE<br>TEST. | If you are unauthorized,<br>do not do this engine<br>test. |
| **uncap (v) — UNNAPPROVED** | REMOVE (v)<br>(A CAP [TN] OR CAPS<br>[TN]) | REMOVE THE CAPS<br>FROM THE HOSES. | Uncap the hoses. |
| **unclip (v) — UNNAPPROVED** | REMOVE (v)<br>(FROM A CLIP [TN] OR<br>CLIPS [TN]) | REMOVE THE VISOR<br>FROM THE CLIP. | Unclip the visor. |
| **uncoil (v) — UNNAPPROVED** | UNWIND (v) | UNWIND THE CABLES<br>CAREFULLY. | Uncoil the cables<br>carefully. |
| **uncontaminated**<br>**(adj)** | CLEAN (adj) | MAKE SURE THAT THE<br>HYDRAULIC FLUID IS<br>CLEAN. | Make sure that the<br>hydraulic fluid is<br>uncontaminated. |
| CONTAMINATION (n) |  | MAKE SURE THAT<br>THERE IS NO<br>CONTAMINATION IN<br>THE FUEL TANKS. | Make sure that the fuel<br>tanks are<br>uncontaminated. |
| **uncouple (v) — UNNAPPROVED** | DISCONNECT (v) | DISCONNECT THE<br>TOW BAR FROM THE<br>VEHICLE. | Uncouple the tow bar<br>from the vehicle. |
| **uncovered (adj) — UNNAPPROVED** | COVER (TN) | DO NOT PUT A COVER<br>ON THE CONTAINER. | Leave the container<br>uncovered. |
| **undamaged (adj) — UNNAPPROVED** | NOT DAMAGED | MAKE SURE THAT THE<br>SKIN IS NOT<br>DAMAGED. | Make sure that the skin<br>is undamaged. |
| **UNDEMANDED**<br>**(adj)** | That occurs without an<br>apparent cause | IF YOU GET AN<br>UNDEMANDED<br>MOVEMENT, DO A<br>TEST OF THE<br>SYSTEM. |  |
