# Page 205–208 of 434

> **Source:** ASD-STE100 Issue 9, January 2025
> **Pages:** 205–208 of 434

# Page 205 of 434

| Word (part of speech) | Approved meaning/ALTERNATIVES | STE EXAMPLE | Non-STE example |
|---|---|---|---|
| **dent (v) — UNNAPPROVED** | DENT (TN) | DO NOT MAKE DENTS<br>IN THE BELLOWS. | Do not dent the bellows. |
| **depend (v) — UNNAPPROVED** | IF (conj) | THE TENSION IN THE<BR>CABLES DECREASES<BR>IF THE TEMPERATURE<BR>INCREASES. | Cable tension changes<BR>depending on the<BR>temperature. |
| **deplete (v) — UNNAPPROVED** | DECREASE (v) | DO NOT OPERATE<BR>THE BRAKES TO<BR>DECREASE THE<BR>PRESSURE IN THE<BR>ACCUMULATORS. | Do not deplete<BR>accumulators by<BR>operating the brakes. |
| **DEPLOY (v),**<br>**DEPLOYS,**<br>**DEPLOYED,**<br>**DEPLOYED** | To move or cause to<br>move from a specified<br>position of storage and<br>into operation | WHEN THE THRUST<BR>REVERSER DEPLOYS,<BR>KEEP PERSONNEL<BR>AWAY FROM THE<BR>AIRCRAFT. <br> DEPLOY THE SLIDE<BR>RAFT. |  |
| **deposit (n) — UNNAPPROVED** | PARTICLE (n)<br>CONTAMINATION (n) | IF THERE ARE METAL<BR>PARTICLES IN THE OIL<BR>FILTER, EXAMINE THE<BR>FILTER ELEMENT FOR<BR>WEAR. <br> FLUSH THE PIPES TO<BR>REMOVE<BR>CONTAMINATION. | If there are metal<BR>deposits in the oil filter,<BR>check the filter element<BR>for wear. <br> Flush the pipes to<BR>remove deposits. |
| **depress (v) — UNNAPPROVED** | PUSH (v) | PUSH THE BUTTON<BR>AND THEN RELEASE<BR>IT. | Depress and release the<BR>button. |
| **depressurize (v) — UNNAPPROVED** | PRESSURE (TN) | RELEASE THE<BR>PRESSURE FROM THE<BR>HYDRAULIC SYSTEM. | Depressurize the<BR>hydraulic system. |
| **DEPTH (n)** | The distance from the<BR>top down, from the<BR>surface down, from the<BR>front surface to the rear<BR>surface | MEASURE THE DEPTH<BR>OF THE DENT AS<BR>SHOWN IN FIGURE 4. |  |
| **describe (v) — UNNAPPROVED** | GIVE (v) | THIS SECTION GIVES<BR>THE PROCEDURES<BR>FOR THE LEAK TEST<BR>OF THE SYSTEM. | This section describes<BR>the procedures for<BR>testing the system for<BR>leaks. |
| **deselect (v) — UNNAPPROVED** | CANCEL (v) | PUSH THE BUTTON TO<BR>CANCEL THE FREEZE<BR>MODE. | <BR>Press the button to<BR>deselect the freeze<BR>mode. |

# Page 206 of 434

| Word (part of speech) | Approved meaning/ALTERNATIVES | STE EXAMPLE | Non-STE example |
|---|---|---|---|
| **design (v) — UNNAPPROVED** | HAVE (v) | THE MAIN LANDING<BR>GEAR DOORS HAVE<BR>STEPS FOR ACCESS<BR>TO THE LANDING<BR>GEAR BAY. | The main landing gear<BR>doors are designed with<BR>steps for access to the<BR>landing gear bay. |
| **desired (adj) — UNNAPPROVED** | NECESSARY (adj)<br>CORRECT (adj) | ADD THE NECESSARY<BR>QUANTITY OF OIL. <br> TIGHTEN THE<BR>TURNBUCKLE UNTIL<BR>THE TENSION IN THE<BR>CABLE IS CORRECT. | Add the desired quantity<BR>of oil. <br> Tighten the turnbuckle<BR>until you have the<BR>desired tension in the<BR>cable. |
| **destroy (v) — UNNAPPROVED** | BREAK (v) | BREAK THE<BR>CONTAINER TO MAKE<BR>SURE THAT YOU<BR>CANNOT USE IT<BR>AGAIN. | To prevent further use,<BR>destroy the container. |
| **detach (v) — UNNAPPROVED** | DISCONNECT (v)<br>DISENGAGE (v)<br>REMOVE (v) | DISCONNECT THE<BR>PIPELINE FROM THE<BR>UNION. <br> BEFORE YOU MOVE<BR>THE CONTROLS,<BR>DISENGAGE THE<BR>LOCKS. <br> DO NOT REMOVE THE<BR>PROTECTIVE LAYER. | Detach the pipeline from<BR>the union. <br> Before moving the<BR>controls, detach the<BR>locks. <br> Do not detach the<BR>protective film. |
| **detail (n) — UNNAPPROVED** | INSTRUCTION (n) | THIS PROCEDURE<BR>GIVES THE<BR>INSTRUCTIONS TO<BR>ATTACH THE PYLON. | This procedure gives<BR>details on how to attach<BR>the pylon. |
| **detail (v) — UNNAPPROVED** | GIVE (v)<br>REFER (v)<br>SPECIFIED (adj) | THIS SECTION GIVES<BR>THE REMOVAL/<BR>INSTALLATION<BR>INSTRUCTIONS. <br> DO THE LEAK TEST<BR>(REFER TO<BR>PARAGRAPH 4.0). <br> DO THE LEAK TEST AS<BR>SPECIFIED IN<BR>PARAGRAPH 4.0. | This section details the<BR>Removal / Installation<BR>instructions. <br> Do the leak test as<BR>detailed in<BR>paragraph 4.0. <br> <BR>Do the leak test as<BR>detailed in<BR>paragraph 4.0. |

# Page 207 of 434

| Word (part of speech) | Approved meaning/ALTERNATIVES | STE EXAMPLE | Non-STE example |
|---|---|---|---|
| **detect (v) — UNNAPPROVED** | FIND (v)<br>SENSE (v) | TO FIND DAMAGE ON<BR>WIRES, RUB A CLOTH<BR>ALONG THEM. <br> THE COMPUTER<BR>SENSES THE<BR>DIFFERENCES<BR>BETWEEN THE<BR>SIGNALS. | To detect damage to<BR>wires, rub a cloth along<BR>them. <br> The computer detects<BR>discrepancies between<BR>the signals. |
| **DETERIORATION**<br>**(n)** | A worse condition | THIS CONDITION WILL<BR>CAUSE<BR>DETERIORATION OF<BR>THE SURFACE. |  |
| **determine (v) — UNNAPPROVED** | FIND (v)<br>GIVE (v)<br>SELECT (v)<br>CALCULATE (v) | FIND THE DEFECTS IN<BR>THE SYSTEM. <br> DIMENSIONS 1 AND 2<BR>GIVE THE CORRECT<BR>POSITION. <br> SELECT THE<BR>HYDRAULIC SYSTEM<BR>THAT YOU WILL<BR>PRESSURIZE. <br> CALCULATE THE<BR>DIMENSION OF THE<BR>SHIM WITH THIS<BR>FORMULA: | Determine the defects in<BR>the system. <br> The correct position is<BR>determined by<BR>dimensions 1 and 2. <br> Determine which<BR>hydraulic system you will<BR>pressurize. <br> Determine the dimension<BR>of the shim with this<BR>formula: |
| **detrimental (adj) — UNNAPPROVED** | DANGEROUS (adj)<br>DAMAGE (n) | HYDRAULIC FLUID IS<BR>DANGEROUS FOR<BR>YOUR HEALTH. <br> SMALL QUANTITIES<BR>OF SURFACE<BR>BLOOMING, WHICH<BR>CAN OCCUR ON<BR>ITEMS IN STORAGE,<BR>DO NOT CAUSE<BR>DAMAGE TO THE<BR>COMPONENT. | Hydraulic fluid is<BR>detrimental to health. <br> Light surface blooming,<BR>which can occur on<BR>items in storage, is not<BR>detrimental to the<BR>component. |

# Page 208 of 434

| Word (part of speech) | Approved meaning/ALTERNATIVES | STE EXAMPLE | Non-STE example |
|---|---|---|---|
| **develop (v) — UNNAPPROVED** | START (v)<br>CAUSE (v) | IF A FIRE STARTS,<BR>OPERATE THE FIRE<BR>SHUTOFF VALVE. <br> DO NOT LET<BR>HYDRAULIC FLUID<BR>STAY ON YOUR SKIN.<BR>HYDRAULIC FLUID<BR>CAN CAUSE<BR>DERMATITIS. | If a fire develops,<BR>operate the fire shutoff<BR>valve. <br> Do not leave hydraulic<BR>fluid on your skin, as<BR>dermatitis could develop. |
| **deviate (v) — UNNAPPROVED** | OBEY (v) | PERSONNEL MUST<BR>OBEY THIS<BR>PROCEDURE. | Personnel must not<BR>deviate from this<BR>procedure. |
| **DEVICE (n)** | Something used to do a<BR>task | INSTALL THE SAFETY<BR>DEVICES. |  |
| **devise (v) — UNNAPPROVED** | MAKE (v)<br>FIND (v) | IF THE HOLDING<BR>FIXTURE IS NOT<BR>AVAILABLE, MAKE A<BR>SUPPORT FROM THE<BR>SHIPPING<BR>CONTAINER. <br> FIND NEW<BR>TROUBLESHOOTING<BR>PROCEDURES. | If the holding fixture is<BR>not available, devise one<BR>from the shipping<BR>container. <br> Devise new<BR>troubleshooting<BR>procedures. |
| **diagnose (v) — UNNAPPROVED** | FIND (v) | FIND THE CAUSE OF<BR>THE MALFUNCTION. | Diagnose the cause of<BR>the malfunction. |
| **DIAGONALLY**<br>**(adv)** | In a diagonal direction | APPLY THE FIRST<BR>LAYER OF TAPE<BR>ACROSS THE CUTOUT<BR>AND THE SECOND<BR>AND THIRD LAYERS<BR>DIAGONALLY. |  |
| **diametrically (adv) — UNNAPPROVED** | OPPOSITE (adj) | MAKE SURE THAT THE<BR>TWO OPPOSITE<BR>V-GROOVES ALIGN<BR>WITH THE RAILS. | <BR>Ensure the two<BR>diametrically opposed<BR>V-grooves are in line<BR>with the rails. |
| **differ (v) — UNNAPPROVED** | DIFFERENT (adj) | IF THE VALUES ARE<BR>DIFFERENT, DO THIS<BR>TEST. | If the values differ, do<BR>the following test. |
| **DIFFERENCE (n)** | That which is different<BR>between two quantities,<BR>numbers, or functions | THE DIFFERENCE<BR>BETWEEN THE TWO<BR>DIMENSIONS MUST<BR>NOT BE MORE THAN<BR>0.10 mm. |  |
