# Page 381–384 of 434

> **Source:** ASD-STE100 Issue 9, January 2025
> **Pages:** 381–384 of 434

# Page 381 of 434

| **Word**<br>**(part of speech)** | **Approved meaning/**<br>**ALTERNATIVES** | **STE EXAMPLE** | **Non-STE example** |
|---|---|---|---|
| **still (adv) — UNNAPPROVED** | STAY (v)<br>CONTINUE (v) | MAKE SURE THAT THE<BR>“OVHT” LIGHT STAYS<BR>ON.<br>MAKE SURE THAT THE<BR>ROTOR CONTINUES<BR>TO TURN. | <BR>Make sure that the<BR>“OVHT” light is still<BR>illuminated.<br><BR>Make sure that the rotor<BR>still turns. |
| **stimulate (v) — UNNAPPROVED** | INCREASE (v) | INCREASE THE<BR>AIRFLOW. | Stimulate the airflow. |
| **stir (v) — UNNAPPROVED** | MIX (v) | MIX THE BONDING<BR>MATERIAL WITH A<BR>SPATULA. | Stir the bonding material<BR>with a spatula. |
| **STOP (v),**<br>**STOPS,**<br>**STOPPED,**<br>**STOPPED** | 1.<br>To cause the end<br>of a procedure,<br>movement, or an<br>operation<br>2.<br>To come to an end | STOP THE ENGINE.<br>WHEN THE FLOW<BR>STOPS, REMOVE THE<BR>DRAIN HOSE. |  |
| **store (v) — UNNAPPROVED** | KEEP (v)<br>CONTAIN (v)<br>STORAGE (TN) | KEEP THE<BR>CARTRIDGES IN A<BR>SAFETY AREA.<br>THE FIRE<BR>EXTINGUISHER<BR>BOTTLES CONTAIN A<BR>DRY CHEMICAL<BR>POWDER AGENT.<br>WHEN YOU PUT THE<BR>UNIT INTO STORAGE,<BR>OBEY THE<br>APPLICABLE<BR>STORAGE<br>INSTRUCTIONS. | Cartridges should be<BR>stored in a safety area.<br>The fire extinguisher<BR>bottles store a dry<BR>chemical powder agent.<br>When you store the unit,<br>obey the applicable<br>storage instructions. |
| **STOW (v),**<br>**STOWS,**<br>**STOWED,**<br>**STOWED** | To move or cause to<br>move into a specified<br>position of storage. | STOW THE LIFE VEST<br>SAFELY BELOW THE<br>PASSENGER SEAT.<br>MAKE SURE THAT THE<br>THRUST REVERSER<BR>STOWS WHEN YOU<br>PUSH THE QUADRANT<br>CONTROL FORWARD. |  |

# Page 382 of 434

| **Word**<br>**(part of speech)** | **Approved meaning/**<br>**ALTERNATIVES** | **STE EXAMPLE** | **Non-STE example** |
|---|---|---|---|
| **STRAIGHT (adj)**<br>**(STRAIGHTER,**<br>**(STRAIGHTEST)** | Without curves or bends | MAKE SURE THAT THE<br>STRAIGHT PART OF<br>THE RIGGING PIN IS<br>SMOOTH. |  |
| **straighten (v) — UNNAPPROVED** | STRAIGHT (adj) | DO NOT TRY TO MAKE<br>THE BENDS IN THE<br>CABLE STRAIGHT. | Do not try to straighten<br>the bends in the cable. |
| **strain (v) — UNNAPPROVED** | FILTER (TN)<br>STRAIN (TN) | BEFORE YOU USE<br>THE OIL, PUT IT<br>THROUGH A FILTER.<br>DO NOT PUT STRAIN<br>ON THE BELLOWS. | Strain the oil before use.<br>Do not strain bellows. |
| **strap (v) — UNNAPPROVED** | ATTACH (v)<br>(WITH STRAPS [TN]) | ATTACH THE CABLES<br>TO THE STRUCTURE<br>WITH AN APPLICABLE<br>STRAP. | Strap the cables to the<br>structure. |
| **stress (v) — UNNAPPROVED** | FORCE (TN) | DO NOT PUT TOO<br>MUCH FORCE ON THE<br>DUCTING. | Do not stress the ducting<br>unnecessarily. |
| **strictly (adv) — UNNAPPROVED** | FULLY (adv) | FULLY OBEY THE<br>SAFETY<br>PRECAUTIONS. | Strictly obey the safety<br>precautions. |
| **strike (v) — UNNAPPROVED** | HIT (v) | MAKE SURE THAT THE<br>SLING DOES NOT HIT<br>THE SURFACE. | Make certain that the<br>sling does not strike the<br>surface. |
| **STRIP (n)** | A piece of material that<br>is long and thin, but not<br>wide | PUT A STRIP OF<br>ADHESIVE TAPE<br>ALONG THE<br>INSULATION BLANKET. |  |
| **strip (v) — UNNAPPROVED** | REMOVE (v) | REMOVE THE<br>INSULATION FROM<br>THE WIRE. | Strip the insulation from<br>the wire. |
| **STRIPE (n)** | A line on a surface which<br>is a different color | THE FLAG HAS RED<br>AND WHITE STRIPES. |  |
| **striped (adj) — UNNAPPROVED** | STRIPE (n) | THE FLAG HAS RED<br>AND WHITE STRIPES. | The flag is striped red<br>and white. |
| **stroke (n) — UNNAPPROVED** | TRAVEL (n) | TO BLEED THE<br>BRAKING SYSTEM,<br>OPERATE THE HAND<br>PUMP HANDLE<br>THROUGH ITS FULL<br>TRAVEL. | Bleed the braking<br>system by applying full<br>strokes to the hand<br>pump handle. |

# Page 383 of 434

| **Word**<br>**(part of speech)** | **Approved meaning/**<br>**ALTERNATIVES** | **STE EXAMPLE** | **Non-STE example** |
|---|---|---|---|
| **STRONG (adj)**<br>**(STRONGER,**<br>**(STRONGEST)** | With much strength,<br>power, or concentration | WHEN WINDS ARE<br>STRONG, MOOR THE<br>AIRCRAFT<br>CAREFULLY. |  |
| **STRUCTURAL**<br>**(adj)** | Related to the structure | THE CHASSIS IS A<br>STRUCTURAL<br>COMPONENT OF THE<br>VEHICLE. |  |
| **STRUCTURALLY**<br>**(adv)** | Related to the structure | THE LIST GIVES YOU<br>STRUCTURALLY<br>IMPORTANT ITEMS. |  |
| **STRUCTURE (n)** | 1.<br>A construction<br>2.<br>The arrangement of<br>something | ATTACH THE WIRES<br>TO THE STRUCTURE.<br>THE INTRODUCTION<br>GIVES YOU THE<br>STRUCTURE OF THE<br>MAINTENANCE<br>MANUAL. |  |
| **SUBASSEMBLY**<br>**(n)** | An assembly that is a<br>part of a larger assembly | DO NOT CHANGE THE<br>POSITION OF THE<br>SUBASSEMBLIES. |  |
| **submerge (v) — UNNAPPROVED** | PUT (v) | PUT THE FILTER<br>ELEMENT FULLY INTO<br>THE FLUID. | Submerge the filter<br>element in the fluid. |
| **submit (v) — UNNAPPROVED** | SEND (v) | SEND THE METAL<br>PARTICLES TO A<br>LABORATORY FOR<br>ANALYSIS. | Submit the metal<br>particles to a laboratory<br>for analysis. |
| **SUBSEQUENT**<br>**(adj)** | Following in an<br>unspecified time or<br>sequence<br>Use NEXT (adj)<br>for the first<br>occurrence that<br>follows<br>immediately in<br>time or sequence. | A SUBSEQUENT<br>REPAIR WILL BE FOR<br>THE NEW<br>CONFIGURATION<br>ONLY.<br>DO THE NEXT<br>INSPECTION. | Do the immediately<br>subsequent inspection. |

# Page 384 of 434

| **Word**<br>**(part of speech)** | **Approved meaning/**<br>**ALTERNATIVES** | **STE EXAMPLE** | **Non-STE example** |
|---|---|---|---|
| **SUBSEQUENTLY**<br>**(adv)** | After an unspecified time<br>Use THEN (adv)<br>for an occurrence<br>that follows<br>immediately in<br>time or sequence.<br> | MAKE SURE THAT THE<BR>TOOL IS<br>SUBSEQUENTLY<br>AVAILABLE FOR THE<br>INSTALLATION<br>PROCEDURE.<br>LIFT THE COVER.<br>THEN, PULL THE<BR>HANDLE.<br> | Lift the cover and<br>subsequently pull the<br>handle.<br> |
| **subsequent to**<br>**(prep)** | AFTER (conj) | AFTER YOU INSTALL<BR>THE COMPONENT,<br>REMOVE THE<BR>HANDLING TOOL. | Remove the handling<br>tool subsequent to the<br>installation of the<br>component. |
| **substance (n) — UNNAPPROVED** | MATERIAL (n) | THE PRIMER<br>CONTAINS A<br>MATERIAL THAT<br>PREVENTS<br>CORROSION. | The primer contains a<br>substance that prevents<br>corrosion. |
| **substitute (adj) — UNNAPPROVED** | EQUIVALENT (adj)<br>ALTERNATIVE (adj) | IF THE SPECIFIED<br>MATERIAL IS NOT<br>AVAILABLE, YOU CAN<br>USE AN EQUIVALENT<br>ONE.<br>IF THIS SPECIAL TOOL<br>IS NOT AVAILABLE,<br>USE AN ALTERNATIVE<br>METHOD. | A substitute material<br>may be used if the<br>specified one is not<br>available.<br>If this special tool is not<br>available, use a<br>substitute method. |
| **substitute (n) — UNNAPPROVED** | ALTERNATIVE (n) | YOU CAN USE<br>ALTERNATIVES FOR<br>THESE ITEMS. | Equivalent substitutes<br>may be used for these<br>items. |
| **substitute (v) — UNNAPPROVED** | REPLACE (v) | DO NOT REPLACE THE<br>SELF-LOCKING NUTS<br>WITH PLAIN NUTS. | Do not substitute the<br>self-locking nuts with<br>plain nuts. |
| **SUBTRACT (v),**<br>**SUBTRACTS,**<br>**SUBTRACTED,**<br>**SUBTRACTED** | To take from a number<br>or quantity | SUBTRACT<br>COEFFICIENT "A"<br>FROM THE<br>INDICATION. |  |
