# Page 189 of 434

**Page 2-1-C14**

**Page 2-1-C14 Part 2 - Dictionary**

**Issue 9 2025-01-15**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
||---|---|---|---|
||**COMPONENT (n)**|A part, subassembly, or<br>unit that has a specified<br>function|CLEAN THESE<br>COMPONENTS WITH<br>APPROVED<br>SOLVENTS.|
||**comprehensive**<br>**(adj)**|FULL (adj)|DO A FULL<brINSPECTION OF THE<br>FAIRING.|Do a comprehensive<br>inspection of the fairing.|
||**COMPRESS (v),**<br>**COMPRESSES,**<br>**COMPRESSED,**<br>**COMPRESSED**|To decrease or cause to<br>decrease in dimension<br>or volume|COMPRESS THE<br>SPRING AND<br>CAREFULLY INSTALL<br>THE COVER.|
||||WHEN THE SPRING<br>COMPRESSES, THE<br>VALVE OPENS.|
||**comprise (v) — UNNAPPROVED**|HAVE (v)|THE VALVE<br>ASSEMBLY HAS<br>THESE PARTS:|The valve assembly<br>comprises these parts:|
|||CONTAIN (v)|EACH SURVIVAL KIT<br>CONTAINS THESE<br>ITEMS.|Each survival kit<br>comprises these items.|
||**compulsory (adj) — UNNAPPROVED**|MANDATORY (adj)|BEFORE YOU INSTALL<br>A NEW COMPONENT,<br>IT IS MANDATORY TO<br>REPLACE THE<br>FILTER.|Before you install a new<br>component, it is<br>compulsory to replace the<br>filter.|
||**compute (v) — UNNAPPROVED**|CALCULATE (v)|CALCULATE THE<br>VOLTAGE IN THE<br>CIRCUIT.|Compute the voltage in<br>the circuit.|
||**concentrate (v) — UNNAPPROVED**|ALL (adj)|ALL THE WEIGHT<br>MUST BE ON THE<br>SPAR TIP.|The weight must be<br>concentrated on the spar<br>tip.|
||**CONCENTRATION**<br>**(n)**|The strength of<br>something contained in a<br>mixture|<br>IN A HIGH<br>CONCENTRATION,<br>THIS MATERIAL IS<br>POISONOUS.|
||**CONCENTRIC (adj)**|That has a common<br>center|THE EXTERNAL<br>DIAMETER MUST BE<br>CONCENTRIC TO THE<br>INTERNAL DIAMETER.|
||**concern (v) — UNNAPPROVED**|APPLICABLE (adj)|THIS PROCEDURE IS<br>APPLICABLE ONLY TO<br>A TYPE B UNIT.|This procedure only<br>concerns a Type B unit.|

# Page 190 of 434

**Page 2-1-C15**

**Page 2-1-C15**

**Issue 9 2025-01-15**

**Part 2 - Dictionary**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
||---|---|---|---|
||**conclusion (n) — UNNAPPROVED**|END (n)|AT THE END OF THE<br>TEST, SET THE<br>SWITCH TO "NORMAL."|
|At the conclusion of the<br>test, you must switch to<br>NORMAL.|
|||RESULT (n)|IF THE RESULTS OF<br>THE TEST ARE<br>UNSATISFACTORY,<br>REPLACE THE UNIT.|If the conclusions of the<br>test are unsatisfactory,<br>replace the unit.|
||**concurrently (adj) — UNNAPPROVED**|AT THE SAME TIME|DO THESE TWO<br>PROCEDURES AT THE<br>SAME TIME.|These two procedures<br>must be applied<br>concurrently.|
||**CONDENSATION**<br>**(n)**|The result when a gas<br>changes into a liquid|SET THE SWITCH TO<br>THE "ON" POSITION<br>TO REMOVE THE<br>CONDENSATION.|

||**CONDITION (n)**|1.
Something that is<br>necessary for what<br>occurs|THESE INITIAL<br>CONDITIONS ARE<br>NECESSARY TO GET<br>CORRECT RESULTS.|

||

|2.
The state of an item|DO A CHECK OF THE<br>UNIT CONDITION.|

||
|Use IF (conj) for<br>"on the condition<br>that."|IF THERE IS NO WIND,<br>DO THE TEST<br>OUTDOORS.|On the condition that<br>there is no wind, do the<br>test outdoors.|
||**conduct (v) — UNNAPPROVED**|DO (v)|DO THE LEAK TEST.|Conduct the leak test.|
||**confine to (v) — UNNAPPROVED**|ONLY (adv)|IF THE DAMAGE IS<br>ONLY TO THE MIDDLE<br>TREADS, THE TIRE IS<br>SERVICEABLE.|If the damage is confined<br>to the middle treads, the<br>tire is serviceable.|
||**confirm (v) — UNNAPPROVED**|MAKE SURE (v)|DO A GROUND RUN<br>OF THE ENGINE TO<br>MAKE SURE THAT<br>YOU GET THE SAME<br>INDICATIONS.|Do a ground run of the<br>engine to confirm the<br>indications.|
||**conflict (n) — UNNAPPROVED**|DIFFERENT (adj)|IF THE TWO<br>INDICATIONS ARE<br>DIFFERENT, DO THE<br>TEST AGAIN.|If there is a conflict<br>between the two<br>indicators, repeat the test.|
||
|AGREE (v)|IF THE TWO<br>INDICATIONS DO NOT<br>AGREE, DO THE TEST<br>AGAIN.|If there is a conflict<br>between the two<br>indicators, repeat the test.|

# Page 191 of 434

**Page 2-1-C16**

**Page 2-1-C16**

**Issue 9 2025-01-15**

**Part 2 - Dictionary**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
||---|---|---|---|
||**conform (v) — UNNAPPROVED**|AGREE (v)|IF THE FLAP<br>EXTENSION DOES<br>NOT AGREE WITH THE<br>POSITION OF THE<br>FLAP CONTROL<br>LEVER, DO THE<br>RIGGING PROCEDURE<br>AGAIN.|If the flap extension does<br>not conform to the setting<br>of the flap control lever,<br>do the rigging procedure<br>again.|
||**conformance (n) — UNNAPPROVED**|AGREE (v)|THE INDICATIONS<br>MUST AGREE WITH<br>THOSE IN TABLE 2.|The indications must be<br>in conformance with<br>those in Table 2.|
||**conformity (n) — UNNAPPROVED**|AGREE (v)|THE PRECISION OF<br>THE GAUGES MUST<br>AGREE WITH THE<br>APPLICABLE QUALITY<br>STANDARD.|The accuracy of the<br>gauges must be in<br>conformity with the<br>applicable quality<br>standard.|
||**CONNECT (v),**<br>**CONNECTS,**<br>**CONNECTED,**<br>**CONNECTED**|To come together or<br>cause to come together<br>to make one unit or<br>system|CONNECT THE<br>ELECTRICAL<br>CONNECTORS TO THE<br>INSTRUMENT.|
||
|PLUG "A" CONNECTS<br>TO SOCKET "B".|
||**CONNECTION (n)**|That which connects or<br>is connected|MAKE SURE THAT ALL<br>THE FUEL AND AIR<br>CONNECTIONS ARE<br>INSTALLED.|
||**consecutive (adj) — UNNAPPROVED**|ONE (TN) AFTER THE<br>OTHER|DO NOT DO MORE<br>THAN THREE STARTS,<br>ONE AFTER THE<br>OTHER.|Do not do more than<br>three consecutive starts.|
||**consecutively**<br>**(adv)**|ONE (TN) AFTER THE<br>OTHER|DO THESE STEPS ONE<br>AFTER THE OTHER.|
|These actions must be<br>done consecutively.|
||
|SEQUENCE (n)|DO THE WORK STEPS<br>IN SEQUENCE.|Do the work steps<br>consecutively.|
||**consequence (n) — UNNAPPROVED**|BECAUSE OF (prep)|BECAUSE OF THIS<br>DEFECT, THE UNIT<br>WILL NOT OPERATE.|As a consequence of this<br>defect, the unit will not<br>operate.|

# Page 192 of 434

**Page 2-1-C17**

**Page 2-1-C17**

**Issue 9 2025-01-15**

**Part 2 - Dictionary**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
||---|---|---|---|
||**consider (v) — UNNAPPROVED**|THINK (v)|IF YOU THINK THAT<br>THE INDICATION IS<br>NOT CORRECT, DO<br>THE TEST AGAIN.|If you consider that the<br>indication is not correct,<br>do the test again.|
||**considerable (adj) — UNNAPPROVED**|LARGE (adj)|CLEAN YOUR SKIN<br>WITH A LARGE<br>QUANTITY OF WATER.|Clean your skin with a<br>considerable quantity of<br>water.|
||
|IMPORTANT (adj)|CONTAMINATION OF<br>CABIN AIR CAN BE AN<BR>IMPORTANT<br>PROBLEM.|Contamination of cabin<br>air can be a considerable<br>problem.|
||
|DANGEROUS (adj)|HYDRAULIC FLUID IS<br>DANGEROUS FOR<br>YOUR EYES.|Hydraulic fluid can cause<br>considerable eye injury.|
||**consist of (v) — UNNAPPROVED**|HAVE (v)|EACH ANTENNA HAS<br>THREE PARTS.|Each antenna consists of<br>three parts.|
||**consistent (adj) — UNNAPPROVED**|AGREE (v)|MAKE SURE THAT THE<br>INDICATIONS AGREE<br>WITH THE POSITION<br>OF THE FLAPS.|
|Check that the<br>indications are consistent<br>with the position of the<br>flaps.|
||**CONSTANT (adj)**|That continues to be the<br>same, without change|MAKE SURE THAT THE<br>CABIN PRESSURE<br>STAYS CONSTANT.|
||**CONSTANTLY**<br>**(adv)**|Incessantly|THE INSTRUMENT<br>WILL CONSTANTLY<br>SHOW THIS VALUE.|
||**construct (v) — UNNAPPROVED**|ASSEMBLE (v)|ASSEMBLE THE UNIT.|Construct the unit.|
||**consult (v) — UNNAPPROVED**|REFER (v)|FOR MORE<BR>INFORMATION, REFER<BR>TO THE USER'S<BR>MANUAL.|For more information,<br>consult the User's<br>Manual.|
||**CONTACT (v)**<br>**CONTACTS,**<br>**CONTACTED**|To start communication|CONTACT CUSTOMER<BR>SERVICES.|
||

**,**
**CONTACTED**|For other<br>meanings, use:|

||
|TOUCH (v)|TIGHTEN THE<br>FIXTURE SCREW<br>UNTIL IT TOUCHES<br>THE SURFACE.|Tighten the fixture screw<br>until it contacts the<br>surface.|
