# Page 421–424 of 434

> **Source:** ASD-STE100 Issue 9, January 2025
> **Pages:** 421–424 of 434

# Page 421 of 434

| **Word (part of speech)** | **Approved meaning/ALTERNATIVES** | **STE EXAMPLE** | **Non-STE example** |
|---|---|---|---|
| **WITH (prep)** | Function word that<br>shows association or<br>relationship, help or<br>sharing, a means or<br>instrument | ALIGN THE MARK<br>WITH THE<br>LONGITUDINAL AXIS.<br>Refer to<br>section 9, GR-2.<br>ATTACH THE FLANGE<br>(10) WITH THE FOUR<br>BOLTS (15).<br>REMOVE THE<br>VALVE (2) WITH THE<br>EXTRACTOR. |  |
| **withdraw (v) — UNNAPPROVED** | REMOVE (v) | REMOVE THE<br>INDICATOR FROM THE<br>INSTRUMENT PANEL. | Withdraw the indicator<br>from the instrument<br>panel. |
| **within (prep) — UNNAPPROVED** | IN (prep)<br>IN ... OR LESS<br>IN LESS THAN | A FILTER PREVENTS<br>CONTAMINATION OF<br>THE COMPONENTS IN<br>THE SYSTEM.<br>LIGHT L4 COMES ON<br>IN 5 SECONDS OR<br>LESS.<br>MAKE SURE THAT THE<br>WARNING LIGHT<br>COMES ON IN LESS<br>THAN 3 SECONDS. | A filter prevents<br>contamination of the<br>components within the<br>system.<br>Light L4 illuminates<br>within 5 seconds.<br>Make sure that the<br>warning light illuminates<br>within 3 seconds. |
| **WITHOUT (prep)** | Not with | SMALL DAMAGE IS<br>PERMITTED WITHOUT<br>REPAIR. REFER TO<br>TABLE 1 FOR THE<br>APPLICABLE LIMITS. |  |
| **withstand (v) — UNNAPPROVED** | RESISTANT (adj) | THIS MATERIAL IS<br>RESISTANT TO FIRE. | This material can<br>withstand fire. |
| **WORK (n)** | That which you do when<br>you use physical<br>strength, or mental<br>power | DO THE WORK IN A<br>CLEAN AREA. |  |
| **work (v) — UNNAPPROVED** | WORK (n) | BE CAREFUL WHEN<br>YOU DO WORK NEAR<br>FUEL TANKS. | Be careful when you<br>work near fuel tanks. |
| **would (v) — UNNAPPROVED** | CAN (v) | SOLVENTS THAT STAY<br>ON THE PART CAN<br>CAUSE CORROSION. | <br>Solvents left on the part<br>would corrode the part. |

# Page 422 of 434

| **Word (part of speech)** | **Approved meaning/ALTERNATIVES** | **STE EXAMPLE** | **Non-STE example** |
|---|---|---|---|
| **wrap (v) — UNNAPPROVED** | PUT (v)<br>WIND (v) | PUT THE PART IN<br>OILPAPER.<br>WIND MASKING TAPE<br>AROUND THE PART. | Wrap the part in<br>oilpaper.<br>Wrap masking tape<br>around the part. |
| **WRITE (v),**<br>**WRITES,**<br>**WROTE,**<br>**WRITTEN** | To record data or<br>information as words,<br>letters, or symbols | WRITE THE TEST<br>DATE ON THE<br>CERTIFICATE. |  |
| **wrong (adj) — UNNAPPROVED** | INCORRECT (adj) | IDENTIFY THE<br>BELLCRANK AND<br>SHAFT WITH MARKS.<br>THESE MARKS WILL<br>PREVENT AN<br>INCORRECT<br>INSTALLATION. | Mark the bellcrank and<br>shaft to prevent wrong<br>installation. |
| **wrongly (adv) — UNNAPPROVED** | INCORRECTLY (adv) | IF THE HOSES ARE<br>INCORRECTLY<br>INSTALLED, DAMAGE<br>CAN OCCUR. | Damage can occur if<br>hoses are wrongly<br>installed. |

# Page 423 of 434

Blank Page

# Page 424 of 434

| **Word (part of speech)** | **Approved meaning/ALTERNATIVES** | **STE EXAMPLE** | **Non-STE example** |
|---|---|---|---|
| **YES (adv)** | Function word that<br>shows the positive<br>answer to a question | DOES THE LIGHT<br>COME ON? YES OR<br>NO? |  |
| **yet (conj) — UNNAPPROVED** | BUT (conj) | TIGHTEN THE NUTS,<br>BUT KEEP THEM<br>SUFFICIENTLY LOOSE<br>TO REMOVE THEM<br>WITH YOUR HAND. | The nuts should be<br>tightened, yet loose<br>enough to remove by<br>hand. |
| **yet (adv) — UNNAPPROVED** | AT THIS TIME | DO NOT REMOVE THE<br>FIXTURE COVER AT<br>THIS TIME. | Do not remove the<br>fixture cover yet. |
| **YOU (pron)** | The reader or the user | YOU CAN CONTINUE<br>THE TEST.<br>HOT SURFACES CAN<br>BURN YOU. |  |
| **YOUR (adj)** | Related to the reader or<br>the user | IF YOU GET SOLVENT<br>IN YOUR EYES, FLUSH<br>THEM IMMEDIATELY<br>WITH WATER. |  |
| **yourself (pron) — UNNAPPROVED** | YOU (pron) | DO NOT USE YOUR<br>HANDS TO PREVENT<br>MOVEMENT OF THE<br>LP COMPRESSOR. IF<br>YOU DO, THE LP<br>COMPRESSOR CAN<br>CAUSE YOU INJURY<br>AND CAN CAUSE<br>DAMAGE TO THE<br>EQUIPMENT. | Do not use your hands<br>to prevent movement of<br>the LP compressor. If<br>you do, you can cause<br>injury to yourself and<br>damage to the<br>equipment. |
| **zero (v) — UNNAPPROVED** | ZERO (TN) | ADJUST THE METER<br>TO ZERO. | Zero the meter. |
