# Page 177–180 of 434

> **Source:** ASD-STE100 Issue 9, January 2025
> **Pages:** 177–180 of 434

# Page 177 of 434

| Word (POS) | Approved meaning / ALTERNATIVES | STE example | Non-STE example |
|------------|--------------------------------|-------------|-----------------|
| care (n) — UNNAPPROVED | PRECAUTION (n) | WHEN YOU DO WORK WITH HIGH VOLTAGES, OBEY THE SAFETY PRECAUTIONS. | You must take care when you work with high voltages. |
|  | CAREFUL (adj) | BE CAREFUL WHEN YOU INSTALL THE NUTS. | Take care when installing the nuts. |
|  | CAREFULLY (adv) | REMOVE THE GEARBOX CAREFULLY. | Remove the gearbox with great care. |
| CAREFUL (adj) | With precaution | BE CAREFUL WHEN YOU REMOVE THE COVER. |  |
| CAREFULLY (adv) | In a careful manner | CAREFULLY APPLY A BEAD OF SEALING COMPOUND. |  |
| carry (v) — UNNAPPROVED | TRANSMIT (v) | THE CABLE TRANSMITS THE ELECTRICAL ENERGY FROM THE IGNITION EXCITER TO THE IGNITER. | The cable carries the electrical energy from the ignition exciter to the igniter. |
|  | TRANSPORT (TN) | THIS VEHICLE IS FOR THE TRANSPORT OF FIVE PASSENGERS. | This vehicle is meant to carry five passengers. |
| carry out (v) — UNNAPPROVED | DO (v) You can use a more accurate command verb. | DO THE LEAK TEST. | Carry out the leak test. |
|  | MEASURE (v) | MEASURE THE CLEARANCE OF THE IMPELLER. | Carry out the clearance measurement of the impeller. |
| case (n) — UNNAPPROVED | CONDITION (n) | FIGURE 1 SHOWS THE DATA FOR ALL OPERATIONAL CONDITIONS. | The data for all operational cases are shown in Figure 1. |
| case (in case of) (conj) | IF (conj) | IF THERE IS A FIRE, OPERATE THE CRASH SWITCHES. | In case of a fire, operate the crash switches. |

# Page 178 of 434

| Word (POS) | Approved meaning / ALTERNATIVES | STE example | Non-STE example |
|------------|--------------------------------|-------------|-----------------|
| CATCH (v), CATCHES, CAUGHT, CAUGHT | To stop or prevent the movement of something | THE LUG ON THE PANEL OPENING CATCHES THE BOTTOM OF THE DRAWER. |  |
|  | For other meanings, use: | DO NOT LET THE TOOL CATCH ON THE PANEL. |  |
|  | COLLECT (v) | COLLECT THE LEAKAGE IN A GRADUATED BEAKER. | Catch the leakage in a graduated beaker. |
| categorize (v) — UNNAPPROVED | CATEGORY (TN) | THE TESTING EQUIPMENT DIVIDES THE FAULTS INTO CATEGORIES. | The testing equipment categorizes the faults. |
| CAUSE (n) | Something that brings about a result | DO THE TROUBLESHOOTING PROCEDURE TO FIND THE CAUSE OF THE MALFUNCTION. |  |
| CAUSE (v), CAUSES, CAUSED, CAUSED | To be the cause of | METAL OBJECTS CAN CAUSE MAGNETIC INTERFERENCE. |  |
| caution (v) — UNNAPPROVED | TELL (v) | TELL ALL PERSONNEL NOT TO SMOKE NEAR FUEL TANKS. | Caution all personnel not to smoke near fuel tanks. |
| cautiously (adv) — UNNAPPROVED | CAREFULLY (adv) | CAREFULLY FEEL THE HEATER WITH YOUR HANDS TO MAKE SURE THAT IT OPERATES. | Cautiously feel the heater with your hands to make sure that it operates. |
| cavity (n) — UNNAPPROVED | HOLE (n) | FILL THE HOLE WITH RESIN. | Fill the cavity with resin. |
|  | SPACE (n) | FILL THE SPACE BETWEEN THE PATCH AND THE ADJACENT STRUCTURE WITH SEALANT. | Fill the cavity between the patch and the adjacent structure with sealant. |
| cease (v) — UNNAPPROVED | STOP (v) | THE WARNING STOPS AT 17 DEG. | The warning ceases at 17 deg. |

# Page 179 of 434

| Word (POS) | Approved meaning / ALTERNATIVES | STE example | Non-STE example |
|------------|--------------------------------|-------------|-----------------|
| center (v) — UNNAPPROVED | CENTER (TN) | ALIGN THE PISTON WITH THE CENTER OF THE SLEEVE. | Center the piston in the sleeve. |
| centralize (v) — UNNAPPROVED | CENTER (TN) | SET THE CONTROLS TO THE CENTER POSITION. | Centralize the controls. |
| certain (adj) — UNNAPPROVED | SURE (adj) | IF YOU ARE NOT SURE THAT THE RESULTS ARE CORRECT, DO THE TEST AGAIN. | If you are not certain that the results are correct, do the test again. |
|  | SOME (adj) | SOME FUNCTIONS ARE NOT AVAILABLE. | Certain functions are not available. |
|  | SPECIFIED (adj) | THE SPECIFIED FUNCTIONS ARE NOT AVAILABLE. | Certain functions are not available. |
| certify (v) — UNNAPPROVED | WRITE (v) | WRITE THE CHANGE IN THE LOGBOOK. | Certify the change in the logbook. |
|  | APPROVAL (n) | GET APPROVAL FROM YOUR SUPERVISOR FOR THE REPAIR. | Get the supervisor to certify the repair. |
| chafe (v) — UNNAPPROVED | RUB (v) | DO NOT LET THE WIRES RUB. | Do not let the wires chafe. |
| chafed (adj) — UNNAPPROVED | WORN (adj) | EXAMINE THE TUBING FOR WORN AREAS. | Examine the tubing for chafed areas. |
| chance (by chance) (n) | RISK (n) | IF THERE IS A RISK OF FUEL LEAKAGE, PUT A CONTAINER BELOW THE UNIT. | If there is a chance of fuel leakage, put a container below the unit. |
|  | ACCIDENTALLY (adv) | IF THE LEVER MOVED ACCIDENTALLY, DO THE TEST AGAIN. | If, by chance, the lever moved, do the test again. |
| CHANGE (n) | That which occurs when something changes | THE COLOR CHANGE SHOWS THAT THE TEMPERATURE IS TOO HIGH. |  |

# Page 180 of 434

| Word (POS) | Approved meaning / ALTERNATIVES | STE example | Non-STE example |
|------------|--------------------------------|-------------|-----------------|
| CHANGE (v), CHANGES, CHANGED, CHANGED | To become or to cause to become different | IF THE HUMIDITY CHANGES FREQUENTLY, PUT A COVER ON THE UNIT. |  |
|  | For other meanings, use: | CHANGE THE COLOR OF THE DISPLAY. |  |
|  | REPLACE (v) | REPLACE THE DAMAGED VALVE. | Change the damaged valve. |
| channel (v) — UNNAPPROVED | CHANNEL (TN) | INSTALL THE WIRES IN THE CHANNEL ALONG THE HOUSING. | Channel the wires along the housing. |
| characteristic (n) — UNNAPPROVED | PROPERTY (n) | THE PROPERTIES OF THESE SEALANTS PREVENT CORROSION. | The characteristics of these sealants prevent corrosion. |
|  | QUALITY (n) | DO NOT USE THIS MATERIAL BECAUSE IT DOES NOT HAVE THE NECESSARY QUALITIES. | Do not use this material because it doesn't have the necessary characteristics. |
| CHARGE (v), CHARGES, CHARGED, CHARGED | To accumulate or add electrical energy | CHARGE THE BATTERY.<br>MAKE SURE THAT THE BATTERY CHARGES. |  |
|  | For other meanings, use: |  |  |
|  | FILL (v) | FILL THE TANK WITH 10 LITERS OF METHANOL. | Charge the tank with 10 liters of methanol. |
|  | PRESSURIZE (v) | PRESSURIZE THE ACCUMULATOR WITH NITROGEN. | Charge the accumulator with nitrogen. |
| CHECK (n) | The procedure you do to make sure that something operates correctly or has no defects | DO A CHECK OF THE HYDRAULIC SYSTEM.<br>DO A CHECK FOR LOOSE FASTENERS. |  |
