# Page 261 of 434

**Page 2-1-H3**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
||---|---|---|---|
||**heat (v) — UNNAPPROVED**|HEAT (n)|USE HEAT TO<br>INCREASE THE<br>TEMPERATURE OF<br>THE OIL TO 40°C.|Heat the oil to 40°C.|
|||HOT (adj)|WHEN THE OIL IS HOT,<br>IT FLOWS FREELY.|<br>When you heat the oil, it<br>flows freely.|
||**HEAVY (adj)**<br>**(HEAVIER,**<br>**HEAVIEST)**|That has a large mass,<br>weight, or force|A SUPPORT WILL BE<br>NECESSARY<br>BECAUSE THE<br>CONTROL UNIT IS<br>HEAVY.|
||**HEIGHT (n)**|The vertical distance|THE HEIGHT FROM<br>THE GROUND TO THE<br>TOP OF THE FIN CAN<br>CHANGE.|
||**heighten (v) — UNNAPPROVED**|INCREASE (v)|STRONG WINDS WILL<br>INCREASE THE RISK<br>OF DAMAGE.|Strong winds will<br>heighten the risk of<br>damage.|
||**help (n) — UNNAPPROVED**|AID (n)|GET MEDICAL AID<br>IMMEDIATELY.|You must get medical<br>help immediately.|
||**HELP (v),**<br>**HELPS,**<br>**HELPED,**<br>**HELPED**|To make something<br>easier or better|PETROLATUM HELPS<br>TO PREVENT<br>CORROSION OF THE<br>TERMINALS.|
||**helpful (adj) — UNNAPPROVED**|HELP (v)|RECORD THE<br>LOCKWIRE<br>POSITIONS. THIS<br>INFORMATION WILL<br>HELP YOU DURING<br>THE ASSEMBLY<br>PROCEDURE.|Record the lockwire<br>positions. This will be<br>helpful during the<br>assembly procedure.|
||**HERE (adv)**|In this position|TO DOWNLOAD THE<br>FILE, CLICK HERE.|
||**hesitation (n) — UNNAPPROVED**|SMOOTHLY (adv)|MAKE SURE THAT THE<br>SOLENOID OPERATES<br>SMOOTHLY.|<br>Make sure that the<br>solenoid operates<br>without hesitation.|
|||CORRECTLY (adv)|THE VALVE MUST<br>OPERATE<br>CORRECTLY.|The valve must operate<br>without hesitation.|
|||IMMEDIATELY (adv)|WHEN YOU OPEN THE<br>CIRCUIT BREAKER,<br>THE LIGHT MUST<br>COME ON<br>IMMEDIATELY.|When you open the<br>circuit breaker, the light<br>must come on without<br>hesitation.|

# Page 262 of 434

**Page 2-1-H4**

**Part 2 - Dictionary**

**Issue 9 2025-01-15**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
||---|---|---|---|
||**HIGH (adj)**<br>**(HIGHER,**<br>**HIGHEST)**|That is of large value|USE THE SPECIAL<br>PROTECTION FOR<br>STORAGE IN HIGH<br>TEMPERATURES.|
||**highly (adv) — UNNAPPROVED**|VERY (adv)|TOLUENE IS VERY<br>FLAMMABLE.|Toluene is highly<br>flammable.|
||**hinder (v) — UNNAPPROVED**|PREVENT (v)|SCRATCHES CAN<br>PREVENT THE FREE<br>MOVEMENT OF THE<br>PISTON IN THE<br>SLEEVE.|Scratches can hinder the<br>movement of the piston<br>in the sleeve.|
|||DECREASE (v)|A CLOGGED DUCT<br>WILL DECREASE<br>AIRFLOW.|A clogged duct will<br>hinder airflow.|
|||BLOCKAGE (n)|MAKE SURE THAT<br>THERE IS NO<br>BLOCKAGE IN THE<br>PIPE THAT PREVENTS<br>AIRFLOW.|Make sure that there is<br>nothing in the pipe to<br>hinder airflow.|
|||CLOGGED (adj)|MAKE SURE THAT THE<br>PIPE IS NOT<br>CLOGGED.|Make sure that there is<br>nothing in the pipe to<br>hinder airflow.|
||**hinge (v) — UNNAPPROVED**|TURN (v)|THE PANELS TURN ON<br>TWO NYLON STRAPS.|Panels hinge on two<br>nylon straps.|
||**HIT (v),**<br>**HITS,**<br>**HIT,**<br>**HIT**|To touch suddenly and<br>with much force|DO NOT HIT THE<br>CARTRIDGE.|
||**hitch (v) — UNNAPPROVED**|CONNECT (v)|CONNECT THE<br>TOWING ARM TO THE<br>NOSEWHEEL.|Hitch the towing arm to<br>the nosewheel.|
||**hoist (v) — UNNAPPROVED**|LIFT (v)|LIFT THE MODULE.|Hoist the module.|
||**hold (n) — UNNAPPROVED**|HOLD (v)|MAKE SURE THAT<br>YOU HOLD THE ROD<br>TIGHTLY.|Make sure that you have<br>a tight hold on the rod.|
||**HOLD (v),**<br>**HOLDS,**<br>**HELD,**<br>**HELD**|1.<br>To continue to have<br>in the hand or grip|HOLD THE ROD<br>TIGHTLY.|
|||2.<br>To continue to have<br>in a specified<br>location, position, or<br>condition|HOLD THE AIRSPEED<br>INDICATION AT THE<br>SAME VALUE FOR<br>2 MINUTES.|

**Issue 9 Part 2 - Dictionary 2025-01-15**

# Page 263 of 434

**Page 2-1-H5**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
||---|---|---|---|
||**hold back (v) — UNNAPPROVED**|PREVENT (v)|AT FULL THRUST, the<br>BRAKES MUST<br>PREVENT MOVEMENT<br>OF THE AIRCRAFT.|At full thrust, the brakes<br>must hold the aircraft<br>back.|
||**hold off (v) — UNNAPPROVED**|PREVENT (v)|THE PROTECTIVE<br>PAINT WILL PREVENT<br>CORROSION FOR SIX<br>MONTHS.|The protective paint will<br>hold off corrosion for six<br>months.|
||**HOLE (n)**|An empty space in a<br>solid object|MAKE SURE THAT THE<br>HOLES IN THE<br>BUSHING ALIGN WITH<br>THOSE IN THE<br>HOUSING.|
||**hook (v) — UNNAPPROVED**|PUT (v)|PUT THE SLING ON<br>THE SHACKLE.|Hook the sling on the<br>shackle.|
||**hook up (v) — UNNAPPROVED**|CONNECT (v)|CONNECT THE<br>TOWING ARM TO THE<br>NOSE GEAR.|Hook the towing arm up<br>to the nose gear.|
||**HORIZONTAL (adj)**|Parallel to the horizon or<br>a baseline|ADJUST THE SLING<br>UNTIL THE FLAP IS<br>HORIZONTAL.|
||**HORIZONTALLY**<br>**(adv)**|In a horizontal position|THE VALVE IS<br>INSTALLED<br>HORIZONTALLY.|
||**HOT (adj)**<br>**(HOTTER,**<br>**HOTTEST)**|At a high temperature|DRY THE SURFACE<br>WITH HOT AIR.|
||**house (v) — UNNAPPROVED**|CONTAIN (v)|THE MODULE<br>CONTAINS FIVE<br>COMPONENTS.|The module houses five<br>components.|
||**HOW (adv)**|By which manner|PARAGRAPH 7.0<br>TELLS YOU HOW TO<br>INSTALL THE UNIT.|
||**however (adv) — UNNAPPROVED**|BUT (conj)|THE DRYING TIME IS<br>USUALLY 24 HOURS.<br>BUT THE PROCEDURE<br>IN THIS STEP WILL<br>DECREASE THE<br>DRYING TIME TO<br>12 HOURS.|The drying time is<br>usually 24 hours.<br>However, the procedure<br>in this step will decrease<br>the drying time to<br>12 hours.|

# Page 264 of 434

**Page 2-1-H6**

**Part 2 - Dictionary**

**Issue 9 2025-01-15**

##### **ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
||---|---|---|---|
||**huge (adj) — UNNAPPROVED**|LARGE (adj)|TO REMOVE THE<br>PAINT STRIPPER,<br>FLUSH THE SURFACE<br>WITH LARGE<br>QUANTITIES OF<br>WATER.|To remove the paint<br>stripper, flush the<br>surface with huge<br>quantities of water.|
||**hum (v) — UNNAPPROVED**|HUM (TN)|ADJUST THE<br>POTENTIOMETER<br>UNTIL YOU DO NOT<br>HEAR A HUM FROM<br>THE LOUDSPEAKER.|Adjust the potentiometer<br>until the loudspeaker no<br>longer hums.|
||**hurt (v) — UNNAPPROVED**|INJURY (n)|BE CAREFUL WHEN<br>YOU DO THIS<br>PROCEDURE. IF THE<br>UNIT FALLS, IT CAN<br>CAUSE INJURY TO<br>PERSONS.|Be careful when you do<br>this procedure. If the unit<br>falls, it can hurt persons.|
||**HYDRAULIC (adj)**|Related to, or operated<br>by, pressurized liquid|CONNECT THE<br>FITTINGS TO THE<br>HYDRAULIC TEST<br>BENCH.|
||**HYDRAULICALLY**<br>**(adv)**|With hydraulic power|MAKE SURE THAT THE<br>LINES ARE<br>HYDRAULICALLY<br>OPERATED.|

**Issue 9 2025-01-15**

**Part 2 - Dictionary**
