# Page 345 of 434

**Page 2-1-R5**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
||---|---|---|---|---|
||**RECYCLE (v),**<br>**RECYCLES,**<br>**RECYCLED,**<br>**RECYCLED**|To put a used material<br>through a process to<br>make it possible to use it<br>or its components again<br>For other<br>meanings, use:|MAKE SURE THAT<br>YOU RECYCLE THE<br>REMOVED<br>INSULATION<br>MATERIAL.|

|||CYCLE (n)|DO ONE MORE TEST<br>CYCLE OF THE<br>COMPONENT.|Recycle the component<br>through a test.
||**reduce (v) — UNNAPPROVED**|DECREASE (v)|SLOWLY DECREASE<br>THE SPEED.|Slowly reduce the<br>speed.
||**REFER (v),**<br>**REFERS,**<br>**REFERRED,**<br>**REFERRED**|1.<br>To tell a person<br>where to find<br>information|REFER TO CHAPTER<br>28 FOR THE<BR>INSTALLATION<br>PROCEDURE.
|||2.<br>To give information|BEFORE YOU DO THIS<br>PROCEDURE,<BR>ENGAGE THE RAMP<BR>SERVICE DOOR<BR>SAFETY CONNECTOR<BR>PIN (THE PIN THAT:<br>HOLDS THE RAMP<br>SERVICE DOOR,<br>REFER TO IN THIS<br>PROCEDURE AS THE<br>“SAFETY CONNECTOR<br>PIN”).
||**reference (n) — UNNAPPROVED**|REFER (v)|REFER TO<br>CHAPTER 20 FOR THE<br>STANDARD TORQUE<br>VALUES.|Reference is made to<br>Chapter 20 for the<br>standard torque values.
||**referenced (adj) — UNNAPPROVED**|SHOW (v)|MAKE SURE THAT THE<br>GRAPH SHOWS THIS<br>POINT.
|Make sure that this point<br>is referenced on the<br>graph.
||**refill (v) — UNNAPPROVED**|FILL (v)|FILL THE CONTAINER<br>AGAIN.|Refill the container.
||**refit (v) — UNNAPPROVED**|INSTALL (v)|INSTALL THE LINKAGE<br>AGAIN.|Refit the linkage.
||REPAIR (v)|ON THE SUBMARINE,<br>REPAIR ALL DAMAGE<br>AND REPLACE ALL<br>WORN PARTS.|Refit the submarine.

# Page 346 of 434

**Page 2-1-R6**

**Part 2 - Dictionary**

**Issue 9 2025-01-15**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
||---|---|---|---|---|

||**reflect (v) — UNNAPPROVED**|REFLECTION (n)|THE RETICLE IMAGE<br>MAKES A REFLECTION<br>ON THE BOTTOM<br>SURFACE OF THE<br>GLASS.|The reticle image<br>reflects on the bottom<br>surface of the glass.

||**REFLECTION (n)**|Something that occurs<br>when energy comes<br>against a surface which<br>sends it back|A CLEAN SURFACE<br>GIVES A BETTER<BR>REFLECTION.|
||**REFUEL (v),**<br>**REFUELS,**<br>**REFUELED,**<br>**REFUELED**|To supply with fuel|REFUEL THE VEHICLE.|

||**register (v) — UNNAPPROVED**|SHOW (v)|ADJUST THE “SET +40”<br>CONTROL UNTIL THE<br>POINTER SHOWS +40.|Adjust the “SET +40”<br>control until the pointer<br>registers +40.
||**regrease (v) — UNNAPPROVED**|APPLY (v)|APPLY GREASE TO<br>THE ROD AGAIN.|Regrease the rod.
||MORE (adj)|PUT MORE GREASE<br>ON THE JOINT UNTIL<br>YOU CAN MOVE IT.|Regrease the joint until<br>you can move it.

||**REGULAR (adj)**|At specified or equal<br>intervals|THE COMPUTER<br>GIVES REGULAR<br>INPUTS TO THE<br>CONTROL SYSTEM.|
||**REGULARLY (adv)**|In a regular manner|IF THE FAILURE<br>OCCURS REGULARLY,<br>DO A SYSTEM TEST.|

||**regulate (v) — UNNAPPROVED**|CONTROL (v)|CONTROL THE<br>ELECTRICAL<br>CURRENT.|Regulate the electrical<br>current.
||ADJUST (v)|ADJUST THE TIRE<br>PRESSURE AS<br>NECESSARY.|Regulate the tire<br>pressure as necessary.

**Issue 9 2025-01-15**

**Part 2 - Dictionary**

# Page 347 of 434

**Page 2-1-R7**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
||---|---|---|---|---|

||**regulation (n) — UNNAPPROVED**|ADJUSTMENT (n)|THE TEMPERATURE<br>ADJUSTMENT IS<br>AUTOMATIC.|The regulation of<br>temperature is<br>automatic.
||CONTROL (n)|THE TEMPERATURE<br>CONTROL IS<br>AUTOMATIC.|The regulation of<br>temperature is<br>automatic.
||CONTROL (v)|A SENSOR CONTROLS<br>THE TEMPERATURE IN<br>THE COMPARTMENT.
|The regulation of<br>temperature in the<br>compartment is effected<br>by a sensor.
||**reinflate (v) — UNNAPPROVED**|INFLATE (v)|INFLATE THE TIRE<br>AGAIN.|Reinflate the tire.
||**reinforce (v) — UNNAPPROVED**|MAKE … STRONGER|DOUBLERS MAKE THE<br>JOINT STRONGER.|Doublers reinforce the<br>joint.
||**reinstall (v) — UNNAPPROVED**|INSTALL (v)|AFTER YOU ADJUST<br>THE UNIT, INSTALL<br>THE COVER AGAIN.|Reinstall the cover after<br>you adjust the unit.
||**reinstallation (n) — UNNAPPROVED**|INSTALLATION (n)|ONLY APPROVED<br>PERSONNEL Can DO<br>THE INSTALLATION<br>PROCEDURE.|This reinstallation must<br>be performed by<br>qualified personnel.

||**REJECT (v),**<br>**REJECTS,**<br>**REJECTED,**<br>**REJECTED**|To make a decision that<br>something is<br>unsatisfactory|REJECT THE PARTS<br>THAT ARE DAMAGED.|

||**rejection (n) — UNNAPPROVED**|REJECT (v)|IF THE TEST IS NOT<br>SATISFACTORY,<br>REJECT THE<br>COMPONENT.|Rejection is mandatory if<br>the test proves the<br>component to be<br>defective.
||**relate (v) — UNNAPPROVED**|RELATED (adj)|THE PROCEDURES<br>ARE RELATED TO THE<br>SYSTEM TEST.|The procedures relate to<br>the system test.

||**RELATED (adj)**|That has a relation|CLEAN THE BALLS OF<br>THE ELECTRICAL<br>LATCH AND ITS<br>RELATED SOCKETS.|
||**RELATION (n)**|The connection between<br>two or more things<br>caused by their<br>functions, values, or<br>conditions|THE RELATION<br>BETWEEN THE TWO<br>CONTROL SYSTEMS<br>KEEPS THE AIRCRAFT<br>STABLE.|

# Page 348 of 434

**Page 2-1-R8**

**Part 2 - Dictionary**

**Issue 9 2025-01-15**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
||---|---|---|---|---|

||**relay (v) — UNNAPPROVED**|SEND (v)|SEND THE<br>INFORMATION TO THE<br>ENGINEERING<br>DEPARTMENT.|Relay the information to<br>the engineering<br>department.

||**RELEASE (v),**<br>**RELEASES,**<br>**RELEASED,**<br>**RELEASED**|To make free, to let go|RELEASE THE<br>INSTRUMENT PANEL<br>TO GET ACCESS TO<br>THE CONNECTIONS.|

||**relevant (adj) — UNNAPPROVED**|RELATED (adj)|REMOVE THE ROD<br>END FROM THE<br>RELATED PIVOT.|Withdraw the rod end<br>from the relevant pivot.
||THEIR (adj)|INSTALL THE BOLTS<br>IN THEIR HOLES.|Install the bolts in the<br>relevant holes.
||ITS (adj)|INSTALL THE<br>COMPUTER IN ITS<br>RACK.|Install the computer in<br>the relevant rack.
||**relieve (v) — UNNAPPROVED**|RELEASE (v)|RELEASE THE<br>TENSION IN THE<br>CABLE.|Relieve the tension in<br>the cable.
||**remain (v) — UNNAPPROVED**|STAY (v)|THE FLAGS MUST<br>STAY OUT OF VIEW.|The flags must remain<br>out of view.

||**REMAINING (adj)**|That continues to stay|REMOVE THE<br>REMAINING SEALANT<br>WITH SOLVENT.|

||**remnant (n) — UNNAPPROVED**|REMAINING (adj)|REMOVE THE<br>REMAINING SEALANT<br>FROM THE FLOOR<br>COVERING.|Remove sealant<br>remnants from the floor<br>covering.
||**removable (adj) — UNNAPPROVED**|REMOVE (v)|FIND THE PART OF<br>THE BARREL THAT<br>YOU CAN REMOVE.|Find the removable part<br>of the barrel.

||**REMOVAL (n)**|A procedure which<br>removes an object|THE SUPERVISOR<br>MUST GIVE THE<br>APPLICABLE<br>PROCEDURE FOR<br>CORROSION<br>REMOVAL.|
||**REMOVE (v),**<br>**REMOVES,**<br>**REMOVED,**<br>**REMOVED**|To take or move<br>something away from its<br>initial position|REMOVE THE<br>INDICATOR FROM THE<br>PANEL.|

||**render (v) — UNNAPPROVED**|MAKE (v)|MAKE THE SYSTEM<br>ELECTRICALLY SAFE.|Render the system<br>electrically safe.

**Issue 9 Part 2 - Dictionary 2025-01-15**
