<!-- section: DICT_Q-Z | pages: 325-328 | verified: true -->

# Page 325 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **OUTBOARD (adj)** | Farther from the MEASURE THE longitudinal axis of MOVEMENT OF THE something INBOARD AND OUTBOARD FLAPS. |
| **OUTBOARD (adv)** | In, or to, a position MOVE THE JACK farther from the OUTBOARD TO longitudinal axis of DISENGAGE IT FROM something THE JACKING POINT. OUTBOARD OF At a position farther from PUT THE ACCESS (prep) the longitudinal axis PLATFORM IN A POSITION THAT IS OUTBOARD OF THE FLAP TRACK. |
| **OUTDOORS (adv)** | Not in a building DO THIS WORK OUTDOORS. |
| **OUTER (adj)** | Located on the outside APPLY SEALANT ON or farther from the center THE OUTER SURFACE. of an object |
| **outline (v) — UNNAPROVED** | GIVE (v) THIS SECTION GIVES This section outlines the YOU THE procedures needed to PROCEDURES THAT find the faults. ARE NECESSARY TO FIND THE FAULTS. |
| **OUTPUT (n)** | The data, power, energy THE IMPEDANCE that comes out of MATCHING equipment or a system TRANSFORMERS SUPPLY 60 W OUTPUT TO THE LOUDSPEAKERS. |
| **outside (adj) — UNNAPROVED** | EXTERNAL (adj) THE EXTERNAL The outside temperature TEMPERATURE IS is indicated on the SHOWN ON THE central display unit. CENTRAL DISPLAY UNIT. |
| **OUTER (adj)** | CLEAN THE OUTER Clean the outside SURFACE WITH WARM surface with warm water. WATER. |

# Page 326 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **outside (adv) — UNNAPROVED** | OUTDOORS (adv) DO THIS PROCEDURE Do this procedure OUTDOORS. outside. |
| **outside (n) — UNNAPROVED** | EXTERNAL (adj) FOLD THE EDGING Fold the edging against AGAINST THE the outside of the EXTERNAL SIDE OF insulation blankets. THE INSULATION BLANKET. |
| **OUTER (adj)** | FOLD THE EDGING Fold the edging against AGAINST THE OUTER the outside of the SIDE OF THE insulation blankets. INSULATION BLANKET. |
| **outside (prep) — UNNAPROVED** | NEAR (prep) WHEN YOU DO WORK When you do work in a IN A FUEL TANK, A fuel tank, a second SECOND PERSON person must be outside MUST BE NEAR THE the tank at all times. TANK AT ALL TIMES. |
| **outwards (adv) — UNNAPROVED** | OUT (adv) MOVE THE DOOR OUT Move the door outwards AND FORWARD. and forwards. |
| **over (prep) — UNNAPROVED** | ABOVE (prep) MAKE SURE THAT THE Make sure the hydraulic HYDRAULIC FLUID fluid level is not over the LEVEL IS NOT ABOVE FULL mark. THE "FULL" MARK. |
| **ALONG (prep)** | APPLY THE WEIGHT The weight must be EQUALLY ALONG THE evenly spread over the STABILIZER SPAN. stabilizer span. |
| **ON (prep)** | INSTALL THE STOP Install the stop sleeve SLEEVE ON THE over the sliding member. SLIDING MEMBER. MORE THAN DO NOT INSTALL Do not install shims over SHIMS WITH A 0.1 mm thick. THICKNESS OF MORE THAN 0.1 mm. For movement BEFORE OVER- above land or WATER OPERATION water, use a AT LOW ALTITUDES, technical noun. APPLY CORROSION- PREVENTIVE FLUID TO THE DOOR HINGES OF THE LANDING GEAR. |

# Page 327 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example
OVERBOARD Out of a vessel RELEASE THE AIR
(adv) OVERBOARD.

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **overfill (v) — UNNAPROVED** | TOO MUCH DO NOT PUT TOO Do not overfill the MUCH FLUID IN THE lubrication hole. LUBRICATION HOLE. |
| **overfull (adj) — UNNAPROVED** | TOO FULL IF THE TANK IS TOO If the tank is overfull, you FULL, YOU CANNOT cannot pressurize it PRESSURIZE IT correctly. CORRECTLY. |
| **overhaul (v) — UNNAPROVED** | OVERHAUL (TN) DO AN OVERHAUL OF Overhaul the No. 2 THE No. 2 ENGINE. engine. |
| **overheat (v) — UNNAPROVED** | TOO HOT IF YOU PRESSURIZE Rapid charging THE OXYGEN BOTTLE overheats the oxygen QUICKLY, IT WILL bottle. BECOME TOO HOT. |
| **OVERLAP (n)** | The area in which a part IF THE OVERLAP IS of one surface is on a MORE THAN 0,01 mm, part of a second surface REPLACE THE PART. |
| **overlap (v) — UNNAPROVED** | OVERLAP (n) MAKE AN OVERLAP Overlap the surfaces by OF 10 mm. 10 mm. |
| **OVERRIDE (v)** | , To prevent the automatic MANUALLY OVERRIDE OVERRIDES, operation of a part or THE START OVERRODE, system SEQUENCE. OVERRIDDEN |
| **overtighten (v) — UNNAPROVED** | TIGHTEN TOO MUCH DO NOT TIGHTEN THE Do not overtighten the FITTINGS TOO MUCH. fittings. TOO TIGHT DO NOT MAKE THE Do not overtighten the FITTINGS TOO TIGHT. fittings. TOO TIGHTLY DO NOT INSTALL THE Do not overtighten the FITTINGS TOO fittings. TIGHTLY. |

# Page 328 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example
Blank Page
Page 2-1-O10 Part 2 - Dictionary Issue 9
2025-01-15
