# Page 269–272 of 434

> **Source:** ASD-STE100 Issue 9, January 2025
> **Pages:** 269–272 of 434

# Page 269 of 434

| Word (POS) | Approved meaning / ALTERNATIVES | STE example | Non-STE example |
|------------|--------------------------------|-------------|-----------------|
| impossible (adj) — UNNAPPROVED | NOT POSSIBLE | THUS, IT IS NOT POSSIBLE TO GIVE A STANDARD VALUE. | Thus, it is impossible to give a standard value. |
| impossible (adj) — UNNAPPROVED | CANNOT (v) | YOU CANNOT FILL THE CONTAINERS WHILE THEY ARE INSTALLED ON THE AIRCRAFT. | It is impossible to recharge containers while installed on aircraft. |
| impregnate (v) — UNNAPPROVED | SOAK (v) | SOAK THE FILTER ELEMENTS IN OIL. | The filter elements must be impregnated with oil. |
| impression (n) — UNNAPPROVED | THINK (v) | IF YOU THINK THAT A TIRE HAS LOW PRESSURE, DO THE STEPS THAT FOLLOW: | If you have the impression that a tire has low pressure, do the steps that follow: |
| improper (adj) — UNNAPPROVED | INCORRECT (adj) | INCORRECT ADJUSTMENT OF THE STOP BOLTS ON THE RUDDER PEDALS CAN CAUSE DAMAGE. | Improper adjustment of the stop bolts on the rudder pedals can cause damage. |
| improperly (adv) — UNNAPPROVED | INCORRECTLY (adv) | IF THE HINGE IS INCORRECTLY ADJUSTED, YOU CANNOT CLOSE THE PANEL. | If the hinge is improperly adjusted, the panel will not close. |
| improve (v) — UNNAPPROVED | BETTER (adj) | DO NOT ADJUST THE PARTS AGAIN TO MAKE THEIR POSITION BETTER. | Do not readjust the parts to improve their position. |
| impurity (n) — UNNAPPROVED | UNWANTED MATERIAL | USE A FILTER TO REMOVE UNWANTED MATERIAL FROM THE HYDRAULIC OIL. | Filter the hydraulic oil to remove impurities. |
| impurity (n) — UNNAPPROVED | CONTAMINATION (n) | CONTAMINATION CAN CAUSE A FAILURE. | Impurities may cause a failure. |
| IN (adv) | To, or into a location or position | MAKE SURE THAT THE SWITCHES ARE PUSHED IN. | |

# Page 270 of 434

| Word (POS) | Approved meaning / ALTERNATIVES | STE example | Non-STE example |
|------------|--------------------------------|-------------|-----------------|
| IN (prep) | Function word that shows location, position, condition, time, or limits | LET THE SWITCH STAY IN THE SET POSITION. | |
| IN (prep) | | THE COMPENSATORS ARE IN THE WING BAY. | |
| IN (prep) | | DO NOT PARK THE VEHICLE IN STRONG WINDS. | |
| IN (prep) | | MAKE SURE THAT THE LIGHT COMES ON IN 5 SECONDS. | |
| IN (prep) | | MAKE SURE THAT THE CRACKS ARE IN THE LIMITS. | |
| IN FRONT OF (prep) | In a position ahead of | PUT CHOCKS IN FRONT OF THE WHEELS. | |
| IN PROGRESS (adv) | Occurring | IF AN INTERACTIVE SESSION IS IN PROGRESS, LET IT CONTINUE UNTIL IT IS FULLY COMPLETED. | |
| inactive (adj) — UNNAPPROVED | NOT ACTIVE | THE AUTOTHRUST SYSTEM IS ENGAGED BUT IT IS NOT ACTIVE. | The autothrust system is engaged but inactive. |
| inadvertent (adj) — UNNAPPROVED | ACCIDENTAL (adj) | ACCIDENTAL OPERATION OF THE SYSTEM CAN KILL YOU. | Inadvertent operation of the system could cause fatal injuries. |

# Page 271 of 434

| Word (POS) | Approved meaning / ALTERNATIVES | STE example | Non-STE example |
|------------|--------------------------------|-------------|-----------------|
| inadvertently (adv) — UNNAPPROVED | ACCIDENTALLY (adv) | IF YOU ACCIDENTALLY PUT TOO MUCH FUEL IN THE TANK, OPEN THE DRAIN VALVE. | If the tank is inadvertently overfilled, open the drain valve. |
| INBOARD (adj) | Nearer to the longitudinal axis | REMOVE THE INBOARD FAIRING OF THE FLAP HINGE. | |
| INBOARD (adv) | In or to a position nearer to the longitudinal axis | THE LANDING GEAR RETRACTS INBOARD INTO THE BAY. | |
| INBOARD OF (prep) | At a position nearer to the longitudinal axis | PUT THE ACCESS PLATFORM IN POSITION BELOW THE ACCESS PANEL THAT IS INBOARD OF THE FLAP TRACK. | |
| INCIDENT (n) | An important occurrence that can cause damage or have dangerous results | RECORD ALL INCIDENTS OF WATER FOUND IN THE FUEL. | |
| incline (n) — UNNAPPROVED | SLOPE (n) | YOU CAN ADJUST THE SLOPE OF THE RAMP. | You can adjust the incline of the ramp. |
| INCLUDE (v), INCLUDES, INCLUDED, INCLUDED | To make, or to be, part of | THIS CHAPTER INCLUDES THE PROCEDURES FOR THE REMOVAL OF THE COMPONENTS. | |
| including (prep) — UNNAPPROVED | THRU (prep) | DO TESTS 4 THRU 8 AGAIN. | Repeat from test 4 up to and including test 8. |
| including (prep) — UNNAPPROVED | WITH (prep) | SEND THE DEFECTIVE COVER, WITH THE OIL SAMPLES, TO THE REPAIR CENTER. | Return the defective cover, including the oil samples, to the repair center. |
| incompatible (adj) — UNNAPPROVED | NOT COMPATIBLE | THIS SOFTWARE IS NOT COMPATIBLE WITH OTHER OPERATING SYSTEMS. | This software is incompatible with other operating systems. |
| incompatible (adj) — UNNAPPROVED | | THIS COOLANT IS NOT COMPATIBLE WITH ALUMINUM ALLOYS. | This coolant is incompatible with aluminum alloys. |

# Page 272 of 434

| Word (POS) | Approved meaning / ALTERNATIVES | STE example | Non-STE example |
|------------|--------------------------------|-------------|-----------------|
| incomplete (adj) — UNNAPPROVED | NOT FULL | IF THE ACTUATOR TRAVEL IS NOT FULL, ADJUST THE RODS AGAIN. | If the actuator travel is incomplete, readjust the rods. |
| incomplete (adj) — UNNAPPROVED | NOT COMPLETED | IF THE ADJUSTMENT IS NOT COMPLETED, THE VALUES SHOWN ON THE INDICATOR WILL BE INCORRECT. | If the adjustment is incomplete, the values shown on the indicator will be incorrect. |
| incomplete (adj) — UNNAPPROVED | ALL (adj) | IF YOU DO NOT HAVE ALL THE RESULTS, DO THE TEST AGAIN. | If the results are incomplete, do the test again. |
| incorporate (v) — UNNAPPROVED | INCLUDE (v) | ALL MODELS INCLUDE A MICROPROCESSOR CONTROL UNIT. | All models incorporate a microprocessor control unit. |
| incorporate (v) — UNNAPPROVED | HAVE (v) | SOME RELAYS HAVE A POTENTIOMETER. | Some relays incorporate a potentiometer. |
| incorporation (n) — UNNAPPROVED | INCLUDE (v) | THE MANUFACTURER INCLUDED A SECOND DIODE TO INCREASE THE RELIABILITY OF THE MOTOR. | Incorporation of a second diode increased the reliability of the motor. |
| INCORRECT (adj) | Not correct | IF THE TRIM TAB ADJUSTMENT IS INCORRECT, DO STEPS 7 THRU 10. | |
| INCORRECTLY (adv) | In an incorrect manner | IF YOU SEE THE RED MARK, THE PART IS INSTALLED INCORRECTLY. | |
