<!-- section: DICT_A-F | pages: 169-172 | verified: true -->

# Page 169 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **associated (adj) — UNNAPROVED** | CORRECT (adj) INSTALL THE DUMP Install the dump valve VALVE AND THE with the associated CORRECT GASKET. gasket. |
| **RELATED (adj)** | REMOVE THE PANELS Remove the panels from FROM THE RELATED the associated doors. DOORS. |
| **ITS (adj)** | REMOVE THE BOLT Remove the bolt and the AND ITS WASHER. associated washer. |
| **THEIR (adj)** | REMOVE THE EIGHT Remove the eight bolts BOLTS AND THEIR and the associated WASHERS. washers. |
| **assume (v) — UNNAPROVED** | THINK (v) IF YOU THINK THAT If damage is assumed to YOU CAN REPAIR THE be repairable, refer to DAMAGE, REFER TO the repair section. THE REPAIR SECTION. |
| **assure (v) — UNNAPROVED** | MAKE SURE (v) USE A PLUMB LINE TO Use a plumb line to MAKE SURE THAT THE assure that the wall is WALL IS VERTICAL. vertical. |
| **as to (prep) — UNNAPROVED** | ABOUT (prep) REFER TO TABLE 7001 Refer to Table 7001 for FOR INFORMATION information as to the ABOUT HOW THE construction of the pivot PIVOT ASSEMBLY IS assembly. MADE. |
| **asymmetric (adj) — UNNAPROVED** | NOT SYMMETRICAL IF THE RESULT THAT If you get an asymmetric YOU GET IS NOT result, do a rigging test. SYMMETRICAL, DO A RIGGING TEST. |
| **AT (prep)** | Function word that DISCONNECT THE shows the location, HOSE AT THE PITOT position, direction, or HEAD. time that something occurs AT APPROXIMATELY 300 KNOTS, THE LIGHT COMES ON. WITH THE NOSEWHEEL AT 30 DEG. TO THE CENTER LINE, SET THE LEVER TO "UP." |

# Page 170 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

| ATTACH (v), |
| --- |
| ATTACHES, |
| ATTACHED, |
| ATTACHED |

### THERE ARE NO

### BUBBLES.

### TEMPORARILY

### ATTACH THE CABLE

### TO THE ADJACENT

### STRUCTURE.

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **attachment (n) — UNNAPROVED** | ATTACH (v) MAKE SURE THAT THE Make sure that the DUCT IS CORRECTLY attachment of the duct to ATTACHED TO THE the filter is correct. FILTER. |
| **attain (v) — UNNAPROVED** | SHOW (v) WHEN THE When 28 volts DC is VOLTMETER SHOWS attained, the relay 28 VOLTS DC, THE closes. RELAY CLOSES. |
| **BE (v)** | WHEN THE VOLTAGE When 28 volts DC is IS 28 VOLTS DC, THE attained, the relay RELAY CLOSES. closes. |
| **GET (v)** | WHEN YOU GET When 28 volts DC is 28 VOLTS DC, THE attained, the relay RELAY CLOSES. closes. |
| **attempt (n) — UNNAPROVED** | TRY (v) TRY TO LIFT THE Make an attempt to lift COVER MANUALLY. the cover manually. |
| **attempt (v) — UNNAPROVED** | TRY (v) TRY TO FIND THE Attempt to find the DEFECT. defect. |
| **attention (n) — UNNAPROVED** | AID (n) IF YOU GET PAINT If you get paint spray in SPRAY IN YOUR EYES, your eyes, get medical GET MEDICAL AID. attention. |
| **CAREFUL (adj)** | BE CAREFUL WHEN Pay attention when you YOU REMOVE THE remove the control unit. CONTROL UNIT. |
| **MONITOR (v)** | MONITOR THE Pay attention to the RESULTS. results. |

# Page 171 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **audible (adj) — UNNAPROVED** | HEAR (v) IF YOU CANNOT HEAR If the alarm is not THE ALARM, ADJUST audible, adjust the THE VOLUME volume control. CONTROL. |
| **LISTEN (v)** | LISTEN FOR AIR Check the lines for LEAKAGE FROM THE audible air leakage. LINES. |
| **augment (v) — UNNAPROVED** | INCREASE (v) A MIXTURE OF WATER A mixture of water and AND METHANOL methanol augments the INCREASES THE power of the engine. POWER OF THE ENGINE. |
| **aurally (adv) — UNNAPROVED** | LISTEN (v) LISTEN TO MAKE Check aurally to ensure SURE THAT THE FLUID fluid flow. FLOWS. |
| **HEAR (v)** | YOU CAN HEAR THE The warning is given WARNING IN THE aurally in the cockpit. COCKPIT. |
| **authentic (adj) — UNNAPROVED** | ACCURATE (adj) IF THE ADJUSTMENT If the adjustment of the OF THE STOPS IS NOT stops is not correct, the CORRECT, THE results of the test will not RESULTS OF THE be authentic. TEST WILL NOT BE ACCURATE. |
| **AUTHORITY (n)** | An official organization BEFORE YOU CHANGE that gives approval to THE PROCEDURE, something GET THE APPROVAL OF THE DESIGN AUTHORITY. |
| **authorized (adj) — UNNAPROVED** | APPROVED (adj) ONLY APPROVED Only authorized persons PERSONS ARE are permitted to stay in PERMITTED TO STAY this area. IN THIS AREA. |
| **AUTOMATIC (adj)** | That operates without THE AUTOMATIC other input SYSTEM WILL OPEN THE DOORS. AUTOMATICALLY That operates without THE FUEL FLOW (adv) other input STOPS AUTOMATICALLY. |

# Page 172 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **AUXILIARY (adj)** | 1. That operates in a LUBRICANTS FOR THE secondary function ENGINE AND THE AUXILIARY EQUIPMENT ARE THE SAME. 2. That gives help USE AUXILIARY SCREWS TO ASSEMBLE THE UNIT TEMPORARILY. |
| **AVAILABLE (adj)** | Prepared or supplied for IF ELECTRICAL you to use POWER IS AVAILABLE, DO A CONTINUITY CHECK. |
| **avert (v) — UNNAPROVED** | PREVENT (v) IF THE MICROSWITCH If the microswitch BECOMES becomes unserviceable, UNSERVICEABLE, deactivate the actuator DEACTIVATE THE to avert damage to the ACTUATOR TO valve. PREVENT DAMAGE TO THE VALVE. |
| **avoid (v) — UNNAPROVED** | PREVENT (v) TURN THE CONTROLS Turn the controls slowly SLOWLY TO PREVENT to avoid damage. DAMAGE. DO NOT DO NOT PUSH ON THE Avoid pushing on the SEALS. seals. |
| **aware (adj) — UNNAPROVED** | KNOW (v) ALL PERSONNEL All personnel must be MUST KNOW THE aware of the health risks. HEALTH RISKS. |
| **TELL (v)** | TELL ALL PERSONNEL All personnel must be ABOUT THE NEW aware of the new rules. RULES. AWAY FROM In or to a different DO THE WORK IN AN (prep) position or direction AREA AWAY FROM EQUIPMENT OR METAL FRAME BUILDINGS. |
| **AXIAL (adj)** | Related to an axis DO STEPS 1 THRU 4 TO MAKE SURE THAT NO AXIAL LOAD IS ON THE ROD. |
| **AXIALLY (adv)** | Related to an axis APPLY THE LOAD AXIALLY. |
