# Page 273–276 of 434

> **Source:** ASD-STE100 Issue 9, January 2025
> **Pages:** 273–276 of 434

# Page 273 of 434

| Word (POS) | Approved meaning / ALTERNATIVES | STE example | Non-STE example |
|------------|--------------------------------|-------------|-----------------|
| increase (n) — UNAPPROVED | INCREASE (v) | THE TEMPERATURE MUST INCREASE. | There must be an increase in temperature. |
| INCREASE (v), INCREASES, INCREASED, INCREASED | To make or become larger or higher in value | INCREASE THE VANE ANGLE TO 90 DEGREES. MAKE SURE THAT THE TEMPERATURE INCREASES TO 30 °C. | |
| INCREMENT (n) | One of a sequence of regular operations done one after the other, to increase or decrease an adjustable quantity | ADJUST THE STOP BOLT IN INCREMENTS OF 5 mm. | |
| incur (v) — UNAPPROVED | CAUSE (v) | REMOVAL OF THE UNIT BEFORE 24 HOURS CAN CAUSE DAMAGE. | Removal of the unit before 24 hours can incur damage. |
| independent (adj) — UNAPPROVED | INDEPENDENTLY (adv) | THIS UNIT OPERATES INDEPENDENTLY. | The operation of this unit is independent. |
| INDEPENDENTLY (adv) | Without a relation with | THE EMERGENCY SYSTEM IS CONTROLLED INDEPENDENTLY. | |
| indicate (v) — UNAPPROVED | SHOW (v) | THE POINTER SHOWS ZERO FEET. | The pointer indicates zero feet. |
| indicate (v) — UNAPPROVED | IDENTIFY (v) | A 406 MHz DIGITAL SIGNAL IDENTIFIES THE EMERGENCY LOCATOR TRANSMITTER AND ITS LOCATION. | A 406 MHz digital signal indicates the emergency locator transmitter and its location. |
| indicate (v) — UNAPPROVED | SPECIFIED (adj) | IF TOLERANCES ARE NOT SPECIFIED, REFER TO GENERAL TOLERANCE VALUES. | If tolerances are not indicated, refer to general tolerance values. |
| INDICATION (n) | Something that is shown | MAKE SURE THAT THE INDICATION IS CORRECT. | |
| induce (v) — UNAPPROVED | CAUSE (v) | SCRATCHES IN THE WINDSCREEN CAN CAUSE CRACKS. | Scratches in the windscren may induce cracks. |

# Page 274 of 434

| Word (POS) | Approved meaning / ALTERNATIVES | STE example | Non-STE example |
|------------|--------------------------------|-------------|-----------------|
| ineffective (adj) — UNAPPROVED | UNSERVICEABLE (adj) | IF THE PUMP IS UNSERVICEABLE, REPLACE IT. | If the pump is ineffective, replace it. |
| ineffective (adj) — UNAPPROVED | UNSATISFACTORY (adj) | IF THE OPERATION OF THE PUMP IS UNSATISFACTORY, REPLACE IT. | If the operation of the pump is ineffective, replace it. |
| ineffective (adj) — UNAPPROVED | NOT OPERATE | IF THE PUMP DOES NOT OPERATE CORRECTLY, REPLACE IT. | If the pump is ineffective, replace it. |
| inflammable (adj) — UNAPPROVED | FLAMMABLE (adj) | SOLVENT IS VERY FLAMMABLE. | Solvent is highly inflammable. |
| INFLATE (v), INFLATES, INFLATED, INFLATED | To make or become larger as a result of pressurization by a gas | INFLATE THE TIRES WITH NITROGEN. OPERATION OF THE HANDLE RELEASES THE GAS, AND THE SLIDE-RAFT INFLATES. | |
| inform (v) — UNAPPROVED | TELL (v) | TELL THE MANUFACTURER ABOUT THE PROBLEM. | Inform the manufacturer about the problem. |
| INFORMATION (n) | Data collected and made available for a specified function | THIS MANUAL CONTAINS INFORMATION ABOUT MAINTENANCE PROCEDURES. | |
| ingest (v) — UNAPPROVED | SWALLOW (v) | IF YOU SWALLOW HYDRAULIC FLUID, GET MEDICAL AID IMMEDIATELY. | If you ingest hydraulic fluid, get medical aid immediately. |
| ingress (n) — UNAPPROVED | GO INTO | IF WATER GOES INTO THE COMPONENT, DAMAGE WILL OCCUR. | Water ingress will damage the component. |

# Page 275 of 434

| Word (POS) | Approved meaning / ALTERNATIVES | STE example | Non-STE example |
|------------|--------------------------------|-------------|-----------------|
| inhale (v) — UNAPPROVED | BREATHE (v) | DO NOT BREATHE THE SOLVENT FUMES. | Do not inhale the solvent fumes. |
| inhibit (v) — UNAPPROVED | PREVENT (v) | ALODINE PREVENTS CORROSION. | Alodine inhibits corrosion. |
| INITIAL (adj) | That is related to the start | MOVE THE LEVER BACK TO ITS INITIAL POSITION. | |
| INITIALLY (adv) | At the start | INITIALLY, THE SPEED INCREASES TO 3000 RPM. | |
| initiate (v) — UNAPPROVED | START (v) | START THE TEST AT 2000 RPM. | Initiate the test at 2000 rpm. |
| inject (v) — UNAPPROVED | PUT (v) | PUT OIL INTO THE GEARBOX WITH A SYRINGE. | Inject oil into the gearbox with a syringe. |
| injection (n) — UNAPPROVED | PUT (v) | PUT THE CORROSION PREVENTIVE OIL INTO THE PUMP WITH A SYRINGE. | The injection of the corrosion preventive oil into the pump must be done with a syringe. |
| injure (v) — UNAPPROVED | INJURY (n) | MAKE SURE THAT THE END OF THE SAFETY WIRE WILL NOT CAUSE INJURY TO PERSONS. | Make sure that the end of the safety wire will not injure persons. |
| INJURY (n) | Damage to a person | BEND THE ENDS OF THE LOCKING WIRE TO PREVENT INJURY. | |
| INNER (adj) | Nearer to the center of an object | THE INNER SURFACE OF THE PART IS BLACK. | |
| inoperative (adj) — UNAPPROVED | OFF (adj) | BEFORE YOU DRAIN THE FUEL, MAKE SURE THAT THE SYSTEM IS OFF. | Before you drain the fuel, make sure that the system is inoperative. |
| inoperative (adj) — UNAPPROVED | NOT OPERATE | MAKE SURE THAT THE DEMISTING SYSTEM DOES NOT OPERATE. | Make sure that the demisting system is inoperative. |
| INPUT (n) | The data, power, or energy put into equipment or a system | THE UNIT COMPARES THE INPUTS FROM THE TWO SENSORS TO THE COMPUTER. | |

# Page 276 of 434

| Word (POS) | Approved meaning / ALTERNATIVES | STE example | Non-STE example |
|------------|--------------------------------|-------------|-----------------|
| insert (v) — UNAPPROVED | PUT (v) | PUT THE SLEEVE INTO THE OPENING. | Insert the sleeve into the opening. |
| insert (v) — UNAPPROVED | ENGAGE (v) | MAKE SURE THAT THE SHAFT ENGAGES IN THE MATING PART. | Check that the shaft is inserted in the mating part. |
| inside (adj) — UNAPPROVED | INNER (adj) | CLEAN THE INNER SURFACE OF THE CONTAINER. | Clean the inside surface of the container. |
| inside (n) — UNAPPROVED | INNER (adj) | PAINT THE INNER SURFACE OF THE PUMP ASSEMBLY. | Paint the inside surface of the pump assembly. |
| inside (prep) — UNAPPROVED | IN (prep) | THERE MUST BE LUBRICANT IN THE HOLE. | There must be lubricant inside the hole. |
| inside (prep) — UNAPPROVED | INTO (prep) | BEFORE YOU PUT THE TOOLS INTO THE STORAGE BOX, MAKE SURE THAT THEY HAVE THE NECESSARY PROTECTIVE COVERS. | Before you place the tools inside the storage box, make sure they have suitable protective covers. |
| inspect (v) — UNAPPROVED | EXAMINE (v) | EXAMINE ALL THE DRAIN HOLES. | Inspect all the drain holes. |
| inspect (v) — UNAPPROVED | INSPECTION (n) | DO AN INSPECTION OF THE WORK. | Inspect the work. |
| INSPECTION (n) | The procedure which compares an object with its standard or specification | USE A VOLTMETER TO DO THIS INSPECTION. | |
| INSTALL (v), INSTALLS, INSTALLED, INSTALLED | To attach an item in or to a second item | INSTALL THE NEW O-RINGS ON THE SPINDLE. | |
| INSTALLATION (n) | The procedure which installs an item | REFER TO PARAGRAPH 3 FOR THE INSTALLATION OF THE UNIT. | |
| instead (adv) — UNAPPROVED | ALTERNATIVE (n) | USE A SPATULA AS AN ALTERNATIVE. | Use a spatula instead. |
