# Page 253 of 434

**Page 2-1-G3**

**Page 2-1-G3**

**Issue 9 2025-01-15**

**Part 2 - Dictionary**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**||---|---|---|---|
|**genuine (adj) — UNNAPPROVED**|CORRECT (adj)|MAKE SURE THAT THE<BR>INDICATION ON THE<BR>GAGUE IS CORRECT.|Make sure that the<BR>reading on the gauge is<BR>genuine.|
|**GET (v),**<br>**GETS,**<br>**GOT**<br>No other verb<br>forms.|To obtain, to come into<br>the state of having<br>Do not use this<br>word to mean<br>BECOME, GO,<br>DECREASE,<br>INCREASE.<br>Refer to rule 9.2<br>and the entries<br>from "get" until<BR>"get to" that<br>follow.|IF YOU GET THE FLUID<BR>ON YOUR SKIN, FLUSH<BR>YOUR SKIN<BR>IMMEDIATELY WITH<BR>CLEAN WATER.||
|**get (v) — UNNAPPROVED**|BECOME (v)|DO NOT LET THE<BR>HEATER BECOME TOO<BR>HOT.|Do not let the heater get<BR>too hot.|
|**get away (v) — UNNAPPROVED**|GO AWAY|BEFORE THE ENGINE<BR>STARTS, GO AWAY<BR>FROM THE EXHAUST<BR>AREA.|Get away from the<BR>exhaust area before the<BR>engine starts.|
|**get down (v) — UNNAPPROVED**|DECREASE (v)|IF THE TEMPERATURE<BR>DECREASES TO LESS<BR>THAN ZERO, DRAIN<BR>THE WATER SYSTEM.|If the temperature gets<BR>down to below zero,<BR>drain the water system.|
|||GO DOWN|BE CAREFUL WHEN<BR>YOU GO DOWN THE<BR>LADDER FROM THE<BR>COCKPIT TO THE<BR>AVIONICS<BR>COMPARTMENT.|Be careful when you get<BR>down the ladder from the<BR>cockpit into the avionics<BR>compartment.|
|**get into (v) — UNNAPPROVED**|GO INTO|INSTALL CAPS ON THE<BR>RECEPTACLES TO<BR>MAKE SURE THAT<BR>UNWANTED MATERIAL<BR>DOES NOT GO INTO<BR>THE RECEPTACLES.|Install caps to make sure<br>that foreign objects do<BR>not get into the<BR>receptacles.|
|**get off (v) — UNNAPPROVED**|MOVE OFF|BEFORE YOU MOVE<BR>THE AILERONS, TELL<BR>ALL PERSONS TO<BR>MOVE OFF THE<BR>WINGS.|Before you move the<br>ailerons, tell all persons<br>to get off the wings.|

# Page 254 of 434

**Page 2-1-G4**

**Page 2-1-G4**

**Issue 9 2025-01-15**

**Part 2 - Dictionary**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**||---|---|---|---|
|**get to (v) — UNNAPPROVED**|BE (v)|THE MOTOR STOPS<BR>WHEN THE LIMIT<BR>SWITCHES ARE AT<BR>THE END OF THEIR<BR>TRAVEL.|The motor stops when<br>the limit switches get to<br>the end of their travel.|
|||GO (v)|GO TO THE TOOL<BR>ROOM FOR THE<BR>NECESSARY TOOLS.|Get to the tool room for<br>the necessary tools.|
|||INCREASE (v)|WHEN THE<BR>TEMPERATURE OF<BR>THE VENTILATION AIR<BR>INCREASES TO 27 °C,<BR>THE DISCHARGE<BR>VALVE OPENS.|When the temperature of<br>the ventilation air gets to<br>27 °C, the discharge<br>valve opens.|
|**GIVE (v),**<br>**GIVES,**<br>**GAVE,**<br>**GIVEN**|To provide|THIS SECTION GIVES<BR>THE CLEANING<BR>PROCEDURES FOR<BR>THE DISASSEMBLED<BR>PARTS.|
|**gleam (v) — UNNAPPROVED**|SHINY (adj)|POLISH THE SURFACE<BR>WITH A SOFT CLOTH<BR>UNTIL IT BECOMES<BR>SHINY.|Polish the surface with a<br>soft cloth until it gleams.|
|**glitch (n) — UNNAPPROVED**|ERROR (n)|IF THERE IS AN<BR>ERROR IN THE<BR>SYSTEM, THE SCREEN<BR>SHOWS: "NO GO."|If there is a glitch in the<br>system, the screen<br>shows: NO GO.|
|||FAILURE (TN)|IF THERE IS A<BR>FAILURE IN THE<br>SYSTEM, THE SCREEN<BR>SHOWS: "NO GO."|If there is a glitch in the<br>system, the screen<br>shows: NO GO.|
|||UNSERVICEABLE (adj)|IF THE SYSTEM IS<BR>UNSERVICEABLE, THE<br>SCREEN SHOWS: "NO<BR>GO."|If there is a glitch in the<br>system, the screen<br>shows: NO GO.|
|**gloss (n) — UNNAPPROVED**|SHINY (adj)|POLISH THE SURFACE<BR>UNTIL IT IS VERY<BR>SHINY.|Polish the surface to a<br>high gloss.|
|**GLOSSY (adj)**<br>**(GLOSSIER,**<br>**GLOSSIEST)**|Smooth and shiny|APPLY THE PATCH<br>WITH THE MATT SIDE<br>AGAINST THE GLOSSY<br>SURFACE.|

# Page 255 of 434

**Page 2-1-G5**

**Page 2-1-G5**

**Issue 9 2025-01-15**

**Part 2 - Dictionary**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**||---|---|---|---|
|**glow (v) — UNNAPPROVED**|BE (v)|MAKE SURE THAT THE<BR>INDICATOR LIGHT IS<BR>ON.|Make sure that the<BR>indicator light glows.|
||||ADJUST THE<BR>POTENTIOMETER<BR>UNTIL THE LIGHT IS<BR>DIM.|Adjust the potentiometer<br>until the light glows<br>dimly.|
|**glue (v) — UNNAPPROVED**|BOND (v)|BOND THE PATCH TO<BR>THE SURFACE WITH<BR>THE APPLICABLE<BR>GLUE.|Glue the patch to the<br>surface.|
|||ATTACH (v)|ATTACH THE<BR>PROTECTIVE PLATE<br>TO THE SURFACE<br>WITH ADHESIVE<br>MATERIAL.|Glue the protective plate<br>to the surface.|
|**GO (v),**<br>**GOES,**<br>**WENT**|To move to or from<br>something|MAKE SURE THAT THE<BR>POINTER GOES OUT<BR>OF VIEW.|
|No other verb<br>forms.|
|**GO OFF (v),**<br>**GOES OFF,**<br>**WENT OFF**|To become dark when<br>an internal power source<br>is de-energized|THE ANNUNCIATOR<BR>LIGHT GOES OFF.|
|No other verb<br>forms.|
|**GOOD (adj)**<br>**(BETTER,**<br>**BEST)**|That is satisfactory|THIS MATERIAL GIVES<BR>GOOD PROTECTION<br>FROM CORROSION.|
|**gouge (v) — UNNAPPROVED**|GOUGE (TN)|IF A GOUGE OCCURS<BR>IN THE BLADE DURING<BR>REMOVAL, REPLACE<BR>THE BLADE.|If the blade was gouged<br>during removal, replace<br>it.|
|**govern (v) — UNNAPPROVED**|CONTROL (v)|THIS COMPONENT<BR>CONTROLS THE<BR>ENGINE SPEED.|This component governs<br>the engine speed.|
|**grab (v) — UNNAPPROVED**|USE (v)|USE A SCREWDRIVER<br>TO RELEASE THE<BR>CLIPS.|Grab a screwdriver to<br>release the clips.|
|||HOLD (v)|HOLD THE HANDLE.|Grab the handle.|

# Page 256 of 434

**Page 2-1-G6**

**Page 2-1-G6**

**Part 2 - Dictionary**

**Issue 9 2025-01-15**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**||---|---|---|---|
|**gradient (n) — UNNAPPROVED**|SLOPE (n)|WHEN YOU PARK THE<BR>VEHICLE ON A SLOPE,<BR>PUT CHOCKS ON THE<BR>WHEELS.|When you park the<br>vehicle on a gradient,<br>put chocks on the<br>wheels.|
|**gradual (adj) — UNNAPPROVED**|GRADUALLY (adv)|GRADUALLY ADJUST<BR>THE TEMPERATURE.|Make a gradual<br>adjustment to the<BR>temperature.|
|**GRADUALLY (adv)**|Slowly and continuously|GRADUALLY OPEN<BR>THE COCKS ON THE<BR>RECHARGING UNIT.|
|**graph (v) — UNNAPPROVED**|GRAPH (TN)|MAKE A GRAPH OF<BR>THE TEST RESULTS.|Graph the test results.|
|**grasp (v) — UNNAPPROVED**|HOLD (v)|HOLD THE HANDLE.|Grasp the handle.|
|**grave (adj) — UNNAPPROVED**|DANGEROUS (adj)|HYDRAULIC FLUID IS<BR>DANGEROUS FOR<BR>YOUR SKIN.|Hydraulic fluid can cause<br>grave skin problems.|
|**grease (v) — UNNAPPROVED**|LUBRICATE (v)|BEFORE YOU INSTALL<BR>THE O-RING,<BR>LUBRICATE IT WITH<BR>GREASE.|Grease the O-ring before<br>installation.|
|||GREASE (TN)|APPLY GREASE TO<BR>THE FASTENERS.|Grease the fasteners.|
|**great (adj) — UNNAPPROVED**|LARGE (adj)|AN INDICATION OF A<BR>LARGE QUANTITY OF<BR>FUEL SHOWS AN<BR>INCORRECT<BR>ADJUSTMENT OF THE<BR>FLOAT SWITCH.|A great amount of fuel<br>indicates incorrect<br>setting of the float<br>switch.|
|||MORE THAN|IF THE PRESSURE IS<br>MORE THAN 200psi,<BR>CLOSE THE VALVE.|If the pressure is greater<br>than 200 psi, close the<br>valve.|
|||VERY (adv)|BE VERY CAREFUL<BR>WHEN YOU RELEASE<BR>THE PRESSURE.|Take the greatest care<br>when you release the<br>pressure.|
|**greatly (adv) — UNNAPPROVED**|VERY MUCH|THIS METHOD CAN<BR>INCREASE THE RISK<BR>OF INJURY VERY<BR>MUCH.|This method can greatly<br>increase the risk of<br>injury.|
|**grip (n) — UNNAPPROVED**|HOLD (v)|HOLD THE JACK BODY<BR>TIGHTLY WHILE YOU<BR>TURN IT.|Make sure you have a<br>tight grip of the jack body<br>while turning it.|
