# Page 341 of 434

**Page 2-1-R1**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**||---|---|---|---|
||**re- (prefix) — UNNAPPROVED**|In general, use<br>the word AGAIN<br>(adv) or BACK<br>(adv) with the<br>basic word to<br>replace words<br>that have "re-" as<br>a prefix.|||
||**reach (v) — UNNAPPROVED**|GET (v)|WHEN YOU GET THE<br>CORRECT PRESSURE,<br>CLOSE THE VALVE.|When the correct<br>pressure is reached,<br>close the valve.|
|||TOUCH (v)|MAKE SURE THAT THE<br>EXTENSION BAR<br>TOUCHES THE<br>TARGET PLATE.|Make sure that the<br>extension bar reaches<br>the target plate.|
|||BE (v)|WHEN THE FLAPS ARE<br>AT THE 30 DEGREE<br>POSITION, INSTALL<br>THE RIGGING PIN.|When the flaps reach the<br>30 degree position,<br>install the rigging pin.|
||**reactivate (v) — UNNAPPROVED**|ACTIVATE (v)|ACTIVATE THE MODE<br>AGAIN.|Reactivate the mode.|
||**READ (v),**<br>**READS,**<br>**READ,**<br>**READ**|To come to know<br>information with the eyes<br>or electronically|READ THE<br>INDICATORS ON THE<br>CONTROL PANEL.|
||**reading (n) — UNNAPPROVED**|INDICATION (n)|MAKE SURE THAT THE<br>EXHAUST FROM THE<br>GROUND CART DOES<br>NOT CAUSE AN<br>INCORRECT<br>INDICATION.|Avoid an erroneous<br>reading caused by<br>exhaust from ground<br>cart.|
||**readjust (v) — UNNAPPROVED**|ADJUST (v)|AFTER THE<br>INSPECTION, ADJUST<br>THE LINKAGE AGAIN.|Readjust the linkage<br>after the inspection.|
||**ready (adj) — UNNAPPROVED**|PREPARE (v)|MAKE SURE THAT THE<br>CONTROL SYSTEM IS<br>PREPARED FOR<br>OPERATION.|Make sure that the<br>control system is in an<br>operational ready state.|
||**ready (v) — UNNAPPROVED**|PREPARE (v)|PREPARE THE<br>REMOVAL KIT FOR<br>THE REMOVAL OF THE<br>STRUT.|Ready the removal kit for<br>the removal of the strut.|

# Page 342 of 434

**Page 2-1-R2**

**Part 2 - Dictionary**

**Issue 9 2025-01-15**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**||---|---|---|---|
||**real (adj) — UNNAPPROVED**|AGREE (v)|MAKE SURE THAT THE<br>INDICATION ON THE<br>GAUGE AGREES WITH<br>THE QUANTITY OF<br>FUEL THAT IS IN THE<br>TANK.|Make sure that the<br>gauge shows the real<br>quantity of fuel that is in<br>the tank.|
||**REAR (adj)**|Away from the person<br>who looks or from a<br>reference point|INSTALL THE TWO<br>BOLTS IN THE REAR<br>FITTINGS.|
||**REAR (n)**|The rear part or rear<br>surface|THE CIRCUIT<br>BREAKERS ARE<br>INSTALLED ON THE<br>REAR OF THE UNIT.|
||**rear of (prep) — UNNAPPROVED**|AFT OF|THE PUMP IS<br>INSTALLED ON RIB 3,<br>AFT OF THE FRONT<br>SPAR.|The pump is located on<br>rib 3, rear of the front<br>spar.|
|||BEHIND (prep)|THE PUMP IS<br>INSTALLED ON RIB 3,<br>BEHIND THE FRONT<br>SPAR.|The pump is located on<br>rib 3, rear of the front<br>spar.|
||**rearmost (adj) — UNNAPPROVED**|REAR (n)|YOU CANNOT<br>REMOVE THE HALF<br>CLAMP NEAREST TO<br>THE REAR.|The rearmost half clamp<br>is not removable.|
||**REARWARD (adv)**|In the direction of the<br>rear|PULL THE LEVER<br>REARWARD.|
||**reason (n) — UNNAPPROVED**|CAUSE (n)|FIND THE CAUSE OF<br>THE INCORRECT<br>INDICATION.|Find the reason for the<br>wrong indication.|
|||BECAUSE OF (prep)|BECAUSE OF THE<br>POSSIBLE EFFECTS<br>ON YOUR HEALTH,<br>USE ONLY POTABLE<br>WATER.|For health reasons, only<br>use potable water.|
||**reassemble (v) — UNNAPPROVED**|ASSEMBLE (v)|ASSEMBLE THE<br>ACTUATOR AGAIN.|Reassemble the<br>actuator.|
||**rebuild (v) — UNNAPPROVED**|ASSEMBLE (v)|ASSEMBLE THE UNIT<br>AGAIN.|Rebuild the unit.|

**Issue 9 Part 2 - Dictionary 2025-01-15**

# Page 343 of 434

**Page 2-1-R3**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**||---|---|---|---|
||**RECEIVE (v),**<br>**RECEIVES,**<br>**RECEIVED,**<br>**RECEIVED**|To get energy, material,<br>or a signal from a<br>different source|MAKE SURE THAT THE<br>CAPTAIN'S BOOMSET<br>RECEIVES THE<br>SIGNALS CORRECTLY.|
||<br>|
||**RECESS (n)**|An indentation in a<br>surface|WHEN YOU CLEAN<br>THE SURFACES,<br>REMOVE THE STAINS<br>FROM THE<br>RECESSES.|
||**recess (v) — UNNAPPROVED**|RECESS (n)|DO NOT MAKE A<br>RECESS OF MORE<br>THAN 5 mm FOR THE<br>STUDS.|Do not recess studs<br>more than 5 mm.|
|||<br>|
|||THE FLANGE IS IN A<br>RECESS IN THE<br>FUSELAGE.|The flange is recessed<br>into the fuselage.|
||**recharge (v) — UNNAPPROVED**|CHARGE (v)|CHARGE THE<br>BATTERY AGAIN.|Recharge the battery.|
|||FILL (v)|FILL THE FLUID<br>RESERVOIR.|Recharge the fluid<br>reservoir.|
|||PRESSURIZE (v)|PRESSURIZE THE<br>ACCUMULATOR.|Recharge the<br>accumulator.|
||**recheck (v) — UNNAPPROVED**|MEASURE (v)|MEASURE THE<br>DISTANCE BETWEEN<br>THE FACES AGAIN.|Recheck the distance<br>between the faces.|
|||EXAMINE (v)|EXAMINE THE<br>CASTING FOR<br>CORROSION AGAIN.|Recheck the casting for<br>corrosion.|
|||CHECK (n)|DO A LEAKAGE<br>CHECK OF THE<br>FILTER ASSEMBLY<br>AGAIN.|Recheck the filter<br>assembly for leakage.|
||**reclaim (v) — UNNAPPROVED**|REPAIR (v)|REPAIR THE<br>DAMAGED FABRIC<br>AREA.|Reclaim the damaged<br>fabric area.|
||**recleat (v) — UNNAPPROVED**|ATTACH (v)<br>(TO A CLEAT [TN])|ATTACH THE<br>TIEDOWN CORD TO A<br>CLEAT.|Recleat the tiedown<br>cord.|
||**reclose (v) — UNNAPPROVED**|CLOSE (v)|AFTER SERVICING,<br>CLOSE THE<br>COMPARTMENT<br>AGAIN.|Reclose the<br>compartment after<br>servicing.|

# Page 344 of 434

**Page 2-1-R4**

**Part 2 - Dictionary**

**Issue 9 2025-01-15**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**||---|---|---|---|
||**recoil (v) — UNNAPPROVED**|MOVE BACK|BE CAREFUL WHEN<br>THE SLIDE MOVES<br>BACK.|Be careful when the<br>slide recoils.|
|||WIND (v)|WIND THE PROBE<br>WIRE BACK ON THE<br>SPOOL.|Recoil the probe wire<br>back on the spool.|
|||RECOIL (TN)|THE GUN BARREL HAS<br>A QUICK RECOIL.|The gun barrel recoils<br>quickly.|
||**RECOMMEND (v),**<br>**RECOMMENDS,**<br>**RECOMMENDED,**<br>**RECOMMENDED**|To advise that which is<br>best|THE MANUFACTURER<br>RECOMMENDS THAT<br>YOU KEEP THE UNIT<br>IN A DEDICATED<br>AREA.|
||**recondition (v) — UNNAPPROVED**|REPAIR (v)|REPAIR THE SEATS.|Recondition the seats.|
|||OVERHAUL (TN)|DO AN OVERHAUL OF<br>THE ENGINE.|Recondition the engine.|
||**reconstruction (n) — UNNAPPROVED**|REPAIR (n)|RECORD ALL REPAIRS<br>TO THE SKIN<br>SURFACE.|Record all reconstruction<br>of the skin surface.|
|||REPAIR (v)|THIS PROCEDURE<br>TELLS YOU HOW TO<br>REPAIR THE<br>SURFACE.|This procedure is for the<br>reconstruction of the<br>surface.|
||**RECORD (v),**<br>**RECORDS,**<br>**RECORDED,**<br>**RECORDED**|1.<br>To make notes of<br>and keep data to<br>use subsequently|RECORD THE<br>RESULTS.|
|||2.<br>To put data on a<br>storage medium|THE COCKPIT VOICE<br>RECORDER RECORDS<br>SIGNALS FROM FOUR<br>AUDIO INPUTS<br>DURING THE FLIGHT.|
||**recover (v) — UNNAPPROVED**|COLLECT (v)|REMOVE THE NUT<br>AND THE BOLT. THEN,<br>COLLECT THE<br>WASHER.|Remove the nut and the<br>bolt. Then, recover the<br>washer.|
||**rectify (v) — UNNAPPROVED**|CORRECT (v)|BEFORE YOU START<br>THE PROCEDURE<br>AGAIN, CORRECT THE<br>DEFECT.|Rectify the defect before<br>you restart the<br>procedure.|
||**recur (v) — UNNAPPROVED**|OCCUR (v)|IF THE SYMPTOMS<br>OCCUR AGAIN, DO A<br>SYSTEM TEST.|If the symptoms recur,<br>do a system test.|

**Issue 9 2025-01-15**

**Part 2 - Dictionary**
