# Page 261–264 of 434

> **Source:** ASD-STE100 Issue 9, January 2025
> **Pages:** 261–264 of 434

# Page 261 of 434

| Word (POS) | Approved meaning / ALTERNATIVES | STE example | Non-STE example |
|------------|--------------------------------|-------------|-----------------|
| heat (v) — UNNAPPROVED | HEAT (n) | USE HEAT TO INCREASE THE TEMPERATURE OF THE OIL TO 40°C. | Heat the oil to 40°C. |
| heat (v) — UNNAPPROVED | HOT (adj) | WHEN THE OIL IS HOT, IT FLOWS FREELY. | When you heat the oil, it flows freely. |
| HEAVY (adj) (HEAVIER, HEAVIEST) | That has a large mass, weight, or force | A SUPPORT WILL BE NECESSARY BECAUSE THE CONTROL UNIT IS HEAVY. | |
| HEIGHT (n) | The vertical distance | THE HEIGHT FROM THE GROUND TO THE TOP OF THE FIN CAN CHANGE. | |
| heighten (v) — UNNAPPROVED | INCREASE (v) | STRONG WINDS WILL INCREASE THE RISK OF DAMAGE. | Strong winds will heighten the risk of damage. |
| help (n) — UNNAPPROVED | AID (n) | GET MEDICAL AID IMMEDIATELY. | You must get medical help immediately. |
| HELP (v), HELPS, HELPED, HELPED | To make something easier or better | PETROLATUM HELPS TO PREVENT CORROSION OF THE TERMINALS. | |
| helpful (adj) — UNNAPPROVED | HELP (v) | RECORD THE LOCKWIRE POSITIONS. THIS INFORMATION WILL HELP YOU DURING THE ASSEMBLY PROCEDURE. | Record the lockwire positions. This will be helpful during the assembly procedure. |
| HERE (adv) | In this position | TO DOWNLOAD THE FILE, CLICK HERE. | |
| hesitation (n) — UNNAPPROVED | SMOOTHLY (adv) | MAKE SURE THAT THE SOLENOID OPERATES SMOOTHLY. | Make sure that the solenoid operates without hesitation. |
| hesitation (n) — UNNAPPROVED | CORRECTLY (adv) | THE VALVE MUST OPERATE CORRECTLY. | The valve must operate without hesitation. |
| hesitation (n) — UNNAPPROVED | IMMEDIATELY (adv) | WHEN YOU OPEN THE CIRCUIT BREAKER, THE LIGHT MUST COME ON IMMEDIATELY. | When you open the circuit breaker, the light must come on without hesitation. |

# Page 262 of 434

| Word (POS) | Approved meaning / ALTERNATIVES | STE example | Non-STE example |
|------------|--------------------------------|-------------|-----------------|
| HIGH (adj) (HIGHER, HIGHEST) | That is of large value | USE THE SPECIAL PROTECTION FOR STORAGE IN HIGH TEMPERATURES. | |
| highly (adv) — UNNAPPROVED | VERY (adv) | TOLUENE IS VERY FLAMMABLE. | Toluene is highly flammable. |
| hinder (v) — UNNAPPROVED | PREVENT (v) | SCRATCHES CAN PREVENT THE FREE MOVEMENT OF THE PISTON IN THE SLEEVE. | Scratches can hinder the movement of the piston in the sleeve. |
| hinder (v) — UNNAPPROVED | DECREASE (v) | A CLOGGED DUCT WILL DECREASE AIRFLOW. | A clogged duct will hinder airflow. |
| hinder (v) — UNNAPPROVED | BLOCKAGE (n) | MAKE SURE THAT THERE IS NO BLOCKAGE IN THE PIPE THAT PREVENTS AIRFLOW. | Make sure that there is nothing in the pipe to hinder airflow. |
| hinder (v) — UNNAPPROVED | CLOGGED (adj) | MAKE SURE THAT THE PIPE IS NOT CLOGGED. | Make sure that there is nothing in the pipe to hinder airflow. |
| hinge (v) — UNNAPPROVED | TURN (v) | THE PANELS TURN ON TWO NYLON STRAPS. | Panels hinge on two nylon straps. |
| HIT (v), HITS, HIT, HIT | To touch suddenly and with much force | DO NOT HIT THE CARTRIDGE. | |
| hitch (v) — UNNAPPROVED | CONNECT (v) | CONNECT THE TOWING ARM TO THE NOSEWHEEL. | Hitch the towing arm to the nosewheel. |
| hoist (v) — UNNAPPROVED | LIFT (v) | LIFT THE MODULE. | Hoist the module. |
| hold (n) — UNNAPPROVED | HOLD (v) | MAKE SURE THAT YOU HOLD THE ROD TIGHTLY. | Make sure that you have a tight hold on the rod. |
| HOLD (v), HOLDS, HELD, HELD | 1. To continue to have in the hand or grip | HOLD THE ROD TIGHTLY. | |
| HOLD (v), HOLDS, HELD, HELD | 2. To continue to have in a specified location, position, or condition | HOLD THE AIRSPEED INDICATION AT THE SAME VALUE FOR 2 MINUTES. | |

# Page 263 of 434

| Word (POS) | Approved meaning / ALTERNATIVES | STE example | Non-STE example |
|------------|--------------------------------|-------------|-----------------|
| hold back (v) — UNNAPPROVED | PREVENT (v) | AT FULL THRUST, the BRAKES MUST PREVENT MOVEMENT OF THE AIRCRAFT. | At full thrust, the brakes must hold the aircraft back. |
| hold off (v) — UNNAPPROVED | PREVENT (v) | THE PROTECTIVE PAINT WILL PREVENT CORROSION FOR SIX MONTHS. | The protective paint will hold off corrosion for six months. |
| HOLE (n) | An empty space in a solid object | MAKE SURE THAT THE HOLES IN THE BUSHING ALIGN WITH THOSE IN THE HOUSING. | |
| hook (v) — UNNAPPROVED | PUT (v) | PUT THE SLING ON THE SHACKLE. | Hook the sling on the shackle. |
| hook up (v) — UNNAPPROVED | CONNECT (v) | CONNECT THE TOWING ARM TO THE NOSE GEAR. | Hook the towing arm up to the nose gear. |
| HORIZONTAL (adj) | Parallel to the horizon or a baseline | ADJUST THE SLING UNTIL THE FLAP IS HORIZONTAL. | |
| HORIZONTALLY (adv) | In a horizontal position | THE VALVE IS INSTALLED HORIZONTALLY. | |
| HOT (adj) (HOTTER, HOTTEST) | At a high temperature | DRY THE SURFACE WITH HOT AIR. | |
| house (v) — UNNAPPROVED | CONTAIN (v) | THE MODULE CONTAINS FIVE COMPONENTS. | The module houses five components. |
| HOW (adv) | By which manner | PARAGRAPH 7.0 TELLS YOU HOW TO INSTALL THE UNIT. | |
| however (adv) — UNNAPPROVED | BUT (conj) | THE DRYING TIME IS USUALLY 24 HOURS. BUT THE PROCEDURE IN THIS STEP WILL DECREASE THE DRYING TIME TO 12 HOURS. | The drying time is usually 24 hours. However, the procedure in this step will decrease the drying time to 12 hours. |

# Page 264 of 434

| Word (POS) | Approved meaning / ALTERNATIVES | STE example | Non-STE example |
|------------|--------------------------------|-------------|-----------------|
| huge (adj) — UNNAPPROVED | LARGE (adj) | TO REMOVE THE PAINT STRIPPER, FLUSH THE SURFACE WITH LARGE QUANTITIES OF WATER. | To remove the paint stripper, flush the surface with huge quantities of water. |
| hum (v) — UNNAPPROVED | HUM (TN) | ADJUST THE POTENTIOMETER UNTIL YOU DO NOT HEAR A HUM FROM THE LOUDSPEAKER. | Adjust the potentiometer until the loudspeaker no longer hums. |
| hurt (v) — UNNAPPROVED | INJURY (n) | BE CAREFUL WHEN YOU DO THIS PROCEDURE. IF THE UNIT FALLS, IT CAN CAUSE INJURY TO PERSONS. | Be careful when you do this procedure. If the unit falls, it can hurt persons. |
| HYDRAULIC (adj) | Related to, or operated by, pressurized liquid | CONNECT THE FITTINGS TO THE HYDRAULIC TEST BENCH. | |
| HYDRAULICALLY (adv) | With hydraulic power | MAKE SURE THAT THE LINES ARE HYDRAULICALLY OPERATED. | |
