# Page 349–352 of 434

> **Source:** ASD-STE100 Issue 9, January 2025
> **Pages:** 349–352 of 434

# Page 349 of 434

| Word (part of speech) | Approved meaning/ALTERNATIVES | STE EXAMPLE | Non-STE example |
|---|---|---|---|
| **renew (v) — UNNAPPROVED** | NEW (adj) | USE NEW ADHESIVE<br>TAPE. | Renew the adhesive<br>tape. |
| **renovate (v) — UNNAPPROVED** | REPAIR (v)<br>NEW (adj) | REPAIR ALL WORN<br>SURFACES.<br>IF THE PAINT ON THE<br>CONTROL BOX IS<br>DAMAGED, APPLY<br>NEW PAINT. | Renovate all worn<br>surfaces.<br>Renovate any damaged<br>paint on the control box. |
| **repack (v) — UNNAPPROVED** | PUT (v)<br>FILL (v) | PUT THE ASSEMBLY<br>BACK IN THE BOX.<br>FILL THE HOLE WITH<br>GREASE AGAIN. | Repack the assembly in<br>the box.<br>Repack the hole with<br>grease. |
| **repaint (v) — UNNAPPROVED** | PAINT (v) | PAINT ALL THE<br>SURFACES AGAIN. | Repaint all the surfaces. |
| **REPAIR (n)** | The act of repairing or<br>the result when<br>something is repaired | AFTER THE REPAIR,<br>APPLY A PROTECTIVE<br>LAYER OF GREASE TO<br>ALL EXTERNAL<br>SURFACES. |  |
| **REPAIR (v),**<br>**REPAIRS,**<br>**REPAIRED,**<br>**REPAIRED** | To make an item<br>serviceable | REPAIR THE<br>DEFECTIVE WIRING. |  |
| **repairable (adj) — UNNAPPROVED** | REPAIR (v) | IT IS POSSIBLE TO<br>REPAIR THIS<br>DAMAGE. | This damage is<br>repairable. |
| **repeat (v) — UNNAPPROVED** | AGAIN (adv) | DO STEPS (10) THRU<br>(14) AGAIN. | Repeat steps (10) to<br>(14). |
| **repeated (adj) — UNNAPPROVED** | AGAIN AND AGAIN | IF YOU HEAR SIGNALS<br>AGAIN AND AGAIN, DO<br>A CHECK OF THE "AP<br>ENGAGE" BUTTON ON<br>THE FLIGHT MODE<br>PANEL. | If repeated signals are<br>heard, check the AP<br>ENGAGE button on the<br>flight mode panel. |
| **repeatedly (adv) — UNNAPPROVED** | AGAIN AND AGAIN | IF THE VOLTAGE<br>DECREASES AGAIN<br>AND AGAIN, ADJUST<br>THE VOLTAGE<br>REGULATOR. | If voltage drops<br>repeatedly, adjust the<br>voltage regulator. |

# Page 350 of 434

| Word (part of speech) | Approved meaning/ALTERNATIVES | STE EXAMPLE | Non-STE example |
|---|---|---|---|
| **REPLACE (v),**<br>**REPLACES,**<br>**REPLACED,**<br>**REPLACED** | To remove an item and<br>to install a new or<br>serviceable item of the<br>same type | REPLACE THE RELAY. |  |
| **REPLACEMENT**<br>**(n)** | The item you install<br>when you replace an<br>item | MAKE SURE THAT THE<br>REPLACEMENT HAS<br>THE CORRECT<br>DIMENSIONS. |  |
| **replenish (v) — UNNAPPROVED** | FILL (v)<br>ADD (v)<br>REFUEL (v) | FILL THE<br>ACCUMULATOR WITH<br>OIL.<br>ADD OIL TO THE<br>ACCUMULATOR.<br>REFUEL THE VEHICLE. | Replenish the<br>accumulator with oil.<br>Replenish the oil in the<br>accumulator.<br>Replenish the vehicle<br>with fuel. |
| **REPORT (n)** | The information that is<br>recorded about a subject<br>or occurrence | IF THERE IS A<br>REPORT OF DAMAGE,<br>DO AN ACCURATE<br>INSPECTION. |  |
| **reposition (v) — UNNAPPROVED** | MOVE (v)<br>PUT (v)<br>SET (v) | MOVE THE LEVER<br>BACK TO ITS INITIAL<br>POSITION.<br>PUT THE LEVER BACK<br>TO ITS INITIAL<br>POSITION.<br>SET THE SWITCH<br>BACK TO THE OFF<br>POSITION. | Reposition the lever.<br>Reposition the lever.<br>Reposition the switch to<br>OFF. |
| **represent (v) — UNNAPPROVED** | SHOW (v) | THE SUCTION SHOWS<br>AS AN ALTIMETER<br>INDICATION. | The suction is<br>represented by an<br>altimeter reading. |
| **repressurize (v) — UNNAPPROVED** | PRESSURIZE (v) | PRESSURIZE THE<br>TANK AGAIN. | Repressurize the tank. |
| **request (n) — UNNAPPROVED** | TELL (v)<br>WRITE (v) | TELL THE FIRE<br>SERVICE TO HELP<br>YOU.<br>IF AID IS NECESSARY,<br>WRITE TO THE<br>MANUFACTURER. | Make a request for<br>external fire support.<br>Any request for<br>assistance should be<br>addressed to the<br>manufacturer. |

# Page 351 of 434

| Word (part of speech) | Approved meaning/ALTERNATIVES | STE EXAMPLE | Non-STE example |
|---|---|---|---|
| **request (v) — UNNAPPROVED** | TELL (v)<br>WRITE (v) | TELL THE FIRE<br>SERVICE TO HELP<br>YOU.<br>WRITE TO THE<br>MANUFACTURER FOR<br>REPAIR<br>INSTRUCTIONS. | Request external fire<br>support.<br>Request repair<br>instructions from the<br>manufacturer. |
| **require (v) — UNNAPPROVED** | NECESSARY (adj) | DURING THIS<br>PROCEDURE, CLEAN<br>FILTERS ARE<br>NECESSARY. | During this procedure,<br>clean filters are required. |
| **reseal (v) — UNNAPPROVED** | SEAL (v) | SEAL THE CONTAINER<br>AGAIN. | <br>Reseal the container. |
| **reset (v) — UNNAPPROVED** | SET (v) | SET THE INDICATOR<br>TO A NEW POSITION. | Reset the indicator to a<br>new position. |
| **residual (adj) — UNNAPPROVED** | REMAINING (adj) | REMOVE ALL THE<br>REMAINING GREASE. | Remove all residual<br>grease. |
| **residue (n) — UNNAPPROVED** | REMAINING (adj) | REMOVE THE<br>REMAINING GREASE. | Remove the grease<br>residues. |
| **RESISTANT (adj)** | That will help to prevent<br>something | THE MATERIAL OF<br>THE SEATS IS<br>RESISTANT TO FIRE. |  |
| **respective (adj) — UNNAPPROVED** | RELATED (adj)<br>CORRECT (adj) | ATTACH THE CABLES<br>TO THEIR RELATED<br>SHACKLES.<br>INSTALL THE BOLTS<br>IN THEIR CORRECT<br>POSITIONS. | Attach the cables to their<br>respective shackles.<br>Install the bolts in their<br>respective positions. |
| **respectively (adv) — UNNAPPROVED** | RELATED (adj) | ENGINES 1 AND 2<br>SUPPLY HOT AIR TO<br>THEIR RELATED<br>WINGS. | Engines 1 and 2 supply<br>the left and right wings<br>respectively with hot air. |
| **respond (v) — UNNAPPROVED** | RESULT (n) | IF THE INSTRUMENT<br>DOES NOT GIVE A<br>RESULT, DO A TEST. | If the instrument fails to<br>respond, do a test. |
| **rest (n) — UNNAPPROVED** | REMAINING (adj) | THE REMAINING<br>INSTRUCTIONS ARE<br>APPLICABLE ONLY TO<br>APPROVED<br>PERSONNEL. | The rest of these<br>instructions only apply to<br>approved personnel. |

# Page 352 of 434

| Word (part of speech) | Approved meaning/ALTERNATIVES | STE EXAMPLE | Non-STE example |
|---|---|---|---|
| **rest (v) — UNNAPPROVED** | BE (v)<br>PUT (v) | THE VEHICLE MUST<br>BE ON ITS WHEELS.<br>PUT THE REMOVED<br>PART ON A CLEAN<br>SURFACE. | The vehicle must rest on<br>its wheels.<br>Rest the removed part<br>on a clean surface. |
| **restart (v) — UNNAPPROVED** | START (v) | START THE UNIT<br>AGAIN. | Restart the unit. |
| **restore (v) — UNNAPPROVED** | REPAIR (v)<br>PUT (v) | DO NOT REPAIR THE<br>CHROMIC ACID<br>ANODIZING ON THE<br>SKIN PANEL.<br>PUT THE PINS BACK<br>IN THEIR LOCATION. | Do not restore the<br>chromic acid anodizing<br>on the skin panel.<br>Restore the pins to their<br>location. |
| **restrain (v) — UNNAPPROVED** | HOLD (v)<br>STOP (v)<br>PREVENT (v)<br>LIMIT (n) | HOLD THE HOSES IN<br>POSITION.<br>STOP THE FLUID<br>FLOW.<br>THE STOP PREVENTS<br>THE MOVEMENT OF<br>THE ROD.<br>THE VALVE KEEPS<br>THE AIRFLOW IN<br>LIMITS. | Restrain the hoses in<br>position.<br>Restrain all fluid flow.<br>The stop restrains the<br>movement of the rod.<br>The valve restrains the<br>airflow. |
| **restrict (v) — UNNAPPROVED** | DECREASE (v)<br>PREVENT (v)<br>ONLY (adv)<br>LIMIT (n) | THE METERING PLUG<br>DECREASES THE<br>FUEL FLOW.<br>THE STOP PREVENTS<br>THE MOVEMENT OF<br>THE ROD.<br>USE THESE NUTS<br>ONLY FOR THE TEST.<br>THE VALVE KEEPS<br>THE AIRFLOW IN<br>LIMITS. | The metering plug<br>restricts the fuel flow.<br>The stop restricts the<br>movement of the rod.<br>Restrict the use of these<br>nuts to test only.<br>The valve restricts the<br>airflow. |
| **RESULT (n)** | Something that occurs<br>when you do something | IF THESE TESTS DO<br>NOT GIVE THE<br>CORRECT RESULTS,<br>REPLACE THE UNIT. |  |
