# Page 177 of 434

**Page 2-1-C2**

**Part 2 - Dictionary**

**Issue 9 2025-01-15**

**ASD-STE100 Simplified Technical English**

||**Word**
**(part of speech)**|**Approved meaning/**
**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|

||---|---|---|---|

||**care (n) — UNNAPPROVED**|PRECAUTION (n)|WHEN YOU DO WORK
WITH HIGH
VOLTAGES, OBEY THE
SAFETY
PRECAUTIONS.|You must take care
when you work with high
voltages.|
|||CAREFUL (adj)|BE CAREFUL WHEN
YOU INSTALL THE
NUTS.|Take care when
installing the nuts.|
|||CAREFULLY (adv)|REMOVE THE
GEARBOX
CAREFULLY.|Remove the gearbox
with great care.|
||**CAREFUL (adj)**|With precaution|BE CAREFUL WHEN
YOU REMOVE THE
COVER.|
||**CAREFULLY (adv)**|In a careful manner|CAREFULLY APPLY A
BEAD OF SEALING
COMPOUND.|
||**carry (v) — UNNAPPROVED**|TRANSMIT (v)|THE CABLE
TRANSMITS THE
ELECTRICAL ENERGY
FROM THE IGNITION
EXCITER TO THE
IGNITER.|The cable carries the
electrical energy from
the ignition exciter to the
igniter.|
|||TRANSPORT (TN)|THIS VEHICLE IS FOR
THE TRANSPORT OF
FIVE PASSENGERS.|This vehicle is meant to
carry five passengers.|

||**carry out (v) — UNNAPPROVED**|DO (v)|DO THE LEAK TEST.|Carry out the leak test.|

|||You can use a
more accurate
command verb.|||
|||MEASURE (v)|MEASURE THE
CLEARANCE OF THE
IMPELLER.|Carry out the clearance
measurement of the
impeller.|
||**case (n) — UNNAPPROVED**|CONDITION (n)|FIGURE 1 SHOWS THE
DATA FOR ALL
OPERATIONAL
CONDITIONS.|The data for all
operational cases are
shown in Figure 1.|
||**case (in case of)**
**(conj)**|IF (conj)|IF THERE IS A FIRE,
OPERATE THE CRASH
SWITCHES.|In case of a fire, operate
the crash switches.|

# Page 178 of 434

**Page 2-1-C3**

**Issue 9 Part 2 - Dictionary 2025-01-15**

**ASD-STE100 Simplified Technical English**

||**Word**
**(part of speech)**|**Approved meaning/**
**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|

||---|---|---|---|

||**CATCH (v),**
**CATCHES,**
**CAUGHT,**
**CAUGHT**|To stop or prevent the
movement of something|THE LUG ON THE
PANEL OPENING
CATCHES THE
BOTTOM OF THE
DRAWER.|
|||For other
meanings, use:|DO NOT LET THE
TOOL CATCH ON THE
PANEL.|
|||COLLECT (v)|COLLECT THE
LEAKAGE IN A
GRADUATED BEAKER.|Catch the leakage in a
graduated beaker.|
||**categorize (v) — UNNAPPROVED**|CATEGORY (TN)|THE TESTING
EQUIPMENT DIVIDES
THE FAULTS INTO
CATEGORIES.|The testing equipment
categorizes the faults.|
||**CAUSE (n)**|Something that brings
about a result|DO THE
TROUBLESHOOTING
PROCEDURE TO FIND
THE CAUSE OF THE
MALFUNCTION.|
||**CAUSE (v),**
**CAUSES,**
**CAUSED,**
**CAUSED**|To be the cause of|METAL OBJECTS CAN
CAUSE MAGNETIC
INTERFERENCE.|
||**caution (v) — UNNAPPROVED**|TELL (v)|TELL ALL PERSONNEL
NOT TO SMOKE NEAR
FUEL TANKS.|Caution all personnel not
to smoke near fuel
tanks.|
||**cautiously (adv) — UNNAPPROVED**|CAREFULLY (adv)|CAREFULLY FEEL THE
HEATER WITH YOUR
HANDS TO MAKE
SURE THAT IT
OPERATES.|
Cautiously feel the
heater with your hands
to make sure that it
operates.
||**cavity (n) — UNNAPPROVED**|HOLE (n)|FILL THE HOLE WITH
RESIN.|Fill the cavity with resin.
|||SPACE (n)|FILL THE SPACE
BETWEEN THE PATCH
AND THE ADJACENT
STRUCTURE WITH
SEALANT.|Fill the cavity between
the patch and the
adjacent structure with
sealant.|
||**cease (v) — UNNAPPROVED**|STOP (v)|THE WARNING STOPS
AT 17 DEG.|The warning ceases at
17 deg.||

# Page 179 of 434

**Page 2-1-C4**

**Part 2 - Dictionary**

**Issue 9 2025-01-15**

**ASD-STE100 Simplified Technical English**

||**Word**
**(part of speech)**|**Approved meaning/**
**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|

||---|---|---|---|

||**center (v) — UNNAPPROVED**|CENTER (TN)|ALIGN THE PISTON
WITH THE CENTER OF
THE SLEEVE.|Center the piston in the
sleeve.||
||**centralize (v) — UNNAPPROVED**|CENTER (TN)|SET THE CONTROLS
TO THE CENTER
POSITION.|Centralize the controls.||
||**certain (adj) — UNNAPPROVED**|SURE (adj)|IF YOU ARE NOT SURE
THAT THE RESULTS
ARE CORRECT, DO
THE TEST AGAIN.|If you are not certain that
the results are correct,
do the test again.
|||SOME (adj)|SOME FUNCTIONS
ARE NOT AVAILABLE.|Certain functions are not
available.
|||SPECIFIED (adj)|THE SPECIFIED
FUNCTIONS ARE NOT
AVAILABLE.|Certain functions are not
available.|
||**certify (v) — UNNAPPROVED**|WRITE (v)|WRITE THE CHANGE
IN THE LOGBOOK.|Certify the change in the
logbook.
|||APPROVAL (n)|GET APPROVAL FROM
YOUR SUPERVISOR
FOR THE REPAIR.|Get the supervisor to
certify the repair.

||

||**chafe (v) — UNNAPPROVED**|RUB (v)|DO NOT LET THE
WIRES RUB.|Do not let the wires
chafe.||
||**chafed (adj) — UNNAPPROVED**|WORN (adj)|EXAMINE THE TUBING
FOR WORN AREAS.|Examine the tubing for
chafed areas.||
||**chance**
**(by chance) (n)**|RISK (n)|IF THERE IS A RISK OF
FUEL LEAKAGE, PUT A
CONTAINER BELOW
THE UNIT.|If there is a chance of
fuel leakage, put a
container below the unit.
|||ACCIDENTALLY (adv)|IF THE LEVER MOVED
ACCIDENTALLY, DO
THE TEST AGAIN.|If, by chance, the lever
moved, do the test
again.|
||**CHANGE (n)**|That which occurs when
something changes|THE COLOR CHANGE
SHOWS THAT THE
TEMPERATURE IS
TOO HIGH.|

# Page 180 of 434

**Page 2-1-C5**

**Issue 9 2025-01-15**

**Part 2 - Dictionary**

**ASD-STE100 Simplified Technical English**

||**Word**
**(part of speech)**|**Approved meaning/**
**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|

||---|---|---|---|

||**CHANGE (v),**
**CHANGES,**
**CHANGED,**
**CHANGED**|To become or to cause
to become different|IF THE HUMIDITY
CHANGES
FREQUENTLY, PUT A
COVER ON THE UNIT.|
|||For other
meanings, use:|CHANGE THE COLOR
OF THE DISPLAY.|
|||REPLACE (v)|REPLACE THE
DAMAGED VALVE.|Change the damaged
valve.||
||**channel (v) — UNNAPPROVED**|CHANNEL (TN)|INSTALL THE WIRES
IN THE CHANNEL
ALONG THE HOUSING.|Channel the wires along
the housing.||
||**characteristic (n) — UNNAPPROVED**|PROPERTY (n)|THE PROPERTIES OF
THESE SEALANTS
PREVENT
CORROSION.|The characteristics of
these sealants prevent
corrosion.
|||QUALITY (n)|DO NOT USE THIS
MATERIAL BECAUSE
IT DOES NOT HAVE
THE NECESSARY
QUALITIES.|Do not use this material
because it doesn't have
the necessary
characteristics.|
||**CHARGE (v),**
**CHARGES,**
**CHARGED,**
**CHARGED**|To accumulate or add
electrical energy|CHARGE THE
BATTERY.|
|||||MAKE SURE THAT THE
BATTERY CHARGES.
|||For other
meanings, use:|||
|||FILL (v)|FILL THE TANK WITH
10 LITERS OF
METHANOL.|Charge the tank with
10 liters of methanol.
|||PRESSURIZE (v)|PRESSURIZE THE
ACCUMULATOR WITH
NITROGEN.|Charge the accumulator
with nitrogen.

||

||**CHECK (n)**|The procedure you do to
make sure that
something operates
correctly or has no
defects|DO A CHECK OF THE
HYDRAULIC SYSTEM.|
|||||DO A CHECK FOR
LOOSE FASTENERS.||
