<!-- GROUP: 021-dict-q-r -->
<!-- PAGES: 338-357 -->
<!-- SECTION: DICT -->
<!-- KEY: Q-R -->
<!-- WORKERS: R085, R086, R087, R088, R089, R090 -->
<!-- PAGE_COUNT: 20 -->

# Dict Q R

> **Source:** ASD-STE100 Issue 9, January 2025
> **Section:** DICT (Q-R)
> **Pages:** 338-357 of 434 (20 pages)

<!-- Page 338 of 434 -->

| Word (POS) | Approved meaning/ALTERNATIVES | STE EXAMPLE | Non-STE example |
|---|---|---|---|
| qualified (adj) — UNNAPPROVED | APPROVED (adj) | AN APPROVED PERSON MUST DO THE IMPORTANT CHECKS. | A qualified person must do the important checks. |
| QUALITY (n) | Condition, property, or type | THIS MEDICAL EQUIPMENT MUST BE OF GOOD QUALITY. |  |
| QUANTITY (n) | A specified amount or number For an amount that you can count, use NUMBER (n). | APPLY A SMALL QUANTITY OF LUBRICATING OIL ON THE THREADS OF THE BOLTS. MAKE SURE THAT YOU HAVE THE CORRECT NUMBER OF SHIMS AVAILABLE. |  |
| quarterly (adv) — UNNAPPROVED | INTERVAL (n) | SEND REPORTS TO THE AUTHORITIES AT INTERVALS OF THREE MONTHS. | Send reports to the authorities quarterly. |
| questionable (adj) — UNNAPPROVED | NOT SURE | IF YOU ARE NOT SURE OF THEIR CONDITION, REJECT THE PARTS. | Reject the parts that are in a questionable condition. |
| quick (adj) — UNNAPPROVED | QUICKLY (adv) | MAKE SURE THAT THE ROD DOES NOT MOVE QUICKLY. | Make sure that there is no quick movement of the rod. |
| QUICKLY (adv) | In a fast manner | MAKE SURE THAT THE PRESSURE DECREASES QUICKLY. |  |
| quit (v) — UNNAPPROVED | GO (v) | BEFORE YOU START THE ENGINE, MAKE SURE THAT ALL PERSONS GO AWAY FROM THE DANGER AREA. | Before you start the engine, make sure that all persons quit the danger area. |
| STOP (v) | IF THE RED LIGHT COMES ON, STOP THE REFUEL PROCEDURE. |  | If the red light comes on, quit the refuel procedure. |
| quote (v) — UNNAPPROVED | GIVE (v) | THE TABLE GIVES THE MAXIMUM TOLERANCE FOR THE HOLE. | The table quotes the maximum tolerance for the hole. |

<!-- Page 339 of 434 -->
Word Approved meaning/ (part of speech) ALTERNATIVES STE EXAMPLE
Non-STE example
Blank Page

<!-- Page 340 of 434 -->

|---|---|---|---|
| RADIAL (adj) | Along a radius | DO A CHECK FOR RADIAL CUTS, CRACKS, OR SPLITS. |  |
| RADIALLY (adv) | Along a radius | THE FAN BLADES ARE INSTALLED RADIALLY. |  |
| RADIOACTIVE (adj) | Related to radioactivity | DO A CHECK FOR RADIOACTIVE CONTAMINATION. |  |
| raise (v) — UNNAPPROVED | LIFT (v) | DO NOT LIFT THE COVER MORE THAN THE SPECIFIED CLEARANCE. | Do not raise the cover more than the specified clearance. |
| INCREASE (v) | INCREASE THE TEMPERATURE BY 10 DEG. | Raise the temperature 10 deg. |  |
| RETRACT (v) | RETRACT THE LANDING GEAR. | Raise the landing gear. |  |
| RANDOM (adj) | Not regular | DURING THIS PROCEDURE, DO RANDOM CHECKS OF THE TIRE PRESSURE. |  |
| RANDOMLY (adv) | Not regularly | DO THESE CHECKS RANDOMLY. |  |
| RANGE (n) | The limits within which something operates | THE AUDIO SPECTRUM IS THE FREQUENCY RANGE AT WHICH HUMANS CAN HEAR. |  |
| rapid (adj) — UNNAPPROVED | FAST (adj) | CHEMICAL AGENTS CAUSE FAST DETERIORATION OF PAINTED SURFACES. | Chemical agents cause rapid deterioration of painted surfaces. |
| rapidly (adv) — UNNAPPROVED | QUICKLY (adv) | QUICKLY TURN THE HANDLE CLOCKWISE. | Rapidly turn the handle clockwise. |
| RATE (n) | A measurement of how frequently or how quickly something occurs | MAKE SURE THAT THE FLOW RATE IS CORRECT. |  |

<!-- Page 341 of 434 -->

|---|---|---|---|
| re- (prefix) — UNNAPPROVED | In general, use the word AGAIN (adv) or BACK (adv) with the basic word to replace words that have "re-" as a prefix. |  |  |
| reach (v) — UNNAPPROVED | GET (v) TOUCH (v) BE (v) | WHEN YOU GET THE CORRECT PRESSURE, CLOSE THE VALVE. MAKE SURE THAT THE EXTENSION BAR TOUCHES THE TARGET PLATE. WHEN THE FLAPS ARE AT THE 30 DEGREE POSITION, INSTALL THE RIGGING PIN. | When the correct pressure is reached, close the valve. Make sure that the extension bar reaches the target plate. When the flaps reach the 30 degree position, install the rigging pin. |
| reactivate (v) — UNNAPPROVED | ACTIVATE (v) | ACTIVATE THE MODE AGAIN. | Reactivate the mode. |
| READ (v), READS, READ, READ | To come to know information with the eyes or electronically | READ THE INDICATORS ON THE CONTROL PANEL. |  |
| reading (n) — UNNAPPROVED | INDICATION (n) | MAKE SURE THAT THE EXHAUST FROM THE GROUND CART DOES NOT CAUSE AN INCORRECT INDICATION. | Avoid an erroneous reading caused by exhaust from ground cart. |
| readjust (v) — UNNAPPROVED | ADJUST (v) | AFTER THE INSPECTION, ADJUST THE LINKAGE AGAIN. | Readjust the linkage after the inspection. |
| ready (adj) — UNNAPPROVED | PREPARE (v) | MAKE SURE THAT THE CONTROL SYSTEM IS PREPARED FOR OPERATION. | Make sure that the control system is in an operational ready state. |
| ready (v) — UNNAPPROVED | PREPARE (v) | PREPARE THE REMOVAL KIT FOR THE REMOVAL OF THE STRUT. | Ready the removal kit for the removal of the strut. |

<!-- Page 342 of 434 -->

|---|---|---|---|
| real (adj) — UNNAPPROVED | AGREE (v) | MAKE SURE THAT THE INDICATION ON THE GAUGE AGREES WITH THE QUANTITY OF FUEL THAT IS IN THE TANK. | Make sure that the gauge shows the real quantity of fuel that is in the tank. |
| REAR (adj) | Away from the person who looks or from a reference point | INSTALL THE TWO BOLTS IN THE REAR FITTINGS. |  |
| REAR (n) | The rear part or rear surface | THE CIRCUIT BREAKERS ARE INSTALLED ON THE REAR OF THE UNIT. |  |
| rear of (prep) — UNNAPPROVED | AFT OF BEHIND (prep) | THE PUMP IS INSTALLED ON RIB 3, AFT OF THE FRONT SPAR. THE PUMP IS INSTALLED ON RIB 3, BEHIND THE FRONT SPAR. | The pump is located on rib 3, rear of the front spar. The pump is located on rib 3, rear of the front spar. |
| rearmost (adj) — UNNAPPROVED | REAR (n) | YOU CANNOT REMOVE THE HALF CLAMP NEAREST TO THE REAR. | The rearmost half clamp is not removable. |
| REARWARD (adv) | In the direction of the rear | PULL THE LEVER REARWARD. |  |
| reason (n) — UNNAPPROVED | CAUSE (n) BECAUSE OF (prep) | FIND THE CAUSE OF THE INCORRECT INDICATION. BECAUSE OF THE POSSIBLE EFFECTS ON YOUR HEALTH, USE ONLY POTABLE WATER. | Find the reason for the wrong indication. For health reasons, only use potable water. |
| reassemble (v) — UNNAPPROVED | ASSEMBLE (v) | ASSEMBLE THE ACTUATOR AGAIN. | Reassemble the actuator. |
| rebuild (v) — UNNAPPROVED | ASSEMBLE (v) | ASSEMBLE THE UNIT AGAIN. | Rebuild the unit. |

<!-- Page 343 of 434 -->

|---|---|---|---|
| RECEIVE (v), RECEIVES, RECEIVED, RECEIVED | To get energy, material, or a signal from a different source | MAKE SURE THAT THE CAPTAIN'S BOOMSET RECEIVES THE SIGNALS CORRECTLY. |  |
| RECESS (n) | An indentation in a surface | WHEN YOU CLEAN THE SURFACES, REMOVE THE STAINS FROM THE RECESSES. |  |
| recess (v) — UNNAPPROVED | RECESS (n) | DO NOT MAKE A RECESS OF MORE THAN 5 mm FOR THE STUDS. THE FLANGE IS IN A RECESS IN THE FUSELAGE. | Do not recess studs more than 5 mm. The flange is recessed into the fuselage. |
| recharge (v) — UNNAPPROVED | CHARGE (v) FILL (v) PRESSURIZE (v) | CHARGE THE BATTERY AGAIN. FILL THE FLUID RESERVOIR. PRESSURIZE THE ACCUMULATOR. | Recharge the battery. Recharge the fluid reservoir. Recharge the accumulator. |
| recheck (v) — UNNAPPROVED | MEASURE (v) EXAMINE (v) CHECK (n) | MEASURE THE DISTANCE BETWEEN THE FACES AGAIN. EXAMINE THE CASTING FOR CORROSION AGAIN. DO A LEAKAGE CHECK OF THE FILTER ASSEMBLY AGAIN. | Recheck the distance between the faces. Recheck the casting for corrosion. Recheck the filter assembly for leakage. |
| reclaim (v) — UNNAPPROVED | REPAIR (v) | REPAIR THE DAMAGED FABRIC AREA. | Reclaim the damaged fabric area. |
| recleat (v) — UNNAPPROVED | ATTACH (v) (TO A CLEAT [TN]) | ATTACH THE TIEDOWN CORD TO A CLEAT. | Recleat the tiedown cord. |
| reclose (v) — UNNAPPROVED | CLOSE (v) | AFTER SERVICING, CLOSE THE COMPARTMENT AGAIN. | Reclose the compartment after servicing. |

<!-- Page 344 of 434 -->

|---|---|---|---|
| recoil (v) — UNNAPPROVED | MOVE BACK WIND (v) RECOIL (TN) | BE CAREFUL WHEN THE SLIDE MOVES BACK. WIND THE PROBE WIRE BACK ON THE SPOOL. THE GUN BARREL HAS A QUICK RECOIL. | Be careful when the slide recoils. Recoil the probe wire back on the spool. The gun barrel recoils quickly. |
| RECOMMEND (v), RECOMMENDS, RECOMMENDED, RECOMMENDED | To advise that which is best | THE MANUFACTURER RECOMMENDS THAT YOU KEEP THE UNIT IN A DEDICATED AREA. |  |
| recondition (v) — UNNAPPROVED | REPAIR (v) OVERHAUL (TN) | REPAIR THE SEATS. DO AN OVERHAUL OF THE ENGINE. | Recondition the seats. Recondition the engine. |
| reconstruction (n) — UNNAPPROVED | REPAIR (n) REPAIR (v) | RECORD ALL REPAIRS TO THE SKIN SURFACE. THIS PROCEDURE TELLS YOU HOW TO REPAIR THE SURFACE. | Record all reconstruction of the skin surface. This procedure is for the reconstruction of the surface. |
| RECORD (v), RECORDS, RECORDED, RECORDED | 1. To make notes of and keep data to use subsequently 2. To put data on a storage medium | RECORD THE RESULTS. THE COCKPIT VOICE RECORDER RECORDS SIGNALS FROM FOUR AUDIO INPUTS DURING THE FLIGHT. |  |
| recover (v) — UNNAPPROVED | COLLECT (v) | REMOVE THE NUT AND THE BOLT. THEN, COLLECT THE WASHER. | Remove the nut and the bolt. Then, recover the washer. |
| rectify (v) — UNNAPPROVED | CORRECT (v) | BEFORE YOU START THE PROCEDURE AGAIN, CORRECT THE DEFECT. | Rectify the defect before you restart the procedure. |
| recur (v) — UNNAPPROVED | OCCUR (v) | IF THE SYMPTOMS OCCUR AGAIN, DO A SYSTEM TEST. | If the symptoms recur, do a system test. |

<!-- Page 345 of 434 -->

|---|---|---|---|
| RECYCLE (v), RECYCLES, RECYCLED, RECYCLED | To put a used material through a process to make it possible to use it or its components again For other meanings, use: CYCLE (n) | MAKE SURE THAT YOU RECYCLE THE REMOVED INSULATION MATERIAL. DO ONE MORE TEST CYCLE OF THE COMPONENT. | Recycle the component through a test. |
| reduce (v) — UNNAPPROVED | DECREASE (v) | SLOWLY DECREASE THE SPEED. | Slowly reduce the speed. |
| REFER (v), REFERS, REFERRED, REFERRED | 1. To tell a person where to find information 2. To give information | REFER TO CHAPTER 28 FOR THE INSTALLATION PROCEDURE. BEFORE YOU DO THIS PROCEDURE, ENGAGE THE RAMP SERVICE DOOR SAFETY CONNECTOR PIN (THE PIN THAT: HOLDS THE RAMP SERVICE DOOR, REFER TO IN THIS PROCEDURE AS THE “SAFETY CONNECTOR PIN”). |  |
| reference (n) — UNNAPPROVED | REFER (v) | REFER TO CHAPTER 20 FOR THE STANDARD TORQUE VALUES. | Reference is made to Chapter 20 for the standard torque values. |
| referenced (adj) — UNNAPPROVED | SHOW (v) | MAKE SURE THAT THE GRAPH SHOWS THIS POINT. | Make sure that this point is referenced on the graph. |
| refill (v) — UNNAPPROVED | FILL (v) | FILL THE CONTAINER AGAIN. | Refill the container. |
| refit (v) — UNNAPPROVED | INSTALL (v) | INSTALL THE LINKAGE AGAIN. | Refit the linkage. |
| REPAIR (v) | ON THE SUBMARINE, REPAIR ALL DAMAGE AND REPLACE ALL WORN PARTS. | Refit the submarine. |  |

<!-- Page 346 of 434 -->

|---|---|---|---|
| reflect (v) — UNNAPPROVED | REFLECTION (n) | THE RETICLE IMAGE MAKES A REFLECTION ON THE BOTTOM SURFACE OF THE GLASS. | The reticle image reflects on the bottom surface of the glass. |
| REFLECTION (n) | Something that occurs when energy comes against a surface which sends it back | A CLEAN SURFACE GIVES A BETTER REFLECTION. |  |
| REFUEL (v), REFUELS, REFUELED, REFUELED | To supply with fuel | REFUEL THE VEHICLE. |  |
| register (v) — UNNAPPROVED | SHOW (v) | ADJUST THE “SET +40” CONTROL UNTIL THE POINTER SHOWS +40. | Adjust the “SET +40” control until the pointer registers +40. |
| regrease (v) — UNNAPPROVED | APPLY (v) MORE (adj) | APPLY GREASE TO THE ROD AGAIN. PUT MORE GREASE ON THE JOINT UNTIL YOU CAN MOVE IT. | Regrease the rod. Regrease the joint until you can move it. |
| REGULAR (adj) | At specified or equal intervals | THE COMPUTER GIVES REGULAR INPUTS TO THE CONTROL SYSTEM. |  |
| REGULARLY (adv) | In a regular manner | IF THE FAILURE OCCURS REGULARLY, DO A SYSTEM TEST. |  |
| regulate (v) — UNNAPPROVED | CONTROL (v) ADJUST (v) | CONTROL THE ELECTRICAL CURRENT. ADJUST THE TIRE PRESSURE AS NECESSARY. | Regulate the electrical current. Regulate the tire pressure as necessary. |

<!-- Page 347 of 434 -->

|---|---|---|---|
| regulation (n) — UNNAPPROVED | ADJUSTMENT (n) CONTROL (n) CONTROL (v) | THE TEMPERATURE ADJUSTMENT IS AUTOMATIC. THE TEMPERATURE CONTROL IS AUTOMATIC. A SENSOR CONTROLS THE TEMPERATURE IN THE COMPARTMENT. | The regulation of temperature is automatic. The regulation of temperature is automatic. The regulation of temperature in the compartment is effected by a sensor. |
| reinflate (v) — UNNAPPROVED | INFLATE (v) | INFLATE THE TIRE AGAIN. | Reinflate the tire. |
| reinforce (v) — UNNAPPROVED | MAKE … STRONGER | DOUBLERS MAKE THE JOINT STRONGER. | Doublers reinforce the joint. |
| reinstall (v) — UNNAPPROVED | INSTALL (v) | AFTER YOU ADJUST THE UNIT, INSTALL THE COVER AGAIN. | Reinstall the cover after you adjust the unit. |
| reinstallation (n) — UNNAPPROVED | INSTALLATION (n) | ONLY APPROVED PERSONNEL Can DO THE INSTALLATION PROCEDURE. | This reinstallation must be performed by qualified personnel. |
| REJECT (v), REJECTS, REJECTED, REJECTED | To make a decision that something is unsatisfactory | REJECT THE PARTS THAT ARE DAMAGED. |  |
| rejection (n) — UNNAPPROVED | REJECT (v) | IF THE TEST IS NOT SATISFACTORY, REJECT THE COMPONENT. | Rejection is mandatory if the test proves the component to be defective. |
| relate (v) — UNNAPPROVED | RELATED (adj) | THE PROCEDURES ARE RELATED TO THE SYSTEM TEST. | The procedures relate to the system test. |
| RELATED (adj) | That has a relation | CLEAN THE BALLS OF THE ELECTRICAL LATCH AND ITS RELATED SOCKETS. |  |
| RELATION (n) | The connection between two or more things caused by their functions, values, or conditions | THE RELATION BETWEEN THE TWO CONTROL SYSTEMS KEEPS THE AIRCRAFT STABLE. |  |

<!-- Page 348 of 434 -->

|---|---|---|---|
| relay (v) — UNNAPPROVED | SEND (v) | SEND THE INFORMATION TO THE ENGINEERING DEPARTMENT. | Relay the information to the engineering department. |
| RELEASE (v), RELEASES, RELEASED, RELEASED | To make free, to let go | RELEASE THE INSTRUMENT PANEL TO GET ACCESS TO THE CONNECTIONS. |  |
| relevant (adj) — UNNAPPROVED | RELATED (adj) THEIR (adj) ITS (adj) | REMOVE THE ROD END FROM THE RELATED PIVOT. INSTALL THE BOLTS IN THEIR HOLES. INSTALL THE COMPUTER IN ITS RACK. | Withdraw the rod end from the relevant pivot. Install the bolts in the relevant holes. Install the computer in the relevant rack. |
| relieve (v) — UNNAPPROVED | RELEASE (v) | RELEASE THE TENSION IN THE CABLE. | Relieve the tension in the cable. |
| remain (v) — UNNAPPROVED | STAY (v) | THE FLAGS MUST STAY OUT OF VIEW. | The flags must remain out of view. |
| REMAINING (adj) | That continues to stay | REMOVE THE REMAINING SEALANT WITH SOLVENT. |  |
| remnant (n) — UNNAPPROVED | REMAINING (adj) | REMOVE THE REMAINING SEALANT FROM THE FLOOR COVERING. | Remove sealant remnants from the floor covering. |
| removable (adj) — UNNAPPROVED | REMOVE (v) | FIND THE PART OF THE BARREL THAT YOU CAN REMOVE. | Find the removable part of the barrel. |
| REMOVAL (n) | A procedure which removes an object | THE SUPERVISOR MUST GIVE THE APPLICABLE PROCEDURE FOR CORROSION REMOVAL. |  |
| REMOVE (v), REMOVES, REMOVED, REMOVED | To take or move something away from its initial position | REMOVE THE INDICATOR FROM THE PANEL. |  |
| render (v) — UNNAPPROVED | MAKE (v) | MAKE THE SYSTEM ELECTRICALLY SAFE. | Render the system electrically safe. |

<!-- Page 349 of 434 -->

|---|---|---|---|
| renew (v) — UNNAPPROVED | NEW (adj) | USE NEW ADHESIVE TAPE. | Renew the adhesive tape. |
| renovate (v) — UNNAPPROVED | REPAIR (v) NEW (adj) | REPAIR ALL WORN SURFACES. IF THE PAINT ON THE CONTROL BOX IS DAMAGED, APPLY NEW PAINT. | Renovate all worn surfaces. Renovate any damaged paint on the control box. |
| repack (v) — UNNAPPROVED | PUT (v) FILL (v) | PUT THE ASSEMBLY BACK IN THE BOX. FILL THE HOLE WITH GREASE AGAIN. | Repack the assembly in the box. Repack the hole with grease. |
| repaint (v) — UNNAPPROVED | PAINT (v) | PAINT ALL THE SURFACES AGAIN. | Repaint all the surfaces. |
| REPAIR (n) | The act of repairing or the result when something is repaired | AFTER THE REPAIR, APPLY A PROTECTIVE LAYER OF GREASE TO ALL EXTERNAL SURFACES. |  |
| REPAIR (v), REPAIRS, REPAIRED, REPAIRED | To make an item serviceable | REPAIR THE DEFECTIVE WIRING. |  |
| repairable (adj) — UNNAPPROVED | REPAIR (v) | IT IS POSSIBLE TO REPAIR THIS DAMAGE. | This damage is repairable. |
| repeat (v) — UNNAPPROVED | AGAIN (adv) | DO STEPS (10) THRU (14) AGAIN. | Repeat steps (10) to (14). |
| repeated (adj) — UNNAPPROVED | AGAIN AND AGAIN | IF YOU HEAR SIGNALS AGAIN AND AGAIN, DO A CHECK OF THE "AP ENGAGE" BUTTON ON THE FLIGHT MODE PANEL. | If repeated signals are heard, check the AP ENGAGE button on the flight mode panel. |
| repeatedly (adv) — UNNAPPROVED | AGAIN AND AGAIN | IF THE VOLTAGE DECREASES AGAIN AND AGAIN, ADJUST THE VOLTAGE REGULATOR. | If voltage drops repeatedly, adjust the voltage regulator. |

<!-- Page 350 of 434 -->

|---|---|---|---|
| REPLACE (v), REPLACES, REPLACED, REPLACED | To remove an item and to install a new or serviceable item of the same type | REPLACE THE RELAY. |  |
| REPLACEMENT (n) | The item you install when you replace an item | MAKE SURE THAT THE REPLACEMENT HAS THE CORRECT DIMENSIONS. |  |
| replenish (v) — UNNAPPROVED | FILL (v) ADD (v) REFUEL (v) | FILL THE ACCUMULATOR WITH OIL. ADD OIL TO THE ACCUMULATOR. REFUEL THE VEHICLE. | Replenish the accumulator with oil. Replenish the oil in the accumulator. Replenish the vehicle with fuel. |
| REPORT (n) | The information that is recorded about a subject or occurrence | IF THERE IS A REPORT OF DAMAGE, DO AN ACCURATE INSPECTION. |  |
| reposition (v) — UNNAPPROVED | MOVE (v) PUT (v) SET (v) | MOVE THE LEVER BACK TO ITS INITIAL POSITION. PUT THE LEVER BACK TO ITS INITIAL POSITION. SET THE SWITCH BACK TO THE OFF POSITION. | Reposition the lever. Reposition the lever. Reposition the switch to OFF. |
| represent (v) — UNNAPPROVED | SHOW (v) | THE SUCTION SHOWS AS AN ALTIMETER INDICATION. | The suction is represented by an altimeter reading. |
| repressurize (v) — UNNAPPROVED | PRESSURIZE (v) | PRESSURIZE THE TANK AGAIN. | Repressurize the tank. |
| request (n) — UNNAPPROVED | TELL (v) WRITE (v) | TELL THE FIRE SERVICE TO HELP YOU. IF AID IS NECESSARY, WRITE TO THE MANUFACTURER. | Make a request for external fire support. Any request for assistance should be addressed to the manufacturer. |

<!-- Page 351 of 434 -->

|---|---|---|---|
| request (v) — UNNAPPROVED | TELL (v) WRITE (v) | TELL THE FIRE SERVICE TO HELP YOU. WRITE TO THE MANUFACTURER FOR REPAIR INSTRUCTIONS. | Request external fire support. Request repair instructions from the manufacturer. |
| require (v) — UNNAPPROVED | NECESSARY (adj) | DURING THIS PROCEDURE, CLEAN FILTERS ARE NECESSARY. | During this procedure, clean filters are required. |
| reseal (v) — UNNAPPROVED | SEAL (v) | SEAL THE CONTAINER AGAIN. | Reseal the container. |
| reset (v) — UNNAPPROVED | SET (v) | SET THE INDICATOR TO A NEW POSITION. | Reset the indicator to a new position. |
| residual (adj) — UNNAPPROVED | REMAINING (adj) | REMOVE ALL THE REMAINING GREASE. | Remove all residual grease. |
| residue (n) — UNNAPPROVED | REMAINING (adj) | REMOVE THE REMAINING GREASE. | Remove the grease residues. |
| RESISTANT (adj) | That will help to prevent something | THE MATERIAL OF THE SEATS IS RESISTANT TO FIRE. |  |
| respective (adj) — UNNAPPROVED | RELATED (adj) CORRECT (adj) | ATTACH THE CABLES TO THEIR RELATED SHACKLES. INSTALL THE BOLTS IN THEIR CORRECT POSITIONS. | Attach the cables to their respective shackles. Install the bolts in their respective positions. |
| respectively (adv) — UNNAPPROVED | RELATED (adj) | ENGINES 1 AND 2 SUPPLY HOT AIR TO THEIR RELATED WINGS. | Engines 1 and 2 supply the left and right wings respectively with hot air. |
| respond (v) — UNNAPPROVED | RESULT (n) | IF THE INSTRUMENT DOES NOT GIVE A RESULT, DO A TEST. | If the instrument fails to respond, do a test. |
| rest (n) — UNNAPPROVED | REMAINING (adj) | THE REMAINING INSTRUCTIONS ARE APPLICABLE ONLY TO APPROVED PERSONNEL. | The rest of these instructions only apply to approved personnel. |

<!-- Page 352 of 434 -->

|---|---|---|---|
| rest (v) — UNNAPPROVED | BE (v) PUT (v) | THE VEHICLE MUST BE ON ITS WHEELS. PUT THE REMOVED PART ON A CLEAN SURFACE. | The vehicle must rest on its wheels. Rest the removed part on a clean surface. |
| restart (v) — UNNAPPROVED | START (v) | START THE UNIT AGAIN. | Restart the unit. |
| restore (v) — UNNAPPROVED | REPAIR (v) PUT (v) | DO NOT REPAIR THE CHROMIC ACID ANODIZING ON THE SKIN PANEL. PUT THE PINS BACK IN THEIR LOCATION. | Do not restore the chromic acid anodizing on the skin panel. Restore the pins to their location. |
| restrain (v) — UNNAPPROVED | HOLD (v) STOP (v) PREVENT (v) LIMIT (n) | HOLD THE HOSES IN POSITION. STOP THE FLUID FLOW. THE STOP PREVENTS THE MOVEMENT OF THE ROD. THE VALVE KEEPS THE AIRFLOW IN LIMITS. | Restrain the hoses in position. Restrain all fluid flow. The stop restrains the movement of the rod. The valve restrains the airflow. |
| restrict (v) — UNNAPPROVED | DECREASE (v) PREVENT (v) ONLY (adv) LIMIT (n) | THE METERING PLUG DECREASES THE FUEL FLOW. THE STOP PREVENTS THE MOVEMENT OF THE ROD. USE THESE NUTS ONLY FOR THE TEST. THE VALVE KEEPS THE AIRFLOW IN LIMITS. | The metering plug restricts the fuel flow. The stop restricts the movement of the rod. Restrict the use of these nuts to test only. The valve restricts the airflow. |
| RESULT (n) | Something that occurs when you do something | IF THESE TESTS DO NOT GIVE THE CORRECT RESULTS, REPLACE THE UNIT. |  |

<!-- Page 353 of 434 -->

|---|---|---|---|
| result (v) — UNNAPPROVED | CAUSE (v) RESULT (n) | AN INCORRECT CONNECTION WILL CAUSE DAMAGE. REPAIR DAMAGE THAT IS THE RESULT OF CORROSION. | An incorrect connection will result in damage. Repair any damage resulting from corrosion. |
| resume (v) — UNNAPPROVED | START (v) CONTINUE (v) | INCREASE THE PRESSURE UNTIL THE FLOW STARTS AGAIN. CONTINUE THE TEST. | Increase the pressure until the flow resumes. Resume the test. |
| retain (v) — UNNAPPROVED | KEEP (v) | KEEP THE PLUG. | Retain the plug. |
| retorque (v) — UNNAPPROVED | TORQUE (v) | TORQUE THE FITTING AGAIN. | Retorque the fitting. |
| retouch (v) — UNNAPPROVED | APPLY (v) PAINT (v) | APPLY ENAMEL ON THE AREAS WHERE IT IS MISSING. PAINT THE DAMAGED LETTERS ON THE LABEL. | Retouch the missing enamel areas. Retouch the damaged label letters. |
| RETRACT (v), RETRACTS, RETRACTED, RETRACTED | 1. To pull in(to) 2. To move in(to) | RETRACT THE LANDING GEAR. THE NOSE LANDING GEAR RETRACTS INTO THE FUSELAGE. |  |
| retractable (adj) — UNNAPPROVED | RETRACT (v) | THE AIRCRAFT HAS A LANDING GEAR THAT RETRACTS. | The aircraft has a retractable landing gear. |
| RETRACTION (n) | The result when something retracts | DURING THE RETRACTION SEQUENCE, MAKE SURE THAT THE LANDING GEAR DOORS CLOSE. |  |
| return (n) — UNNAPPROVED | GO (v) | AFTER THE AILERONS GO BACK TO NEUTRAL, MAKE SURE THAT THEY ARE FLUSH WITH THE FLAPS. After the AILERONS GO BACK TO NEUTRAL, MAKE SURE THAT THEY ARE FLUSH WITH THE FLAPS. | After the return of the ailerons to neutral, check that they are flush with the flaps. |

<!-- Page 354 of 434 -->

|---|---|---|---|
| return (v) — UNNAPPROVED | GO (v) | THE PLUNGERS MUST GO BACK TO THE CLOSED POSITION. | Plungers must return to the closed position. |
| reusable (adj) — UNNAPPROVED | USE (v) | YOU CAN USE THE MIXTURE AGAIN. | The mixture is reusable. |
| reuse (v) — UNNAPPROVED | USE (v) | IF THE FABRIC IS NOT DAMAGED, USE IT AGAIN. | Reuse the fabric if it is not damaged. |
| reveal (v) — UNNAPPROVED | SHOW (v) | IF THE FUEL SAMPLE SHOWS FREE WATER, DRAIN THE SYSTEM. | If the fuel sample reveals free water, drain the system. |
| reverse (adj) — UNNAPPROVED | OPPOSITE (adj) This word is part of a technical noun when it refers to rearward thrust. | MOVE THE CONTROL IN THE OPPOSITE DIRECTION. MANUALLY TURN THE PROPELLER BLADES TO THE FULL REVERSE POSITION. | Move the control in the reverse direction. |
| reverse (v) — UNNAPPROVED | OPPOSITE (adj) | MOVE THE ROD IN THE OPPOSITE DIRECTION. | Reverse the movement of the rod. |
| review (n) — UNNAPPROVED | INSPECTION (n) EXAMINE (v) | DO AN INSPECTION OF THE DAMAGED AREA. EXAMINE THE DAMAGED AREA. | Do a review of the damaged area. Do a review of the damaged area. |
| rewind (v) — UNNAPPROVED | WIND (v) | WIND THE CABLE BACK ONTO ITS REEL. | Rewind the cable onto its reel. |
| rework (v) — UNNAPPROVED | Refer to technical verbs, manufacturing processes. | EXAMINE FOR SCRATCHES. THEN, LIGHTLY POLISH ALL DAMAGED AREAS. | Examine for scratches and rework all damaged areas. |
| rig (v) — UNNAPPROVED | ADJUST (v) | ADJUST THE SYSTEM. | Rig the system. |
| RIGHT (adj) | On the east side when you look north | DO A FLOW CHECK OF THE PUMP IN THE RIGHT WING TANK. |  |
| right-hand (adj) — UNNAPPROVED | RIGHT (adj) | THE FUEL CONNECTOR IS IN THE RIGHT WING. | The fuel connector is in the right-hand wing. |
| RIGID (adj) | That cannot easily bend or change shape | REMOVE THE SCREWS FROM THE RIGID COVER. |  |

<!-- Page 355 of 434 -->

|---|---|---|---|
| rinse (v) — UNNAPPROVED | FLUSH (v) REMOVE (v) CLEAN (v) | FLUSH THE FILTER WITH HOT WATER. REMOVE THE CLEANING AGENT FROM THE SURFACE. CLEAN THE WINDOW PANE WITH A LARGE QUANTITY OF WATER. | Rinse the filter in hot running water. Rinse the cleaning agent from the surface. Rinse the window pane with a large quantity of water. |
| ripped (adj) — UNNAPPROVED | DAMAGED (adj) | IF THE SEAT COVER IS DAMAGED, REPLACE IT. | If the seat cover is ripped, replace it. |
| rise (n) — UNNAPPROVED | INCREASE (v) | WHEN A FIRE STARTS, THE TEMPERATURE INCREASES AND CAUSES THE DETECTOR TO OPERATE. | When a fire starts, the temperature rise causes the detector to operate. |
| rise (v) — UNNAPPROVED | INCREASE (v) | FILL THE STRUT WITH FLUID UNTIL THE PRESSURE INCREASES. | Fill the strut with fuel until the pressure rises. |
| RISK (n) | The possibility that something that is dangerous occurs | OBEY THE PRECAUTIONS TO PREVENT THE RISK OF FIRE. |  |
| rope off (v) — UNNAPPROVED | ROPE (TN) | PUT ROPES AROUND THE AREA. | Rope off the area. |
| rotary (adj) — UNNAPPROVED | TURN (v) | TURN THE GEARS TO ALIGN THEM. | Use a rotary movement to align the gears. |
| rotate (v) — UNNAPPROVED | TURN (v) | SLOWLY TURN THE VANE. | Slowly rotate the vane. |
| rotation (n) — UNNAPPROVED | TURN (v) | MAKE SURE THAT THE FAN TURNS FREELY. | Ensure the free rotation of the fan. |
| rotational (adj) — UNNAPPROVED | TURN (v) | TURN THE GEARS TO ALIGN THEM. | Use a rotational movement to align the gears. |
| ROUGH (adj) (ROUGHER, ROUGHEST) | Not smooth | CLEAN THE ROUGH SURFACES CAREFULLY. |  |
| roughen (v) — UNNAPPROVED | ROUGH (adj) | MAKE THE FAYING SURFACES ROUGH. | Roughen the faying surfaces. |

<!-- Page 356 of 434 -->

|---|---|---|---|
| roughness (n) — UNNAPPROVED | ROUGH (adj) | MAKE SURE THAT THE AREA OF THE BOND IS SUFFICIENTLY ROUGH. | Make sure the area of the bond has sufficient roughness. |
| round (adj) — UNNAPPROVED | CIRCULAR (adj) | REPAIR THE DAMAGE WITH A CIRCULAR PATCH. | Repair the damage with a round patch. |
| ROUNDED (adj) | Not angular | WHEN YOU INSTALL THE PART, MAKE SURE THAT THE ROUNDED EDGE IS AGAINST THE STRUCTURE. |  |
| route (n) — UNNAPPROVED | ROUTING (n) | MAKE SURE THAT YOU DO NOT CHANGE THE WIRE ROUTING. | Make sure you do not change the wire routes. |
| route (v) — UNNAPPROVED | PUT (v) ROUTING (n) | PUT THE FUELING HOSE ALONG THE GROUND. MAKE SURE THAT THE ROUTING OF THE WIRE IS CORRECT. | Route the fueling hose along the ground. Make sure that the wiring is correctly routed. |
| routine (adj) — UNNAPPROVED | USUAL (adj) | IF SUCH FAILURES BECOME USUAL, REPLACE THE UNIT. | If such failures become routine, replace the unit. |
| ROUTING (n) | The specified direction that cables, pipes, wires, and other parts of a system must go along | DO NOT CHANGE THE ROUTING OF THE PIPE. |  |
| ROW (n) | A number of objects in a line | THE PANELS ARE INSTALLED IN ROWS. |  |
| RUB (v), RUBS, RUBBED, RUBBED | To move or cause something to move with pressure and friction along a surface | RUB THE SURFACE WITH A CLEAN CLOTH. MAKE SURE THAT THE COILS OF THE OXYGEN HOSE DO NOT RUB TOGETHER. |  |
| run (v) — UNNAPPROVED | OPERATE (v) | OPERATE THE ENGINE AT 100% THRUST. | Run the engine at 100% thrust. |
| running (adj) — UNNAPPROVED | FLUSH (v) | FLUSH THE PIPES WITH WATER. | Clean the pipes with running water. |

<!-- Page 357 of 434 -->
Blank Page
