<!-- section: DICT_G-P | pages: 293-296 | verified: true -->

# Page 293 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **KEEP (v)** | , To continue to have or KEEP THE KEEPS, hold COMPOUND IN A KEPT, CLOSED CONTAINER. KEPT |
| **key (v) — UNNAPROVED** | REFER (v) THE ILLUSTRATION The illustration will be REFERS TO EACH keyed to each of the STEP. steps. KEY (TN) INSTALL THE KEY The pulley must be BETWEEN THE keyed to the shaft. PULLEY AND THE SHAFT. |
| **KILL (v)** | , To cause death HIGH VOLTAGES CAN KILLS, KILL YOU. KILLED, KILLED |
| **kind (n) — UNNAPROVED** | TYPE (n) YOU CAN USE TWO Two kinds of sealing TYPES OF SEALING compound can be used. COMPOUND. |
| **kink (v) — UNNAPROVED** | KINK (TN) DO NOT MAKE KINKS Do not kink the cables. IN THE CABLES. |
| **knock (v) — UNNAPROVED** | HIT (v) HIT THE CLAMP ON Knock the clamp on the THE RIGHT SIDE WITH right side with a A HAMMER. hammer. |
| **KNOW (v)** | , To be sure of data, to IF YOU KNOW THE KNOWS, have data ready to use CLEARANCE, YOU KNEW, CAN CALCULATE THE KNOWN THICKNESS OF THE WASHER. |

# Page 294 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example
Blank Page
Page 2-1-K2 Part 2 - Dictionary Issue 9
2025-01-15

# Page 295 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **label (v) — UNNAPROVED** | IDENTIFY (v) IDENTIFY THE Label the component COMPONENT WITH A with a code to help you CODE TO HELP YOU install it again correctly. INSTALL IT AGAIN CORRECTLY. LABEL (TN) PUT A LABEL ON THE Label the relay RELAY ASSEMBLY. assembly. |
| **lack (n) — UNNAPROVED** | NOT SUFFICIENT DAMAGE CAN OCCUR Damage can occur to TO THE PUMP IF the pump if there is a THERE IS NOT lack of oil in the SUFFICIENT OIL IN reservoir. THE RESERVOIR. |
| **LAMINATED (adj)** | Made of laminations THIS PANEL IS MADE OF LAMINATED CARBON FIBER. |
| **LAMINATION (n)** | Layers of one or more IF THE LAMINATION IS materials bonded DAMAGED, REPLACE together THE PANEL. |
| **land (v) — UNNAPROVED** | LANDING (TN) AFTER A HEAVY If the aircraft landed LANDING, DO THE heavily, do the Heavy HEAVY LANDING Landing Inspection. INSPECTION. |
| **LARGE (adj)** | More than average in CLEAN YOUR SKIN (LARGER, dimension, quantity, or WITH A LARGE LARGEST) capacity QUANTITY OF CLEAN WATER. |
| **LAST (adj)** | That comes at the end IMMEDIATELY AFTER THE LAST FLIGHT OF THE DAY, INSTALL ALL COVERS. |
| **LAST (adv)** | After other persons or FILL THE OUTER things TANKS LAST. |
| **last (v) — UNNAPROVED** | CONTINUE (v) THE SIGNALS The signals last CONTINUE FOR 0.8 seconds. 0.8 SECONDS. |
| **LATCH (v)** | , To hold something in MAKE SURE THAT LATCHES, position with a latching YOU LATCH THE LATCHED, device DOOR CORRECTLY. LATCHED MAKE SURE THAT THE DOOR LATCHES CORRECTLY. |

# Page 296 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **later (adj) — UNNAPROVED** | SUBSEQUENT (adj) A SUBSEQUENT A later repair will be for REPAIR WILL BE FOR the new configuration. THE NEW CONFIGURATION. |
| **THEN (adv)** | DO THIS STEP FIRST. Do this step first. At a THEN, DISCONNECT later time, disconnect the THE CABLES. cables. |
| **later (adv) — UNNAPROVED** | SUBSEQUENTLY (adv) MAKE SURE THAT THE Make sure that the tool TOOL IS is available later for the SUBSEQUENTLY installation procedure. AVAILABLE FOR THE INSTALLATION PROCEDURE. |
| **WHEN (conj)** | DO STEPS (3) THRU Do steps (3) to (5). Do (5). DO STEP (6) WHEN step (6) later. THE AILERON If it is possible, MOVEMENT STOPS. give the condition or time. |
| **AFTER (prep)** | THE BAR MOVES The bar moves down DOWN AFTER 20 later. SECONDS. |
| **LATERAL (adj)** | Related to or on the side ADJUST THE LATERAL LEVEL. |
| **LATERALLY (adv)** | In a lateral direction PUSH THE UNIT OUT, AND THEN MOVE IT LATERALLY. |
| **lay (v) — UNNAPROVED** | PUT (v) PUT COVERS ON THE Lay covers on the floor. FLOOR. |
| **LAYER (n)** | A material applied to a APPLY A THIN LAYER surface or put on, or OF SEALING below, a second material COMPOUND ON THE BARE METAL. |
| **lead (v) — UNNAPROVED** | PUT (v) PUT THE TELEFLEX Lead the Teleflex cable CABLE THROUGH THE through the bulkhead. BULKHEAD. |
| **LEAK (n)** | A crack, gap or hole EXAMINE THE SWIVEL which lets fluid or light COUPLINGS FOR go into or come out of LEAKS. something |
