# Page 381 of 434

**Page 2-1-S23**

**Page 2-1-S23**

**Issue 9 2025-01-15**

**Part 2 - Dictionary**

**ASD-STE100 Simplified Technical English**

|**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
|---|---|---|---|
|**still (adv) — UNNAPPROVED**|STAY (v)|MAKE SURE THAT THE<BR>“OVHT” LIGHT STAYS<BR>ON.|<BR>Make sure that the<BR>“OVHT” light is still<BR>illuminated.|
|||CONTINUE (v)|MAKE SURE THAT THE<BR>ROTOR CONTINUES<BR>TO TURN.|<BR>Make sure that the rotor<BR>still turns.|
|**stimulate (v) — UNNAPPROVED**|INCREASE (v)|INCREASE THE<BR>AIRFLOW.|Stimulate the airflow.|
|**stir (v) — UNNAPPROVED**|MIX (v)|MIX THE BONDING<BR>MATERIAL WITH A<BR>SPATULA.|Stir the bonding material<BR>with a spatula.|
|**STOP (v),**<br>**STOPS,**<br>**STOPPED,**<br>**STOPPED**|1.<br>To cause the end<br>of a procedure,<br>movement, or an<br>operation|STOP THE ENGINE.||
|||2.<br>To come to an end|WHEN THE FLOW<BR>STOPS, REMOVE THE<BR>DRAIN HOSE.||
|**store (v) — UNNAPPROVED**|KEEP (v)|KEEP THE<BR>CARTRIDGES IN A<BR>SAFETY AREA.|Cartridges should be<BR>stored in a safety area.|
||CONTAIN (v)|THE FIRE<BR>EXTINGUISHER<BR>BOTTLES CONTAIN A<BR>DRY CHEMICAL<BR>POWDER AGENT.|The fire extinguisher<BR>bottles store a dry<BR>chemical powder agent.|
||STORAGE (TN)|WHEN YOU PUT THE<BR>UNIT INTO STORAGE,<BR>OBEY THE<br>APPLICABLE<BR>STORAGE<br>INSTRUCTIONS.|When you store the unit,<br>obey the applicable<br>storage instructions.|
|**STOW (v),**<br>**STOWS,**<br>**STOWED,**<br>**STOWED**|To move or cause to<br>move into a specified<br>position of storage.|STOW THE LIFE VEST<br>SAFELY BELOW THE<br>PASSENGER SEAT.||
|||MAKE SURE THAT THE<br>THRUST REVERSER<BR>STOWS WHEN YOU<br>PUSH THE QUADRANT<br>CONTROL FORWARD.||

# Page 382 of 434

**Page 2-1-S24**

**Page 2-1-S24**

**Part 2 - Dictionary**

**Issue 9 2025-01-15**

**ASD-STE100 Simplified Technical English**

|**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
|---|---|---|---|
|**STRAIGHT (adj)**<br>**(STRAIGHTER,**<br>**STRAIGHTEST)**|Without curves or bends|MAKE SURE THAT THE<br>STRAIGHT PART OF<br>THE RIGGING PIN IS<br>SMOOTH.||
|**straighten (v) — UNNAPPROVED**|STRAIGHT (adj)|DO NOT TRY TO MAKE<br>THE BENDS IN THE<br>CABLE STRAIGHT.|Do not try to straighten<br>the bends in the cable.|
|**strain (v) — UNNAPPROVED**|FILTER (TN)|BEFORE YOU USE<br>THE OIL, PUT IT<br>THROUGH A FILTER.|Strain the oil before use.|
||STRAIN (TN)|DO NOT PUT STRAIN<br>ON THE BELLOWS.|Do not strain bellows.|
|**strap (v) — UNNAPPROVED**|ATTACH (v)<br>(WITH STRAPS [TN])|ATTACH THE CABLES<br>TO THE STRUCTURE<br>WITH AN APPLICABLE<br>STRAP.|Strap the cables to the<br>structure.|
|**stress (v) — UNNAPPROVED**|FORCE (TN)|DO NOT PUT TOO<br>MUCH FORCE ON THE<br>DUCTING.|Do not stress the ducting<br>unnecessarily.|
|**strictly (adv) — UNNAPPROVED**|FULLY (adv)|FULLY OBEY THE<br>SAFETY<br>PRECAUTIONS.|Strictly obey the safety<br>precautions.|
|**strike (v) — UNNAPPROVED**|HIT (v)|MAKE SURE THAT THE<br>SLING DOES NOT HIT<br>THE SURFACE.|Make certain that the<br>sling does not strike the<br>surface.|
|**STRIP (n)**|A piece of material that<br>is long and thin, but not<br>wide|PUT A STRIP OF<br>ADHESIVE TAPE<br>ALONG THE<br>INSULATION BLANKET.||
|**strip (v) — UNNAPPROVED**|REMOVE (v)|REMOVE THE<br>INSULATION FROM<br>THE WIRE.|Strip the insulation from<br>the wire.|
|**STRIPE (n)**|A line on a surface which<br>is a different color|THE FLAG HAS RED<br>AND WHITE STRIPES.||
|**striped (adj) — UNNAPPROVED**|STRIPE (n)|THE FLAG HAS RED<br>AND WHITE STRIPES.|The flag is striped red<br>and white.|
|**stroke (n) — UNNAPPROVED**|TRAVEL (n)|TO BLEED THE<br>BRAKING SYSTEM,<br>OPERATE THE HAND<br>PUMP HANDLE<br>THROUGH ITS FULL<br>TRAVEL.|Bleed the braking<br>system by applying full<br>strokes to the hand<br>pump handle.|

# Page 383 of 434

**Page 2-1-S25**

**Page 2-1-S25**

**Issue 9 2025-01-15**

**Part 2 - Dictionary**

**ASD-STE100 Simplified Technical English**

|**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
|---|---|---|---|
|**STRONG (adj)**<br>**(STRONGER,**<br>**STRONGEST)**|With much strength,<br>power, or concentration|WHEN WINDS ARE<br>STRONG, MOOR THE<br>AIRCRAFT<br>CAREFULLY.||
|**STRUCTURAL**<br>**(adj)**|Related to the structure|THE CHASSIS IS A<br>STRUCTURAL<br>COMPONENT OF THE<br>VEHICLE.||
|**STRUCTURALLY**<br>**(adv)**|Related to the structure|THE LIST GIVES YOU<br>STRUCTURALLY<br>IMPORTANT ITEMS.||
|**STRUCTURE (n)**|1.<br>A construction|ATTACH THE WIRES<br>TO THE STRUCTURE.||
||2.<br>The arrangement of<br>something|THE INTRODUCTION<br>GIVES YOU THE<br>STRUCTURE OF THE<br>MAINTENANCE<br>MANUAL.||
|**SUBASSEMBLY**<br>**(n)**|An assembly that is a<br>part of a larger assembly|DO NOT CHANGE THE<br>POSITION OF THE<br>SUBASSEMBLIES.||
|**submerge (v) — UNNAPPROVED**|PUT (v)|PUT THE FILTER<br>ELEMENT FULLY INTO<br>THE FLUID.|Submerge the filter<br>element in the fluid.|
|**submit (v) — UNNAPPROVED**|SEND (v)|SEND THE METAL<br>PARTICLES TO A<br>LABORATORY FOR<br>ANALYSIS.|Submit the metal<br>particles to a laboratory<br>for analysis.|
|**SUBSEQUENT**<br>**(adj)**|Following in an<br>unspecified time or<br>sequence|A SUBSEQUENT<br>REPAIR WILL BE FOR<br>THE NEW<br>CONFIGURATION<br>ONLY.||
||Use NEXT (adj)<br>for the first<br>occurrence that<br>follows<br>immediately in<br>time or sequence.|DO THE NEXT<br>INSPECTION.|Do the immediately<br>subsequent inspection.|

# Page 384 of 434

**Page 2-1-S26**

**Page 2-1-S26**

**Part 2 - Dictionary**

**Issue 9 2025-01-15**

**ASD-STE100 Simplified Technical English**

|**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
|---|---|---|---|
|**SUBSEQUENTLY**<br>**(adv)**|After an unspecified time|MAKE SURE THAT THE<BR>TOOL IS<br>SUBSEQUENTLY<br>AVAILABLE FOR THE<br>INSTALLATION<br>PROCEDURE.||
||Use THEN (adv)<br>for an occurrence<br>that follows<br>immediately in<br>time or sequence.<br>|LIFT THE COVER.<br>THEN, PULL THE<BR>HANDLE.<br>|Lift the cover and<br>subsequently pull the<br>handle.<br>|
|**subsequent to**<br>**(prep)**|AFTER (conj)|AFTER YOU INSTALL<BR>THE COMPONENT,<br>REMOVE THE<BR>HANDLING TOOL.|Remove the handling<br>tool subsequent to the<br>installation of the<br>component.|
|**substance (n) — UNNAPPROVED**|MATERIAL (n)|THE PRIMER<br>CONTAINS A<br>MATERIAL THAT<br>PREVENTS<br>CORROSION.|The primer contains a<br>substance that prevents<br>corrosion.|
|**substitute (adj) — UNNAPPROVED**|EQUIVALENT (adj)|IF THE SPECIFIED<br>MATERIAL IS NOT<br>AVAILABLE, YOU CAN<br>USE AN EQUIVALENT<br>ONE.|A substitute material<br>may be used if the<br>specified one is not<br>available.|
||ALTERNATIVE (adj)|IF THIS SPECIAL TOOL<br>IS NOT AVAILABLE,<br>USE AN ALTERNATIVE<br>METHOD.|If this special tool is not<br>available, use a<br>substitute method.|
|**substitute (n) — UNNAPPROVED**|ALTERNATIVE (n)|YOU CAN USE<br>ALTERNATIVES FOR<br>THESE ITEMS.|Equivalent substitutes<br>may be used for these<br>items.|
|**substitute (v) — UNNAPPROVED**|REPLACE (v)|DO NOT REPLACE THE<br>SELF-LOCKING NUTS<BR>WITH PLAIN NUTS.|Do not substitute the<br>self-locking nuts with<br>plain nuts.|
|**SUBTRACT (v),**<br>**SUBTRACTS,**<br>**SUBTRACTED,**<br>**SUBTRACTED**|To take from a number<br>or quantity|SUBTRACT<br>COEFFICIENT “A”<br>FROM THE<br>INDICATION.||
