<!-- section: DICT_Q-Z | pages: 357-360 | verified: true -->

# Pages 357–360 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **relay (v) — UNNAPROVED** | SEND (v) SEND THE Relay the information to INFORMATION TO THE the engineering ENGINEERING department. DEPARTMENT. |
| **RELEASE (v)** | , To make free, to let go RELEASE THE RELEASES, INSTRUMENT PANEL RELEASED, TO GET ACCESS TO RELEASED THE CONNECTIONS. |
| **relevant (adj) — UNNAPROVED** | RELATED (adj) REMOVE THE ROD Withdraw the rod end END FROM THE from the relevant pivot. RELATED PIVOT. |
| **THEIR (adj)** | INSTALL THE BOLTS Install the bolts in the IN THEIR HOLES. relevant holes. |
| **ITS (adj)** | INSTALL THE Install the computer in COMPUTER IN ITS the relevant rack. RACK. |
| **relieve (v) — UNNAPROVED** | RELEASE (v) RELEASE THE Relieve the tension in TENSION IN THE the cable. CABLE. |
| **remain (v) — UNNAPROVED** | STAY (v) THE FLAGS MUST The flags must remain STAY OUT OF VIEW. out of view. |
| **REMAINING (adj)** | That continues to stay REMOVE THE REMAINING SEALANT WITH SOLVENT. |
| **remnant (n) — UNNAPROVED** | REMAINING (adj) REMOVE THE Remove sealant REMAINING SEALANT remnants from the floor FROM THE FLOOR covering. COVERING. |
| **removable (adj) — UNNAPROVED** | REMOVE (v) FIND THE PART OF Find the removable part THE BARREL THAT of the barrel. YOU CAN REMOVE. |
| **REMOVAL (n)** | A procedure which THE SUPERVISOR removes an object MUST GIVE THE APPLICABLE PROCEDURE FOR CORROSION REMOVAL. |
| **REMOVE (v)** | , To take or move REMOVE THE REMOVES, something away from its INDICATOR FROM THE REMOVED, initial position PANEL. REMOVED |
| **render (v) — UNNAPROVED** | MAKE (v) MAKE THE SYSTEM Render the system ELECTRICALLY SAFE. electrically safe. |
| **renew (v) — UNNAPROVED** | NEW (adj) USE NEW ADHESIVE Renew the adhesive TAPE. tape. |
| **renovate (v) — UNNAPROVED** | REPAIR (v) REPAIR ALL WORN Renovate all worn SURFACES. surfaces. |
| **NEW (adj)** | IF THE PAINT ON THE Renovate any damaged CONTROL BOX IS paint on the control box. DAMAGED, APPLY NEW PAINT. |
| **repack (v) — UNNAPROVED** | PUT (v) PUT THE ASSEMBLY Repack the assembly in BACK IN THE BOX. the box. |
| **FILL (v)** | FILL THE HOLE WITH Repack the hole with GREASE AGAIN. grease. |
| **repaint (v) — UNNAPROVED** | PAINT (v) PAINT ALL THE Repaint all the surfaces. SURFACES AGAIN. |
| **REPAIR (n)** | The act of repairing or AFTER THE REPAIR, the result when APPLY A PROTECTIVE something is repaired LAYER OF GREASE TO ALL EXTERNAL SURFACES. |
| **REPAIR (v)** | , To make an item REPAIR THE REPAIRS, serviceable DEFECTIVE WIRING. REPAIRED, REPAIRED |
| **repairable (adj) — UNNAPROVED** | REPAIR (v) IT IS POSSIBLE TO This damage is REPAIR THIS repairable. DAMAGE. |
| **repeat (v) — UNNAPROVED** | AGAIN (adv) DO STEPS (10) THRU Repeat steps (10) to (14) AGAIN. (14). |
| **repeated (adj) — UNNAPROVED** | AGAIN AND AGAIN IF YOU HEAR SIGNALS If repeated signals are AGAIN AND AGAIN, DO heard, check the AP A CHECK OF THE "AP ENGAGE button on the ENGAGE" BUTTON ON flight mode panel. THE FLIGHT MODE PANEL. |
| **repeatedly (adv) — UNNAPROVED** | AGAIN AND AGAIN IF THE VOLTAGE If voltage drops DECREASES AGAIN repeatedly, adjust the AND AGAIN, ADJUST voltage regulator. THE VOLTAGE REGULATOR. |
| **REPLACE (v)** | , To remove an item and REPLACE THE RELAY. REPLACES, to install a new or REPLACED, serviceable item of the REPLACED same type REPLACEMENT The item you install MAKE SURE THAT THE (n) when you replace an REPLACEMENT HAS item THE CORRECT DIMENSIONS. |
| **replenish (v) — UNNAPROVED** | FILL (v) FILL THE Replenish the ACCUMULATOR WITH accumulator with oil. OIL. |
| **ADD (v)** | ADD OIL TO THE Replenish the oil in the ACCUMULATOR. accumulator. |
| **REFUEL (v)** | REFUEL THE VEHICLE. Replenish the vehicle with fuel. |
| **REPORT (n)** | The information that is IF THERE IS A recorded about a subject REPORT OF DAMAGE, or occurrence DO AN ACCURATE INSPECTION. |
| **reposition (v) — UNNAPROVED** | MOVE (v) MOVE THE LEVER Reposition the lever. BACK TO ITS INITIAL POSITION. |
| **PUT (v)** | PUT THE LEVER BACK Reposition the lever. TO ITS INITIAL POSITION. |
| **SET (v)** | SET THE SWITCH Reposition the switch to BACK TO THE OFF OFF. POSITION. |
| **represent (v) — UNNAPROVED** | SHOW (v) THE SUCTION SHOWS The suction is AS AN ALTIMETER represented by an INDICATION. altimeter reading. |
| **repressurize (v) — UNNAPROVED** | PRESSURIZE (v) PRESSURIZE THE Repressurize the tank. TANK AGAIN. |
| **request (n) — UNNAPROVED** | TELL (v) TELL THE FIRE Make a request for SERVICE TO HELP external fire support. YOU. |
| **WRITE (v)** | IF AID IS NECESSARY, Any request for WRITE TO THE assistance should be MANUFACTURER. addressed to the manufacturer. |
| **request (v) — UNNAPROVED** | TELL (v) TELL THE FIRE Request external fire SERVICE TO HELP support. YOU. |
| **WRITE (v)** | WRITE TO THE Request repair MANUFACTURER FOR instructions from the REPAIR manufacturer. INSTRUCTIONS. |
| **require (v) — UNNAPROVED** | NECESSARY (adj) DURING THIS During this procedure, PROCEDURE, CLEAN clean filters are required. FILTERS ARE NECESSARY. |
| **reseal (v) — UNNAPROVED** | SEAL (v) SEAL THE CONTAINER Reseal the container. AGAIN. |
| **reset (v) — UNNAPROVED** | SET (v) SET THE INDICATOR Reset the indicator to a TO A NEW POSITION. new position. |
| **residual (adj) — UNNAPROVED** | REMAINING (adj) REMOVE ALL THE Remove all residual REMAINING GREASE. grease. |
| **residue (n) — UNNAPROVED** | REMAINING (adj) REMOVE THE Remove the grease REMAINING GREASE. residues. |
| **RESISTANT (adj)** | That will help to prevent THE MATERIAL OF something THE SEATS IS RESISTANT TO FIRE. |
| **respective (adj) — UNNAPROVED** | RELATED (adj) ATTACH THE CABLES Attach the cables to their TO THEIR RELATED respective shackles. SHACKLES. |
| **CORRECT (adj)** | INSTALL THE BOLTS Install the bolts in their IN THEIR CORRECT respective positions. POSITIONS. |
| **respectively (adv) — UNNAPROVED** | RELATED (adj) ENGINES 1 AND 2 Engines 1 and 2 supply SUPPLY HOT AIR TO the left and right wings THEIR RELATED respectively with hot air. WINGS. |
| **respond (v) — UNNAPROVED** | RESULT (n) IF THE INSTRUMENT If the instrument fails to DOES NOT GIVE A respond, do a test. RESULT, DO A TEST. |
| **rest (n) — UNNAPROVED** | REMAINING (adj) THE REMAINING The rest of these INSTRUCTIONS ARE instructions only apply to APPLICABLE ONLY TO approved personnel. APPROVED PERSONNEL. |
