# Page 161 of 434

**Page 2-1-A20**

**Part 2 - Dictionary**

**Issue 9 2025-01-15**

##### **ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
||---|---|---|---|

||**associated (adj) — UNNAPPROVED**|CORRECT (adj)|INSTALL THE DUMP
VALVE AND THE
CORRECT GASKET.|Install the dump valve
with the associated
gasket.|
|||RELATED (adj)|REMOVE THE PANELS
FROM THE RELATED
DOORS.|Remove the panels from
the associated doors.|
|||ITS (adj)|REMOVE THE BOLT
AND ITS WASHER.|Remove the bolt and the
associated washer.|
|||THEIR (adj)|REMOVE THE EIGHT
BOLTS AND THEIR
WADGERS.|Remove the eight bolts
and the associated
washers.|
||**assume (v) — UNNAPPROVED**|THINK (v)|IF YOU THINK THAT
YOU CAN REPAIR THE
DAMAGE, REFER TO
THE REPAIR SECTION.|<p>If damage is assumed to</p>
|||<p>be repairable, refer to</p>
|||<p>the repair section.</p>
||**assume (v) — UNNAPPROVED**|THINK (v)|IF YOU THINK THAT
YOU CAN REPAIR THE
DAMAGE, REFER TO
THE REPAIR SECTION.|
If damage is assumed to
be repairable, refer to
the repair section.
||**assume (v) — UNNAPPROVED**|THINK (v)|IF YOU THINK THAT
YOU CAN REPAIR THE
DAMAGE, REFER TO
THE REPAIR SECTION.|
If damage is assumed to
be repairable, refer to
the repair section.
||**assume (v) — UNNAPPROVED**|THINK (v)|IF YOU THINK THAT
YOU CAN REPAIR THE
DAMAGE, REFER TO
THE REPAIR SECTION.|
If damage is assumed to
be repairable, refer to
the repair section.
||**assume (v) — UNNAPPROVED**|THINK (v)|IF YOU THINK THAT
YOU CAN REPAIR THE
DAMAGE, REFER TO
THE REPAIR SECTION.|
If damage is assumed to
be repairable, refer to
the repair section.
||**assume (v) — UNNAPPROVED**|THINK (v)|IF YOU THINK THAT
YOU CAN REPAIR THE
DAMAGE, REFER TO
THE REPAIR SECTION.|
If damage is assumed to
be repairable, refer to
the repair section.
||**assume (v) — UNNAPPROVED**|THINK (v)|IF YOU THINK THAT
YOU CAN REPAIR THE
DAMAGE, REFER TO
THE REPAIR SECTION.|
If damage is assumed to
be repairable, refer to
the repair section.
||**assume (v) — UNNAPPROVED**|THINK (v)|IF YOU THINK THAT
YOU CAN REPAIR THE
DAMAGE, REFER TO
THE REPAIR SECTION.|
If damage is assumed to
be repairable, refer to
the repair section.
||**assume (v) — UNNAPPROVED**|THINK (v)|IF YOU THINK THAT
YOU CAN REPAIR THE
DAMAGE, REFER TO
THE REPAIR SECTION.|
If damage is assumed to
be repairable, refer to
the repair section.
||**assume (v) — UNNAPPROVED**|THINK (v)|IF YOU THINK THAT
YOU CAN REPAIR THE
DAMAGE, REFER TO
THE REPAIR SECTION.|
If damage is assumed to
be repairable, refer to
the repair section.
||**assume (v) — UNNAPPROVED**|THINK (v)|IF YOU THINK THAT
YOU CAN REPAIR THE
DAMAGE, REFER TO
THE REPAIR SECTION.|
If damage is assumed to
be repairable, refer to
the repair section.

**Issue 9 Part 2 - Dictionary 2025-01-15**

# Page 162 of 434

**Page 2-1-A21**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
||---|---|---|---|

||**ATTACH (v),**<br>**ATTACHES,**<br>**ATTACHED,**<br>**ATTACHED**|To stay together or to<br>cause different items to<br>stay together|MAKE SURE THAT THE
LABEL FULLY
ATTACHES TO THE
SURFACE AND THAT
THERE ARE NO
BUBBLES.|
||||TEMPORARILY
ATTACH THE CABLE
TO THE ADJACENT
STRUCTURE.|
||**attachment (n) — UNNAPPROVED**|ATTACH (v)|MAKE SURE THAT THE
DUCT IS CORRECTLY
ATTACHED TO THE
FILTER.|
Make sure that the
attachment of the duct to
the filter is correct.
||**attain (v) — UNNAPPROVED**|SHOW (v)|WHEN THE
VOLTMETER SHOWS
28 VOLTS DC, THE
RELAY CLOSES.|
When 28 volts DC is
attained, the relay
closes.
|||BE (v)|WHEN THE VOLTAGE
IS 28 VOLTS DC, THE
RELAY CLOSES.|
When 28 volts DC is
attained, the relay
closes.
|||GET (v)|WHEN YOU GET
28 VOLTS DC, THE
RELAY CLOSES.|
When 28 volts DC is
attained, the relay
closes.
||**attempt (n) — UNNAPPROVED**|TRY (v)|TRY TO LIFT THE
COVER MANUALLY.|
Make an attempt to lift
the cover manually.
||**attempt (v) — UNNAPPROVED**|TRY (v)|TRY TO FIND THE
DEFECT.|
Attempt to find the
defect.
||**attention (n) — UNNAPPROVED**|AID (n)|IF YOU GET PAINT
SPRAY IN YOUR EYES,
GET MEDICAL AID.|
If you get paint spray in
your eyes, get medical
attention.
|||CAREFUL (adj)|BE CAREFUL WHEN
YOU REMOVE THE
CONTROL UNIT.|
Pay attention when you
remove the control unit.
|||MONITOR (v)|MONITOR THE
RESULTS.|
Pay attention to the
results.

# Page 163 of 434

**Page 2-1-A22**

**Part 2 - Dictionary**

**Issue 9 2025-01-15**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
||---|---|---|---|

||**audible (adj) — UNNAPPROVED**|HEAR (v)|IF YOU CANNOT HEAR
THE ALARM, ADJUST
THE VOLUME
CONTROL.|
If the alarm is not
audible, adjust the
volume control.
|||LISTEN (v)|LISTEN FOR AIR
LEAKAGE FROM THE
LINES.|
Check the lines for
audible air leakage.
||**augment (v) — UNNAPPROVED**|INCREASE (v)|A MIXTURE OF WATER
AND METHANOL
INCREASES THE
POWER OF THE
ENGINE.|
A mixture of water and
methanol augments
the power of the engine.
||**aurally (adv) — UNNAPPROVED**|LISTEN (v)|LISTEN TO MAKE
SURE THAT THE FLUID
FLOWS.|
Check aurally to ensure
fluid flow.
|||HEAR (v)|YOU CAN HEAR THE
WARNING IN THE
COCKPIT.|
The warning is given
aurally in the cockpit.
||**authentic (adj) — UNNAPPROVED**|ACCURATE (adj)|IF THE ADJUSTMENT
OF THE STOPS IS NOT
CORRECT, THE
RESULTS OF THE
TEST WILL NOT BE
ACCURATE.|
If the adjustment of the
stops is not correct, the
results of the test will not
be authentic.
||**AUTHORITY (n)**|An official organization
that gives approval to
something|BEFORE YOU CHANGE
THE PROCEDURE,
GET THE APPROVAL
OF THE DESIGN
AUTHORITY.|
||**authorized (adj) — UNNAPPROVED**|APPROVED (adj)|ONLY APPROVED
PERSONS ARE
PERMITTED TO STAY
IN THIS AREA.|
Only authorized persons
are permitted to stay in
this area.
||**AUTOMATIC (adj)**|That operates without
other input|THE AUTOMATIC
SYSTEM WILL OPEN
THE DOORS.|
||**AUTOMATICALLY**<br>**(adv)**|That operates without
other input|THE FUEL FLOW
STOPS
AUTOMATICALLY.|

**Issue 9 2025-01-15**

**Part 2 - Dictionary**

# Page 164 of 434

**Page 2-1-A23**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
||---|---|---|---|

||**AUXILIARY (adj)**|1. That operates in a
secondary function|LUBRICANTS FOR THE
ENGINE AND THE
AUXILIARY
EQUIPMENT ARE THE
SAME.|
|||2. That gives help|USE AUXILIARY
SCREWS TO
ASSEMBLE THE UNIT
TEMPORARILY.|
||**AVAILABLE (adj)**|Prepared or supplied for
you to use|IF ELECTRICAL
POWER IS AVAILABLE,
DO A CONTINUITY
CHECK.|
||**avert (v) — UNNAPPROVED**|PREVENT (v)|IF THE MICROSWITCH
BECOMES
UNSERVICEABLE,
DEACTIVATE THE
ACTUATOR TO
PREVENT DAMAGE TO
THE VALVE.|
If the microswitch
becomes unserviceable,
deactivate the actuator
to avert damage to the
valve.
||**avoid (v) — UNNAPPROVED**|PREVENT (v)|TURN THE CONTROLS
SLOWLY TO PREVENT
DAMAGE.|
Turn the controls slowly
to avoid damage.
|||DO NOT|DO NOT PUSH ON THE
SEALS.|
Avoid pushing on the
seals.
||**aware (adj) — UNNAPPROVED**|KNOW (v)|ALL PERSONNEL
MUST KNOW THE
HEALTH RISKS.|
All personnel must be
aware of the health risks.
|||TELL (v)|TELL ALL PERSONNEL
ABOUT THE NEW
RULES.|
All personnel must be
aware of the new rules.
||**AWAY FROM**<br>**(prep)**|In or to a different
position or direction|DO THE WORK IN AN
AREA AWAY FROM
EQUIPMENT OR
METAL FRAME
BUILDINGS.|
||**AXIAL (adj)**|Related to an axis|DO STEPS 1 THRU 4
TO MAKE SURE THAT
NO AXIAL LOAD IS ON
THE ROD.|
||**AXIALLY (adv)**|Related to an axis|APPLY THE LOAD
AXIALLY.|
