# Page 329–332 of 434

> **Source:** ASD-STE100 Issue 9, January 2025
> **Pages:** 329–332 of 434

# Page 329 of 434

| Word (part of speech) | Approved meaning/ALTERNATIVES | STE EXAMPLE | Non-STE example |
|---|---|---|---|
| **PREPARE (v), PREPARES, PREPARED, PREPARED** | To make or become ready | PREPARE THE TUBE FOR THE LEAK TEST.<br>PREPARE FOR THE ELECTRICAL BONDING PROCEDURE. |  |
| **prescribed (adj) — UNNAPPROVED** | SPECIFIED (adj) | FILL THE CONTAINER WITH THE SPECIFIED COOLANT FLUID. | Fill the container with the prescribed coolant fluid. |
| **presence (n) — UNNAPPROVED** | BE (v) | THIS INSPECTION IS NECESSARY WHEN THERE ARE DEFECTS. | This inspection is necessary in the presence of defects. |
| **present (adj) — UNNAPPROVED** | BE (v) | IF THERE IS A VOLTAGE AT PIN C OF CONNECTOR F7, THE UNIT IS UNSERVICEABLE. | If a voltage is present at pin C of connector F7, the unit is faulty. |
| **present (v) — UNNAPPROVED** | GIVE (v)<br>SHOW (v) | THIS SECTION GIVES THE APPLICABLE TORQUE VALUES.<br>THE TABLE THAT FOLLOWS SHOWS THE RESULTS OF THE SURVEY. | The applicable torque values are presented in this section.<br>The results of the survey are presented in the following table. |
| **preserve (v) — UNNAPPROVED** | PRESERVATION (TN) | THIS PROCEDURE IS FOR THE PRESERVATION OF STEEL CABLES. | This procedure will preserve the steel cables. |
| **preset (v) — UNNAPPROVED** | SET (v) | SET THE TENSION INDICATOR TO ZERO. | Preset the tension indicator to zero. |
| **press (v) — UNNAPPROVED** | PUSH (v) | PUSH AND HOLD THE TEST BUTTON. | Press and hold the TEST button. |
| **PRESSURIZATION (n)** | The procedure that supplies or increases the pressure | CONTINUE THE PRESSURIZATION FOR 10 MINUTES. |  |
| **PRESSURIZE (v), PRESSURIZES, PRESSURIZED, PRESSURIZED** | To supply pressure | PRESSURIZE THE CHAMBER TO 150 psi. |  |

# Page 330 of 434

| Word (part of speech) | Approved meaning/ALTERNATIVES | STE EXAMPLE | Non-STE example |
|---|---|---|---|
| **PREVENT (v), PREVENTS, PREVENTED, PREVENTED** | To make sure that something does not occur | TO PREVENT DAMAGE TO THE ENGINE, IMMEDIATELY INSTALL PROTECTIVE COVERS ON ALL OPENINGS. |  |
| **prevent (from) (v)** | LET (v) | DO NOT LET THE DOOR OPEN. | Prevent the door from opening. |
| **preventive (adj) — UNNAPPROVED** | PREVENT (v) | THIS COATING PREVENTS CORROSION. | This coating is a preventive measure for corrosion. |
| **PREVIOUS (adj)** | That goes before in an unspecified time or sequence<br>Be accurate. Use LAST (adj) for the event that occurs immediately before in time or sequence. | IF YOU SELECTED "YES" IN A PREVIOUS STEP, GO TO PARAGRAPH 7.5.<br>DO THE LAST INSPECTION AGAIN. | Do the previous inspection again. |
| **PREVIOUSLY (adv)** | Before, earlier, in the past | THIS SOFTWARE FINDS TERMS FROM PREVIOUSLY TRANSLATED FILES. |  |
| **primarily (adv) — UNNAPPROVED** | PRIMARY (adj) | THE PRIMARY FUNCTION OF THE HYDRAULIC SYSTEM IS TO SUPPLY THE PRESSURE TO OPERATE THE FLIGHT CONTROLS. | The hydraulic system primarily supplies the pressure to operate the flight controls. |
| **PRIMARY (adj)** | First in importance | THE PRIMARY FUNCTION OF THE POWER UNIT IS TO SUPPLY ELECTRICAL POWER. |  |
| **prime (v) — UNNAPPROVED** | FILL (v)<br>PUT (v) | FILL THE FILLER HOSE WITH WATER.<br>PUT FUEL IN THE FUEL PUMP. | Prime the filler hose with water.<br>Prime the fuel pump. |

# Page 331 of 434

| Word (part of speech) | Approved meaning/ALTERNATIVES | STE EXAMPLE | Non-STE example |
|---|---|---|---|
| **principal (adj) — UNNAPPROVED** | PRIMARY (adj) | THE PRIMARY FUNCTION OF THE SYSTEM IS TO SUPPLY ELECTRICAL POWER TO THE CONTROL PANEL. | The principal function of the system is to supply electrical power to the control panel . |
| **prior to (prep) — UNNAPPROVED** | BEFORE (conj) | BEFORE YOU DISCONNECT THE HOSES, DRAIN THE SYSTEM. | Drain the system prior to disconnecting the hoses. |
| **priority (n) — UNNAPPROVED** | IMPORTANT (adj)<br>BEFORE (prep)<br>FIRST (adv) | THIS PROCEDURE IS VERY IMPORTANT.<br>BEFORE YOU FILL THE OUTER TANK, FILL THE INNER TANK.<br>DURING THE PROCEDURE THAT FOLLOWS, REPAIR THE UPPER FLANGE FIRST. | This procedure has high priority.<br>The inner tank filling procedure has priority over the outer tank filling procedure.<br>During the following repair procedure, the upper flange has priority. |
| **probability (n) — UNNAPPROVED** | RISK (n) | TO DECREASE THE RISK OF FIRE, OBEY THE SAFETY PRECAUTIONS. | Obey the safety precautions to decrease the probability of fire. |
| **probable (adj) — UNNAPPROVED** | VERY POSSIBLE<br>RISK (n) | IF YOU DO NOT SAFETY THE DOOR, IT IS VERY POSSIBLE THAT STRONG WINDS WILL CAUSE DAMAGE TO THE STRUCTURE.<br>IF YOU DO NOT SAFETY THE DOOR, THERE IS A RISK THAT STRONG WINDS WILL CAUSE DAMAGE TO THE STRUCTURE. | If you do not safety the door, damage to the structure due to strong winds is probable.<br>If you do not safety the door, damage to the structure due to strong winds is probable. |
| **probe (v) — UNNAPPROVED** | FIND (v) (WITH A PROBE [TN]) | FIND THE BLOCKAGE IN THE TUBE WITH AN APPLICABLE PROBE. | Probe the tube to find the blockage. |
| **PROBLEM (n)** | Something that is difficult and for which you must find the correct answer | IF YOU FIND A PROBLEM DURING THE TEST, REFER TO THE FAULT ISOLATION TABLE. |  |

# Page 332 of 434

| Word (part of speech) | Approved meaning/ALTERNATIVES | STE EXAMPLE | Non-STE example |
|---|---|---|---|
| **PROCEDURE (n)** | Steps that are in a sequence | THIS SECTION GIVES THE PROCEDURE TO DISASSEMBLE THE COMPONENT FULLY. |  |
| **proceed (v) — UNNAPPROVED** | CONTINUE (v) | CONTINUE WITH THE ELECTRICAL TEST. | Proceed with the electrical test. |
| **process (in the process of ) (prep)** | DURING (prep)<br>WHILE (conj) | DURING THIS REPAIR, APPLY SUFFICIENT HEAT TO THE UNIT.<br>WHILE YOU DO THIS REPAIR, APPLY SUFFICIENT HEAT TO THE UNIT. | Apply sufficient heat to the unit in the process of doing this repair.<br>Apply sufficient heat to the unit in the process of doing this repair. |
| **process (n) — UNNAPPROVED** | PROCEDURE (n)<br>This word is a technical noun when it means a sequence of changes that occur and cause a result. | THESE TWO ASSEMBLY PROCEDURES ARE ALMOST THE SAME.<br>CORROSION IS AN ELECTROLYTIC PROCESS. | These two assembly processes are almost the same. |
| **process (v) — UNNAPPROVED** | DO (v) THE … PROCEDURE (n) | PUT THE PARTS IN AN ELECTROLYTIC BATH. THEN, DO THE ELECTROPLATING PROCEDURE. | Process the parts in an electrolytic bath. |
| **produce (v) — UNNAPPROVED** | CAUSE (v)<br>GIVE (v)<br>MAKE (v)<br>SUPPLY (v) | ELECTRICAL EQUIPMENT CAN CAUSE INTERFERENCE IN COMMUNICATION.<br>A DILUTED SOLUTION WILL NOT GIVE YOU THE CORRECT<BR>RESULTS.<br>WHEN THE LEVER ENGAGES, IT MAKES A CLICK<br>THE POWER UNIT SUPPLIES THE SYSTEM WITH A VOLTAGE OF 28 V DC. | Electrical equipment can produce interference in communication.<br>A diluted solution does not produce the correct results.<br>The lever produces a click when engaged.<br>The power unit produces a voltage of 28 V DC. |
