<!-- section: DICT_A-F | pages: 237-240 | verified: true -->

# Page 237 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **every (adj) — UNNAPROVED** | ALL (adj) REMOVE ALL SAFETY Every safety pin must be PINS BEFORE FLIGHT. removed before flight. |
| **EACH (adj)** | SET THE BTRY It is necessary to set the SWITCH TO "ON" BTRY switch to ON EACH TIME. every time. |
| **INTERVAL (n)** | DO AN INSPECTION Do an inspection every AT INTERVALS OF 20 000 flight hours. 20 000 FLIGHT HOURS. |
| **evidence (n) — UNNAPROVED** | INDICATION (n) IF THERE IS AN If there is evidence of a INDICATION OF A leak, replace the valve. LEAK, REPLACE THE VALVE. |
| **SIGN (n)** | ONE SIGN OF A LEAK Evidence of a leak of hot OF HOT AIR FROM A air from a joint is that the JOINT IS THAT THE temperature reading TEMPERATURE drops. INDICATION DECREASES. |
| **SHOW (v)** | REPLACE THE Replace the insulation INSULATION blankets with evidence BLANKETS THAT of chafing. SHOW CHAFING. |
| **evidence (v) — UNNAPROVED** | SHOW (v) IF THE TEST SHOWS If no fault is evidenced NO FAULT, CONTINUE by the test, continue the THE PROCEDURE. procedure. |
| **FIND (v)** | IF YOU DO NOT FIND If the inspection does DAMAGE DURING THE not evidence any INSPECTION damage, assemble the PROCEDURE, unit. ASSEMBLE THE UNIT. |
| **evident (adj) — UNNAPROVED** | FIND (v) IF YOU DO NOT FIND If no damage is evident, DAMAGE, CONTINUE continue the inspection. THE INSPECTION. |
| **exact (adj) — UNNAPROVED** | ACCURATE (adj) IF THE INDICATION IS If the indication is not NOT ACCURATE, DO exact, do the test again. THE TEST AGAIN. |
| **CORRECT (adj)** | IF THE INDICATION IS If the indication is not NOT CORRECT, DO exact, do the test again. THE TEST AGAIN. |

# Page 238 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **exactly (adv) — UNNAPROVED** | ACCURATELY (adv) PUT THE REPAIR Put the repair sheet SHEET ACCURATELY exactly on the damaged ON THE DAMAGED area. AREA. |
| **FULLY (adv)** | FIND THE BOLT HOLE Find the bolt hole that THAT ALIGNS FULLY aligns exactly with one WITH ONE OF THE of the outer slots. OUTER SLOTS. |
| **CORRECT (adj)** | THE SEAL MUST BE The seal must fit the OF THE CORRECT groove exactly. DIMENSION FOR THE GROOVE. |
| **examination (n) — UNNAPROVED** | EXAMINE (v) EXAMINE THE BLADE Do an examination of FOR CRACKS. the blades for cracks. |
| **FIND (v)** | IF YOU FIND If the examination CORROSION, reveals corrosion, it REMOVE IT WITH THE must be removed with SPECIFIED MATERIAL. the specified material. |
| **EXAMINE (v)** | , To look carefully at EXAMINE THE EXAMINES, COMPUTER FOR EXAMINED, DAMAGE. EXAMINED |
| **EXAMPLE (n)** | Something from a group FIGURE 2 IS AN which has the same EXAMPLE OF A qualities as the group REPAIR PROCEDURE FOR A DAMAGED WEB. |
| **exceed (v) — UNNAPROVED** | MORE THAN MAKE SURE THAT Ensure that the THE INDICATION IS indication does not NOT MORE THAN exceed 400 knots. 400 KNOTS. |
| **except (prep) — UNNAPROVED** | To replace this KEEP ALL THE PARTS Keep all parts except word, use a THAT ARE those that are broken. different SERVICEABLE AND construction. DISCARD THOSE Be accurate. THAT ARE BROKEN. REMOVE ALL Remove all screws SCREWS, BUT NOT except the one on the THE ONE ON THE left side of the flange. LEFT SIDE OF THE FLANGE. |

# Page 239 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **exception (n) — UNNAPROVED** | To replace this KEEP ALL THE PARTS Keep all parts with the word, use a THAT ARE exception of those that different SERVICEABLE AND are broken. construction. DISCARD THOSE Be accurate. THAT ARE BROKEN. REMOVE ALL Remove all screws with SCREWS, BUT NOT the exception of the one THE ONE ON THE on the left side of the LEFT SIDE OF THE flange. FLANGE. |
| **exceptional (adj) — UNNAPROVED** | UNUSUAL (adj) IF IT IS NECESSARY If exceptional force is TO APPLY UNUSUAL needed to open the unit, FORCE TO OPEN THE examine the control UNIT, EXAMINE THE linkage. CONTROL LINKAGE. |
| **exceptionally (adv) — UNNAPROVED** | UNUSUALLY (adv) IF THE TIRE If the tire pressure is PRESSURE IS exceptionally high, open UNUSUALLY HIGH, the valve. OPEN THE VALVE. |
| **excess (adj) — UNNAPROVED** | TOO MUCH DO NOT APPLY TOO Do not apply excess MUCH ADHESIVE ON adhesive on the gasket. THE GASKET. MORE THAN DO NOT PUT MORE Do not put excess THAN THE weight on the trolley. PERMITTED WEIGHT ON THE TROLLEY. |
| **UNWANTED (adj)** | REMOVE UNWANTED Wipe excess compound COMPOUND FROM from the gasket. THE GASKET. NOT NECESSARY REMOVE ALL Remove all the excess REMAINING SEALANT sealant. THAT IS NOT NECESSARY. |
| **excess (n) — UNNAPROVED** | TOO MUCH IF YOU USE TOO An excess of paint will MUCH PAINT, THE give a poor finish. FINISH WILL BE UNSATISFACTORY. MORE THAN THE HYDRAULIC The hydraulic pressure PRESSURE MUST NOT must not be in excess of BE MORE THAN 200 bar. 200 bar. |

# Page 240 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **excessive (adj) — UNNAPROVED** | TOO MUCH TOO MUCH FORCE Excessive force can CAN CAUSE DAMAGE damage the seal. TO THE SEAL. MORE THAN IF THE PRESSURE IS If the pressure is MORE THAN 1000 kPa, excessive, stop the test. STOP THE TEST. |
| **excessively (adv) — UNNAPROVED** | TOO MUCH BE CAREFUL NOT TO Be careful not to TURN THE INNER excessively rotate the RACES TOO MUCH. inner races. MORE THAN IF THE OIL LEAKAGE If oil leaks excessively, IS MORE THAN FIVE reject the unit. DROPS A MINUTE, REJECT THE UNIT. |
| **exchange (v) — UNNAPROVED** | INTERCHANGE (v) INTERCHANGE THE Exchange the No. 1 and No. 1 AND No. 2 No. 2 computers. Then COMPUTERS. THEN do the test again. DO THE TEST AGAIN. |
| **REPLACE (v)** | REPLACE THE Exchange the O-rings. O-RINGS. |
| **exclude (v) — UNNAPROVED** | NOT INCLUDE THIS PROCEDURE This procedure excludes DOES NOT INCLUDE the removal of the THE REMOVAL OF piston. THE PISTON. NOT USE DO NOT USE Exclude the use of OXYGEN. oxygen. |
| **excluding (prep) — UNNAPROVED** | WITHOUT (prep) THE WEIGHT OF THE The weight of the unit, UNIT, WITHOUT THE excluding the motor, is MOTOR, IS 10 kg. 10 kg. |
| **execute (v) — UNNAPROVED** | DO (v) DO THESE STEPS. Execute the following operations. |
| **exempt (adj) — UNNAPROVED** | NO (adj) MAKE SURE THAT Ensure the oil is exempt THERE ARE NO from metal particles. METAL PARTICLES IN THE OIL. NOT SHOW MAKE SURE THAT Ensure the seals are THE SEALS DO NOT exempt from signs of SHOW SIGNS OF deterioration. DETERIORATION. |
