# Page 185 of 434

**Page 2-1-C10**

**Part 2 - Dictionary**

**Issue 9 2025-01-15**

**ASD-STE100 Simplified Technical English**

|**Word**(part of speech)|**Approved meaning/**ALTERNATIVES|**STE EXAMPLE**|**Non-STE example**|
|---|---|---|---|
|**COIL (n)**|A sequence of loops|MAKE SURE THAT THE COILS OF THE OXYGEN HOSE DO NOT RUB TOGETHER.||
|**coil (v) — UNNAPPROVED**|WIND (v)|WIND THE CABLES CAREFULLY.|Coil the cables carefully.|
|**coincide (v) — UNNAPPROVED**|ALIGN (v)|THE FASTENERS MUST ALIGN WITH THE HOLES IN THE TRACK.|The fasteners must coincide with the holes in the track.|
|**coincident (adj) — UNNAPPROVED**|SYNCHRONIZED (adj)|MAKE SURE THAT THE MOVEMENT OF THE TWO SURFACES IS SYNCHRONIZED.|Make sure that the movement of the two surfaces is coincident.|
|||ALIGN (v)|MAKE SURE THAT THE TWO SURFACES ALIGN.|Make sure that the two surfaces are coincident.|
|**COLD (adj)**(COLDER, COLDEST)|At low temperature|MAKE SURE THAT COLD AIR COMES OUT OF THE OUTLETS.||
|**collapse (v) — UNNAPPROVED**|CLOSE (v)|CLOSE THE BOX.|Collapse the box.|
|||FALL (v)|THE BOARDING BRIDGE FELL.|The boarding bridge collapsed.|
|**COLLECT (v), COLLECTS, COLLECTED, COLLECTED**|To come, or cause to come, together in one location|FLUID COLLECTS IN THE BOTTOM OF THE COWLING.||
||||COLLECT ALL LOOSE ITEMS AND PUT THEM IN THE CONTAINER.||
|**COLOR (n)**|A property of light|THE COLOR CHANGES FROM BLUE TO RED.||
|**color code (v) — UNNAPPROVED**|IDENTIFY (v)|IDENTIFY THE ASSEMBLY WITH THE CORRECT COLOR.|The assembly must be color coded.|
|||CODE (n)|PUT A COLOR CODE ON EACH OF THE ASSEMBLIES.|Color code the assemblies.|
|**colored (adj) — UNNAPPROVED**|COLOR (n)|THE SCALE HAS TWO AREAS OF DIFFERENT COLOR.|The scale is divided into two colored areas.|

<!-- TABLE CONTINUES ON NEXT PAGE -->

# Page 186 of 434

**Page 2-1-C11**

**Issue 9 2025-01-15**

**Part 2 - Dictionary**

**ASD-STE100 Simplified Technical English**

|**Word**(part of speech)|**Approved meaning/**ALTERNATIVES|**STE EXAMPLE**|**Non-STE example**|
|---|---|---|---|
|**combine (v) — UNNAPPROVED**|MIX (v)|MIX THE WATER AND THE GLYCOL.|Combine water and glycol.|
|||PUT TOGETHER|DO NOT PUT DIFFERENT HPT SEGMENTS TOGETHER.|Do not combine different HPT segments.|
|**combustible (adj) — UNNAPPROVED**|FLAMMABLE (adj)|KEEP FLAMMABLE MATERIALS AT A MINIMUM DISTANCE OF 50 FEET FROM THE WORK AREA.||
|**COME (v), COMES, CAME** No other verb forms.|To move to your location|FUMES MUST NOT COME INTO THE CABIN.||
|**COME ON (v), COMES ON, CAME ON** No other verb forms.|To become bright with light when an internal power source is energized|THE LIGHTS MUST COME ON.||
|**commence (v) — UNNAPPROVED**|START (v)|THE WARNING STARTS AND THE INDICATORS FLASH.|The warning commences and the indicators flash.|
|**commencement (n)**|START (v)|AFTER THE TEST STARTS, MONITOR THE RESULTS ON THE SCREEN.|After the test commencement, monitor the results on the screen.|
|**common (adj) — UNNAPPROVED**|SAME (adv)|THE REMOVAL PROCEDURE IS THE SAME FOR THE TWO ITEMS.|The removal procedure is common to both items.|

<!-- TABLE CONTINUES ON NEXT PAGE -->

# Page 187 of 434

**Page 2-1-C12**

Part 2 - Dictionary

**Issue 9 2025-01-15**

**ASD-STE100 Simplified Technical English**

|**Word**(part of speech)|**Approved meaning/**ALTERNATIVES|**STE EXAMPLE**|**Non-STE example**|
|---|---|---|---|
|**communicate (v) — UNNAPPROVED**|CONTACT (v)|FOR MORE INFORMATION, CONTACT THE MANUFACTURER.|For more information, communicate with the manufacturer.|
|||SPEAK (v)|USE A TELEPHONE TO SPEAK WITH THE LINE MANAGER.|Use a telephone to communicate with the line manager.|
|||HEAR (v)|MAKE SURE THAT AIR TRAFFIC CONTROL CAN HEAR YOU.|Make sure that you communicate with ATC.|
|||COMMUNICATION (n)|MAKE SURE THAT THERE IS COMMUNICATION BETWEEN THE SERVER AND THE PC.|Make sure that the server and the PC can communicate.|
|**COMMUNICATION (n)**|The exchange of information through a common system of symbols, signs, or sounds|COMMUNICATION BETWEEN THESE TWO SYSTEMS IS ENCRYPTED.||
|**COMPARE (v), COMPARES, COMPARED, COMPARED**|To examine for differences|COMPARE THE TWO VALUES.||
|**comparison (n) — UNNAPPROVED**|COMPARE (v)|COMPARE THE TWO INDICATIONS.|Make a comparison of the two readings.|
|**COMPATIBLE (adj)**|That can operate together satisfactorily or be used together safely|THIS SOFTWARE IS COMPATIBLE ONLY WITH THE SPECIFIED OPERATING SYSTEM.||
||||THE COOLANT IS COMPATIBLE WITH HIGH-PERFORMANCE ALLOYS.||
|**compile (v) — UNNAPPROVED**|MAKE A LIST|MAKE A LIST OF THE NECESSARY TOOLS.|Compile a list of the required tools.|
|||RECORD (v)|RECORD THE AILERON MOVEMENTS ON FORM B.||
|**compilation (n) — UNNAPPROVED**|COLLECT (v)|COLLECT ALL INSPECTION RECORDS FOR THE COMPONENT.|Compile all inspection records for the component.|

# Page 188 of 434

**Page 2-1-C13**

**Issue 9 2025-01-15**

**Part 2 - Dictionary**

**ASD-STE100 Simplified Technical English**

|**Word**(part of speech)|**Approved meaning/**ALTERNATIVES|**STE EXAMPLE**|**Non-STE example**|
|---|---|---|---|
|**complete (adj) — UNNAPPROVED**|FULL (adj)|EXTEND AND RETRACT THE ACTUATOR THROUGH THREE FULL CYCLES.|Extend and retract the actuator through three complete cycles.|
|||ALL (adj)|SEND ALL THE TEST RESULTS TO THE MANUFACTURER.|The complete test results must be sent to the manufacturer.|
|||COMPLETED (adj)|THE GREEN INDICATION SHOWS THAT SERVICING IS COMPLETED.|The green indication shows that servicing is complete.|
|**COMPLETE (v), COMPLETES, COMPLETED, COMPLETED**|To bring to an end|COMPLETE THE FUNCTIONAL TEST.||
|**COMPLETED (adj)**|Successfully brought to an end|SEND THE COMPLETED REPORT TO THE SUPERVISOR FOR APPROVAL.||
|**completely (adv) — UNNAPPROVED**|FULLY (adv)|BEFORE YOU APPLY THE SECOND LAYER, LET THE FIRST LAYER OF PAINT DRY FULLY.||
|**completion (n) — UNNAPPROVED**|END (n)|AT THE END OF THIS PROCEDURE, REFER TO 72-00-00, TEST 001.|See 72-00-00, Testing 001 upon completion of this procedure.|
|||COMPLETE (v)|TWO HOURS ARE NECESSARY TO COMPLETE THIS TASK.|Completion of the task will require two hours.|
|**complicated (adj) — UNNAPPROVED**|NOT EASY|THIS TEST PROCEDURE IS NOT EASY WITHOUT THE CORRECT EQUIPMENT.|This test procedure is complicated without the right equipment.|
|**comply (v) — UNNAPPROVED**|OBEY (v)|WHEN YOU ASSEMBLE THE UNIT, OBEY THIS PROCEDURE.|When you assemble the unit, comply with this procedure.|
|||Used in law and regulations. Refer to rule 1.12.|THE SHIP CERTIFICATE MUST COMPLY WITH ALL THE REQUIREMENTS OF THE AUTHORITIES.||
