# Page 273 of 434

**Page 2-1-I7**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
||---|---|---|---|
||**increase (n) — UNNAPPROVED**|INCREASE (v)|THE TEMPERATURE<br>MUST INCREASE.|There must be an<br>increase in temperature.|
||**INCREASE (v),**<br>**INCREASES,**<br>**INCREASED,**<br>**INCREASED**|To make or become<br>larger or higher in value|INCREASE THE VANE<br>ANGLE TO<br>90 DEGREES.|
||||MAKE SURE THAT THE<br>TEMPERATURE<br>INCREASES TO 30 °C.|
||**INCREMENT (n)**|One of a sequence of<br>regular operations done<br>one after the other, to<br>increase or decrease an<br>adjustable quantity|ADJUST THE STOP<br>BOLT IN INCREMENTS<br>OF 5 mm.|
||**incur (v) — UNNAPPROVED**|CAUSE (v)|REMOVAL OF THE<br>UNIT BEFORE<br>24 HOURS CAN CAUSE<br>DAMAGE.|<br>Removal of the unit<br>before 24 hours can<br>incur damage.|
||**independent (adj) — UNNAPPROVED**|INDEPENDENTLY (adv)|THIS UNIT OPERATES<br>INDEPENDENTLY.|The operation of this unit<br>is independent.|
||**INDEPENDENTLY**<br>**(adv)**|Without a relation with|THE EMERGENCY<br>SYSTEM IS<br>CONTROLLED<br>INDEPENDENTLY.|
||**indicate (v) — UNNAPPROVED**|SHOW (v)|THE POINTER SHOWS<br>ZERO FEET.|The pointer indicates<br>zero feet.|
|||IDENTIFY (v)|A 406 MHz DIGITAL<br>SIGNAL IDENTIFIES<br>THE EMERGENCY<br>LOCATOR<br>TRANSMITTER AND<br>ITS LOCATION.|A 406 MHz digital signal<br>indicates the emergency<br>locator transmitter and<br>its location.|
|||SPECIFIED (adj)|IF TOLERANCES ARE<br>NOT SPECIFIED,<br>REFER TO GENERAL<br>TOLERANCE VALUES.|If tolerances are not<br>indicated, refer to<br>general tolerance<br>values.|
||**INDICATION (n)**|Something that is shown|MAKE SURE THAT THE<br>INDICATION IS<br>CORRECT.|
||**induce (v) — UNNAPPROVED**|CAUSE (v)|SCRATCHES IN THE<br>WINDSCREEN CAN<br>CAUSE CRACKS.|Scratches in the<br>windscreen may induce<br>cracks.|

# Page 274 of 434

**Page 2-1-I8**

**Part 2 - Dictionary**

**Issue 9 2025-01-15**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
||---|---|---|---|
||**ineffective (adj) — UNNAPPROVED**|UNSERVICEABLE (adj)|IF THE PUMP IS<br>UNSERVICEABLE,<br>REPLACE IT.|If the pump is ineffective,<br>replace it.|
|||UNSATISFACTORY<br>(adj)|IF THE OPERATION OF<br>THE PUMP IS<br>UNSATISFACTORY,<br>REPLACE IT.|If the operation of the<br>pump is ineffective,<br>replace it.|
|||NOT OPERATE|IF THE PUMP DOES<br>NOT OPERATE<br>CORRECTLY,<br>REPLACE IT.|If the pump is ineffective,<br>replace it.|
||**inflammable (adj) — UNNAPPROVED**|FLAMMABLE (adj)|SOLVENT IS VERY<br>FLAMMABLE.|Solvent is highly<br>inflammable.|
||**INFLATE (v),**<br>**INFLATES,**<br>**INFLATED,**<br>**INFLATED**|To make or become<br>larger as a result of<br>pressurization by a gas|INFLATE THE TIRES<br>WITH NITROGEN.|
||||OPERATION OF THE<br>HANDLE RELEASES<br>THE GAS, AND THE<br>SLIDE-RAFT<br>INFLATES.|
||**inform (v) — UNNAPPROVED**|TELL (v)|TELL THE<br>MANUFACTURER<br>ABOUT THE<br>PROBLEM.|Inform the manufacturer<br>about the problem.|
||**INFORMATION (n)**|Data collected and made<br>available for a specified<br>function|THIS MANUAL<br>CONTAINS<br>INFORMATION ABOUT<br>MAINTENANCE<br>PROCEDURES.|
||**ingest (v) — UNNAPPROVED**|SWALLOW (v)|IF YOU SWALLOW<br>HYDRAULIC FLUID,<br>GET MEDICAL AID<br>IMMEDIATELY.|If you ingest hydraulic<br>fluid, get medical aid<br>immediately.|
||**ingress (n) — UNNAPPROVED**|GO INTO|IF WATER GOES INTO<br>THE COMPONENT,<br>DAMAGE WILL<br>OCCUR.|Water ingress will<br>damage the component.|

**Issue 9 2025-01-15**

**Part 2 - Dictionary**

# Page 275 of 434

**Page 2-1-I9**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
||---|---|---|---|
||**inhale (v) — UNNAPPROVED**|BREATHE (v)|DO NOT BREATHE<br>THE SOLVENT FUMES.|Do not inhale the solvent<br>fumes.|
||**inhibit (v) — UNNAPPROVED**|PREVENT (v)|ALODINE PREVENTS<br>CORROSION.|Alodine inhibits<br>corrosion.|
||**INITIAL (adj)**|That is related to the<br>start|MOVE THE LEVER<br>BACK TO ITS INITIAL<br>POSITION.|
||**INITIALLY (adv)**|At the start|INITIALLY, THE SPEED<br>INCREASES TO<br>3000 RPM.|
||**initiate (v) — UNNAPPROVED**|START (v)|START THE TEST AT<br>2000 RPM.|Initiate the test at<br>2000 rpm.|
||**inject (v) — UNNAPPROVED**|PUT (v)|PUT OIL INTO THE<br>GEARBOX WITH A<br>SYRINGE.|Inject oil into the gearbox<br>with a syringe.|
||**injection (n) — UNNAPPROVED**|PUT (v)|PUT THE CORROSION<br>PREVENTIVE OIL INTO<br>THE PUMP WITH A<br>SYRINGE.|The injection of the<br>corrosion preventive oil<br>into the pump must be<br>done with a syringe.|
||**injure (v) — UNNAPPROVED**|INJURY (n)|MAKE SURE THAT THE<br>END OF THE SAFETY<br>WIRE WILL NOT<br>CAUSE INJURY TO<br>PERSONS.|<br>Make sure that the end<br>of the safety wire will not<br>injure persons.|
||**INJURY (n)**|Damage to a person|BEND THE ENDS OF<br>THE LOCKING WIRE<br>TO PREVENT INJURY.|
||**INNER (adj)**|Nearer to the center of<br>an object|THE INNER SURFACE<br>OF THE PART IS<br>BLACK.|
||**inoperative (adj) — UNNAPPROVED**|OFF (adj)|BEFORE YOU DRAIN<br>THE FUEL, MAKE<br>SURE THAT THE<br>SYSTEM IS OFF.|Before you drain the<br>fuel, make sure that the<br>system is inoperative.|
|||NOT OPERATE|MAKE SURE THAT THE<br>DEMISTING SYSTEM<br>DOES NOT OPERATE.|<br>Make sure that the<br>demisting system is<br>inoperative.|
||**INPUT (n)**|The data, power, or<br>energy put into<br>equipment or a system|THE UNIT COMPARES<br>THE INPUTS FROM<br>THE TWO SENSORS<br>TO THE COMPUTER.|

# Page 276 of 434

**Page 2-1-I10**

**Part 2 - Dictionary**

**Issue 9 2025-01-15**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
||---|---|---|---|
||**insert (v) — UNNAPPROVED**|PUT (v)|PUT THE SLEEVE INTO<br>THE OPENING.|Insert the sleeve into the<br>opening.|
|||ENGAGE (v)|MAKE SURE THAT THE<br>SHAFT ENGAGES IN<br>THE MATING PART.|Check that the shaft is<br>inserted in the mating<br>part.|
||**inside (adj) — UNNAPPROVED**|INNER (adj)|CLEAN THE INNER<br>SURFACE OF THE<br>CONTAINER.|Clean the inside surface<br>of the container.|
||**inside (n) — UNNAPPROVED**|INNER (adj)|PAINT THE INNER<br>SURFACE OF THE<br>PUMP ASSEMBLY.|Paint the inside surface<br>of the pump assembly.|
||**inside (prep) — UNNAPPROVED**|IN (prep)|THERE MUST BE<br>LUBRICANT IN THE<br>HOLE.|There must be lubricant<br>inside the hole.|
|||INTO (prep)|BEFORE YOU PUT THE<br>TOOLS INTO THE<br>STORAGE BOX, MAKE<br>SURE THAT THEY<br>HAVE THE<br>NECESSARY<br>PROTECTIVE<br>COVERS.|Before you place the<br>tools inside the storage<br>box, make sure they<br>have suitable protective<br>covers.|
||**inspect (v) — UNNAPPROVED**|EXAMINE (v)|EXAMINE ALL THE<br>DRAIN HOLES.|Inspect all the drain<br>holes.|
|||INSPECTION (n)|DO AN INSPECTION<br>OF THE WORK.|Inspect the work.|
||**INSPECTION (n)**|The procedure which<br>compares an object with<br>its standard or<br>specification|USE A VOLTMETER TO<br>DO THIS INSPECTION.|
||**INSTALL (v),**<br>**INSTALLS,**<br>**INSTALLED,**<br>**INSTALLED**|To attach an item in or to<br>a second item|INSTALL THE NEW<br>O-RINGS ON THE<br>SPINDLE.|
||**INSTALLATION (n)**|The procedure which<br>installs an item|REFER TO<br>PARAGRAPH 3 FOR<br>THE INSTALLATION OF<br>THE UNIT.|
||**instead (adv) — UNNAPPROVED**|ALTERNATIVE (n)|USE A SPATULA AS<br>AN ALTERNATIVE.|Use a spatula instead.|

**Issue 9 2025-01-15**

**Part 2 - Dictionary**
