# Page 349 of 434

**Page 2-1-R9**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
||---|---|---|---|---|
||**renew (v) — UNNAPPROVED**|NEW (adj)|USE NEW ADHESIVE<br>TAPE.|Renew the adhesive<br>tape.|
||**renovate (v) — UNNAPPROVED**|REPAIR (v)|REPAIR ALL WORN<br>SURFACES.|Renovate all worn<br>surfaces.|
|||NEW (adj)|IF THE PAINT ON THE<br>CONTROL BOX IS<br>DAMAGED, APPLY<br>NEW PAINT.|Renovate any damaged<br>paint on the control box.|
||**repack (v) — UNNAPPROVED**|PUT (v)|PUT THE ASSEMBLY<br>BACK IN THE BOX.|Repack the assembly in<br>the box.|
|||FILL (v)|FILL THE HOLE WITH<br>GREASE AGAIN.|Repack the hole with<br>grease.|
||**repaint (v) — UNNAPPROVED**|PAINT (v)|PAINT ALL THE<br>SURFACES AGAIN.|Repaint all the surfaces.|
||**REPAIR (n)**|The act of repairing or<br>the result when<br>something is repaired|AFTER THE REPAIR,<br>APPLY A PROTECTIVE<br>LAYER OF GREASE TO<br>ALL EXTERNAL<br>SURFACES.|
||**REPAIR (v),**<br>**REPAIRS,**<br>**REPAIRED,**<br>**REPAIRED**|To make an item<br>serviceable|REPAIR THE<br>DEFECTIVE WIRING.|
||**repairable (adj) — UNNAPPROVED**|REPAIR (v)|IT IS POSSIBLE TO<br>REPAIR THIS<br>DAMAGE.|This damage is<br>repairable.|
||**repeat (v) — UNNAPPROVED**|AGAIN (adv)|DO STEPS (10) THRU<br>(14) AGAIN.|Repeat steps (10) to<br>(14).|
||**repeated (adj) — UNNAPPROVED**|AGAIN AND AGAIN|IF YOU HEAR SIGNALS<br>AGAIN AND AGAIN, DO<br>A CHECK OF THE "AP<br>ENGAGE" BUTTON ON<br>THE FLIGHT MODE<br>PANEL.|If repeated signals are<br>heard, check the AP<br>ENGAGE button on the<br>flight mode panel.|
||**repeatedly (adv) — UNNAPPROVED**|AGAIN AND AGAIN|IF THE VOLTAGE<br>DECREASES AGAIN<br>AND AGAIN, ADJUST<br>THE VOLTAGE<br>REGULATOR.|If voltage drops<br>repeatedly, adjust the<br>voltage regulator.|

# Page 350 of 434

**Page 2-1-R10**

**Part 2 - Dictionary**

**Issue 9 2025-01-15**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
||---|---|---|---|---|
||**REPLACE (v),**<br>**REPLACES,**<br>**REPLACED,**<br>**REPLACED**|To remove an item and<br>to install a new or<br>serviceable item of the<br>same type|REPLACE THE RELAY.|
||**REPLACEMENT**<br>**(n)**|The item you install<br>when you replace an<br>item|MAKE SURE THAT THE<br>REPLACEMENT HAS<br>THE CORRECT<br>DIMENSIONS.|
||**replenish (v) — UNNAPPROVED**|FILL (v)|FILL THE<br>ACCUMULATOR WITH<br>OIL.|Replenish the<br>accumulator with oil.|
|||ADD (v)|ADD OIL TO THE<br>ACCUMULATOR.|Replenish the oil in the<br>accumulator.|
|||REFUEL (v)|REFUEL THE VEHICLE.|Replenish the vehicle<br>with fuel.|
||**REPORT (n)**|The information that is<br>recorded about a subject<br>or occurrence|IF THERE IS A<br>REPORT OF DAMAGE,<br>DO AN ACCURATE<br>INSPECTION.|
||**reposition (v) — UNNAPPROVED**|MOVE (v)|MOVE THE LEVER<br>BACK TO ITS INITIAL<br>POSITION.|Reposition the lever.|
|||PUT (v)|PUT THE LEVER BACK<br>TO ITS INITIAL<br>POSITION.|Reposition the lever.|
|||SET (v)|SET THE SWITCH<br>BACK TO THE OFF<br>POSITION.|Reposition the switch to<br>OFF.|
||**represent (v) — UNNAPPROVED**|SHOW (v)|THE SUCTION SHOWS<br>AS AN ALTIMETER<br>INDICATION.|The suction is<br>represented by an<br>altimeter reading.|
||**repressurize (v) — UNNAPPROVED**|PRESSURIZE (v)|PRESSURIZE THE<br>TANK AGAIN.|Repressurize the tank.|
||**request (n) — UNNAPPROVED**|TELL (v)|TELL THE FIRE<br>SERVICE TO HELP<br>YOU.|Make a request for<br>external fire support.|
|||WRITE (v)|IF AID IS NECESSARY,<br>WRITE TO THE<br>MANUFACTURER.|Any request for<br>assistance should be<br>addressed to the<br>manufacturer.|

**Issue 9 2025-01-15**

**Part 2 - Dictionary**

# Page 351 of 434

**Page 2-1-R11**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
||---|---|---|---|---|
||**request (v) — UNNAPPROVED**|TELL (v)|TELL THE FIRE<br>SERVICE TO HELP<br>YOU.|Request external fire<br>support.|
|||WRITE (v)|WRITE TO THE<br>MANUFACTURER FOR<br>REPAIR<br>INSTRUCTIONS.|Request repair<br>instructions from the<br>manufacturer.|
||**require (v) — UNNAPPROVED**|NECESSARY (adj)|DURING THIS<br>PROCEDURE, CLEAN<br>FILTERS ARE<br>NECESSARY.|During this procedure,<br>clean filters are required.|
||**reseal (v) — UNNAPPROVED**|SEAL (v)|SEAL THE CONTAINER<br>AGAIN.|<br>Reseal the container.|
||**reset (v) — UNNAPPROVED**|SET (v)|SET THE INDICATOR<br>TO A NEW POSITION.|Reset the indicator to a<br>new position.|
||**residual (adj) — UNNAPPROVED**|REMAINING (adj)|REMOVE ALL THE<br>REMAINING GREASE.|Remove all residual<br>grease.|
||**residue (n) — UNNAPPROVED**|REMAINING (adj)|REMOVE THE<br>REMAINING GREASE.|Remove the grease<br>residues.|
||**RESISTANT (adj)**|That will help to prevent<br>something|THE MATERIAL OF<br>THE SEATS IS<br>RESISTANT TO FIRE.|
||**respective (adj) — UNNAPPROVED**|RELATED (adj)|ATTACH THE CABLES<br>TO THEIR RELATED<br>SHACKLES.|Attach the cables to their<br>respective shackles.|
|||CORRECT (adj)|INSTALL THE BOLTS<br>IN THEIR CORRECT<br>POSITIONS.|Install the bolts in their<br>respective positions.|
||**respectively (adv) — UNNAPPROVED**|RELATED (adj)|ENGINES 1 AND 2<br>SUPPLY HOT AIR TO<br>THEIR RELATED<br>WINGS.|Engines 1 and 2 supply<br>the left and right wings<br>respectively with hot air.|
||**respond (v) — UNNAPPROVED**|RESULT (n)|IF THE INSTRUMENT<br>DOES NOT GIVE A<br>RESULT, DO A TEST.|If the instrument fails to<br>respond, do a test.|
||**rest (n) — UNNAPPROVED**|REMAINING (adj)|THE REMAINING<br>INSTRUCTIONS ARE<br>APPLICABLE ONLY TO<br>APPROVED<br>PERSONNEL.|The rest of these<br>instructions only apply to<br>approved personnel.|

# Page 352 of 434

**Page 2-1-R12**

**Part 2 - Dictionary**

**Issue 9 2025-01-15**

##### **ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
||---|---|---|---|---|
||**rest (v) — UNNAPPROVED**|BE (v)|THE VEHICLE MUST<br>BE ON ITS WHEELS.|The vehicle must rest on<br>its wheels.|
|||PUT (v)|PUT THE REMOVED<br>PART ON A CLEAN<br>SURFACE.|Rest the removed part<br>on a clean surface.|
||**restart (v) — UNNAPPROVED**|START (v)|START THE UNIT<br>AGAIN.|Restart the unit.|
||**restore (v) — UNNAPPROVED**|REPAIR (v)|DO NOT REPAIR THE<br>CHROMIC ACID<br>ANODIZING ON THE<br>SKIN PANEL.|Do not restore the<br>chromic acid anodizing<br>on the skin panel.|
|||PUT (v)|PUT THE PINS BACK<br>IN THEIR LOCATION.|Restore the pins to their<br>location.|
||**restrain (v) — UNNAPPROVED**|HOLD (v)|HOLD THE HOSES IN<br>POSITION.|Restrain the hoses in<br>position.|
|||STOP (v)|STOP THE FLUID<br>FLOW.|Restrain all fluid flow.|
|||PREVENT (v)|THE STOP PREVENTS<br>THE MOVEMENT OF<br>THE ROD.|The stop restrains the<br>movement of the rod.|
|||LIMIT (n)|THE VALVE KEEPS<br>THE AIRFLOW IN<br>LIMITS.|The valve restrains the<br>airflow.|
||**restrict (v) — UNNAPPROVED**|DECREASE (v)|THE METERING PLUG<br>DECREASES THE<br>FUEL FLOW.|The metering plug<br>restricts the fuel flow.|
|||PREVENT (v)|THE STOP PREVENTS<br>THE MOVEMENT OF<br>THE ROD.|The stop restricts the<br>movement of the rod.|
|||ONLY (adv)|USE THESE NUTS<br>ONLY FOR THE TEST.|Restrict the use of these<br>nuts to test only.|
|||LIMIT (n)|THE VALVE KEEPS<br>THE AIRFLOW IN<br>LIMITS.|The valve restricts the<br>airflow.|
||**RESULT (n)**|Something that occurs<br>when you do something|IF THESE TESTS DO<br>NOT GIVE THE<br>CORRECT RESULTS,<br>REPLACE THE UNIT.|

**Issue 9 2025-01-15**

**Part 2 - Dictionary**
