# Page 321 of 434

**Page 2-1-P1**

**ASD-STE100 Simplified Technical English**

|**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
|---|---|---|---|
|**particular (adj) — UNNAPPROVED**|ONLY APPLICABLE|THIS PROCEDURE IS<BR>ONLY APPLICABLE TO<BR>TYPE A PARTS.|This procedure is<BR>particular to type A parts.|
|||VERY (adv)|THIS STEP IS VERY<BR>IMPORTANT.|This step is of particular<BR>importance.|
||**particularly (adv) — UNNAPPROVED**|VERY (adv)|THIS PRECAUTION IS<BR>VERY IMPORTANT.|This precaution is<BR>particularly important.|
||**partly (adv) — UNNAPPROVED**|NOT FULLY|IF THE VALVE DOES<BR>NOT FULLY OPEN,<BR>EXAMINE THE<BR>POSITIONS OF THE<BR>END STOPS ON THE<BR>ACTUATOR.|If the valve opens only<BR>partly, examine the<BR>positions of the end<BR>stops on the actuator.|
||**pass (v) — UNNAPPROVED**|GO (v)|MAKE SURE THAT THE<BR>CABLE GOES ONTO<BR>THE PULLEY.|<BR>Make sure that the cable<BR>passes over the pulley.|
|||THROUGH (prep)|PUT THE ANTENNA<BR>CABLE THROUGH THE<BR>TOP SLOTS.|Pass the antenna cable<BR>through the top slots.|
|||GIVE (v)|GIVE ONE END OF<BR>THE CABLE TO A<BR>SECOND PERSON.|Pass one end of the<BR>cable to another person.|
||**passage (n) — UNNAPPROVED**|FLOW (n)|THE FLOW OF FLUID<BR>THROUGH THE VALVE<BR>MUST BE<BR>CONTINUOUS.|The passage of fluid<BR>through the valve must<BR>be continuous.|
|||HOLE (n)|CAREFULLY PUT THE<BR>TUBE THROUGH THE<BR>HOLE.|Carefully put the tube<BR>through the passage.|
|||OPENING (n)|CAREFULLY PUT THE<BR>TUBE THROUGH THE<BR>OPENING.|Carefully put the tube<BR>through the passage.|
||**past (prep) — UNNAPPROVED**|AROUND (prep)|IF YOU INSTALL THE<BR>SEAL INCORRECTLY,<BR>LEAKS CAN OCCUR<BR>AROUND THE VALVE.|If you install the seal<BR>incorrectly, leaks can<BR>occur past the valve.|
|||THROUGH (prep)|IF YOU INSTALL THE<BR>SEAL INCORRECTLY,<BR>THE FLUID WILL GO<BR>THROUGH IT.|An incorrect installation<BR>of the seal will let fluid go<BR>past it.|
||**PASTE (n)**|A wet, flexible mixture or<BR>compound|MIX THE MATERIALS<BR>UNTIL THEY MAKE A<BR>SOLID PASTE.|

# Page 322 of 434

**Page 2-1-P2**

**Part 2 - Dictionary**
**Issue 9 2025-01-15**
**ASD-STE100 Simplified Technical English**

|**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
|---|---|---|---|
||**PATCH (n)**|A piece of material that<BR>you use to repair a<BR>surface or hole|BOND THE PATCH TO<BR>THE TUBE WITH<BR>ADHESIVE.|
||**penetrate (v) — UNNAPPROVED**|GO THROUGH|IF THE SCRATCH<BR>DOES NOT GO<BR>THROUGH THE<BR>PROTECTIVE LAYER,<BR>THE UNIT IS<BR>SERVICEABLE.|If the scratch does not<BR>penetrate the protective<BR>layer, the unit is<BR>serviceable.|
|||GO INTO|MAKE SURE THAT THE<BR>HYDRAULIC FLUID DOES NOT GO INTO<BR>THE RECEPTACLES.|Make sure that the<BR>hydraulic fluid does not<BR>penetrate the<BR>receptacles.|
||**people (n) — UNNAPPROVED**|PERSON (n)|KEEP ALL PERSONS OUT OF THE WORK AREA.|Keep all people out of<BR>the work area.|
|||PERSONNEL (n)<BR>To select the correct<BR>alternative, refer to the approved<BR>meanings of<BR>PERSON (n) and<BR>PERSONNEL (n).|TELL YOUR<BR>PERSONNEL ABOUT<BR>THESE NEW<BR>REGULATIONS.|Tell your people about<BR>these new regulations.|
||**per (prep) — UNNAPPROVED**|FOR EACH|DO NOT USE MORE THAN TWO WASHERS FOR EACH BOLT.|Do not use more than<BR>two washers per bolt.|
|||REFER (v)|DO THE LEAK TEST:<BR>REFER TO<BR>PARAGRAPH 7.0.|Do the leak test as per<BR>paragraph 7.0.|
||**perforated (adj) — UNNAPPROVED**|HOLE (n)|MAKE SURE THAT THERE ARE NO HOLES IN THE MEMBRANE.|Make sure that the<BR>membrane is not<BR>perforated.|
||**perform (v) — UNNAPPROVED**|DO (v)|DO THE LEAK TEST.|Perform the leak test.|
|||You can use a more accurate verb.|||
|||MEASURE (v)|MEASURE THE VOLTAGE BETWEEN PINS A AND B.|Perform the voltage<BR>measurement between<BR>pins A and B.|

**Issue 9 2025-01-15**
**Part 2 - Dictionary**

# Page 323 of 434

**Page 2-1-P3**

**ASD-STE100 Simplified Technical English**

|**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
|---|---|---|---|
||**PERFORMANCE**<br>**(n)**|The ability of a part, a<BR>mechanism, or system to<BR>do its necessary function<BR>when you compare it<BR>with a standard or<BR>specification<BR>For other meanings, use:|THESE ADJUSTMENTS<BR>WILL INCREASE THE<BR>PERFORMANCE OF<BR>THE ENGINE.|
|||DO (v)|DO THE TEST. THEN, GO TO PARAGRAPH C.|After performance of the<BR>test, go to paragraph C.|
||**PERIOD (n)**|A quantity of time|THE EMERGENCY<BR>LOCATOR<BR>TRANSMITTER HAS A<BR>STANDBY PERIOD OF<BR>30 SECONDS.|
||**periodically (adv) — UNNAPPROVED**|INTERVAL (n)<BR>Give the value.|EXAMINE THE<BR>CONDITION OF THE<BR>HOSES AND SEALS AT<BR>INTERVALS OF TWO<BR>YEARS.|Examine the condition of<BR>hoses and seals<BR>periodically.|
||**PERMANENT (adj)**|Without a limit in time|MAKE SURE THAT THE<BR>PERMANENT<BR>INSTALLATION OF THE<BR>SYSTEM IS SAFE.|
||**PERMANENTLY**<br>**(adv)**|In a permanent manner|THE "NO SMOKING"<br>SIGNS WILL STAY ON<BR>PERMANENTLY.|
||**permissible (adj) — UNNAPPROVED**|PERMITTED (adj)|EQUIVALENT<BR>MATERIALS ARE ALSO<BR>PERMITTED.|Equivalent materials are<BR>also permissible.|
||**permit (v) — UNNAPPROVED**|LET (v)|DO NOT LET THE<BR>FLUID TOUCH YOU.|Do not permit the fluid to<BR>touch you.|
||**PERMITTED (adj)**|Allowed|A MAXIMUM OF TWO<BR>WASHERS IS<BR>PERMITTED FOR<BR>EACH BOLT.|
||**PERPENDICULAR**<br>**(adj)**|At a 90 degree angle to<BR>a given line or plane|MAKE SURE THAT THE<br>TOOL AND FASTENER ARE PERPENDICULAR<BR>TO THE WORK<BR>SURFACE.|

# Page 324 of 434

**Page 2-1-P4**

**Part 2 - Dictionary**
**Issue 9 2025-01-15**
**ASD-STE100 Simplified Technical English**

|**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
|---|---|---|---|
||**persist (v) — UNNAPPROVED**|CONTINUE (v)|IF THE FAULT MESSAGE CONTINUES, PUSH<BR>THE AUDIO CANCEL<BR>SWITCH ON THE TEST<BR>PANEL.|If the fault message<BR>persists, push the<BR>AUDIO CANCEL switch on the test panel.|
||**persistent (adj) — UNNAPPROVED**|CONTINUOUS (adj)|IF YOU HEAR CONTINUOUS<BR>BACKGROUND NOISE,<BR>FIND THE CAUSE.|If you hear persistent<BR>background noise, find<BR>the cause.|
||**PERSON (n)**|A human being|WHEN YOU DO WORK IN ISOLATED<BR>LOCATIONS, MAKE<BR>SURE THAT THERE IS<BR>ALWAYS A PERSON<BR>NEAR YOU.|
||**PERSONNEL (n)**|Persons employed in a<BR>group or organization|TELL YOUR<BR>PERSONNEL ABOUT<BR>THESE NEW<BR>REGULATIONS.|
||**pertinent (adj) — UNNAPPROVED**|APPLICABLE (adj)|MAKE SURE THAT<BR>YOU HAVE ALL THE<BR>APPLICABLE<BR>DOCUMENTS.|Make sure that you have<BR>all the pertinent<BR>documents.|
||**picket (v) — UNNAPPROVED**|MOOR (v)|IF STRONG WINDS<BR>OCCUR, MOOR THE BR>VEHICLE.|Picket the vehicle in<BR>strong winds.|
||**PIECE (n)**|A quantity or segment of<BR>a whole that you can use<BR>on its own, or that can<BR>operate as an individual<BR>item|<BR>REMOVE ALL PIECES<BR>OF THE BROKEN<BR>SEAL.|
||**pierced (adj) — UNNAPPROVED**|HOLE (n)|MAKE SURE THAT THERE ARE NO<BR>HOLES IN THE BR>MEMBRANE.|Make sure that the<BR>membrane is not pierced.|
||**placard (v) — UNNAPPROVED**|PUT (v)<BR>(A PLACARD [TN])|BEFORE YOU START THE TEST, PUT A<BR>PLACARD ON THE<BR> CONTROLS.|Placard the controls<BR>before you start the test.|
||**place (n) — UNNAPPROVED**|POSITION (n)|MAKE SURE THAT ALL<BR>COVERS ARE IN THEIR<BR>POSITION.|Ensure that covers are in<BR>place.|
|||AREA (n)|REPAIR THE BR>DAMAGED AREAS.|Repair the damaged<BR>places.|

**Issue 9 2025-01-15**
**Part 2 - Dictionary**
