<!-- section: DICT_G-P | pages: 265-268 | verified: true -->

# W067 — Gradient through Haul (Pages 265–268)

## Page 265 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

| gradient (n) | SLOPE (n) | WHEN YOU PARK THE | When you park the |
| --- | --- | --- | --- |
|  |  | VEHICLE ON A SLOPE, | vehicle on a gradient, |
|  |  | PUT CHOCKS ON THE | put chocks on the |
|  |  | WHEELS. | wheels. |

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **gradual (adj) — UNNAPROVED** | GRADUALLY (adv) GRADUALLY ADJUST Make a gradual THE TEMPERATURE. adjustment to the temperature. |
| **GRADUALLY (adv)** | Slowly and continuously GRADUALLY OPEN THE COCKS ON THE RECHARGING UNIT. |
| **graph (v) — UNNAPROVED** | GRAPH (TN) MAKE A GRAPH OF Graph the test results. THE TEST RESULTS. |
| **grasp (v) — UNNAPROVED** | HOLD (v) HOLD THE HANDLE. Grasp the handle. |
| **grave (adj) — UNNAPROVED** | DANGEROUS (adj) HYDRAULIC FLUID IS Hydraulic fluid can cause DANGEROUS FOR grave skin problems. YOUR SKIN. |
| **grease (v) — UNNAPROVED** | LUBRICATE (v) BEFORE YOU INSTALL Grease the O-ring before THE O-RING, installation. LUBRICATE IT WITH GREASE. GREASE (TN) APPLY GREASE TO Grease the fasteners. THE FASTENERS. |
| **great (adj) — UNNAPROVED** | LARGE (adj) AN INDICATION OF A A great amount of fuel LARGE QUANTITY OF indicates incorrect FUEL SHOWS AN setting of the float INCORRECT switch. ADJUSTMENT OF THE FLOAT SWITCH. MORE THAN IF THE PRESSURE IS If the pressure is greater MORE THAN 200 psi, than 200 psi, close the CLOSE THE VALVE. valve. |
| **VERY (adv)** | BE VERY CAREFUL Take the greatest care WHEN YOU RELEASE when you release the THE PRESSURE. pressure. |
| **greatly (adv) — UNNAPROVED** | VERY MUCH THIS METHOD CAN This method can greatly INCREASE THE RISK increase the risk of OF INJURY VERY injury. MUCH. |
| **grip (n) — UNNAPROVED** | HOLD (v) HOLD THE JACK BODY Make sure you have a TIGHTLY WHILE YOU tight grip of the jack body TURN IT. while turning it. |

## Page 266 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **grip (v) — UNNAPROVED** | HOLD (v) HOLD THE HANDLE Grip the handle lightly LIGHTLY WITH ONE with one hand. HAND. |
| **GROOVE (n)** | A long channel that is INSTALL THE O-RING not wide IN ITS GROOVE ON THE PISTON. |
| **GROUND (n)** | The surface of the earth YOU CAN ONLY DO THIS PROCEDURE ON THE GROUND. |
| **GROUND (v)** | , To connect to the ground GROUND THE FUEL GROUNDS, or to a large object of TANKS. GROUNDED, zero potential GROUNDED |
| **GROUP (n)** | Objects that are related THIS GROUP OF SEALING COMPOUNDS IS ALSO APPLICABLE IN AN EMERGENCY. |
| **grow (v) — UNNAPROVED** | BECOME (v) IF THE BATTERY If the battery grows too BECOMES TOO HOT, hot, disconnect it. DISCONNECT IT. |
| **guard (v) — UNNAPROVED** | GUARD (TN) MAKE SURE THAT THE Make sure that the GUARDS ARE switches are guarded. INSTALLED ON THE SWITCHES. |
| **guide (v) — UNNAPROVED** | PUT (v) PUT THE CABLE Guide the cable through THROUGH THE the grommet. GROMMET. |
| **MOVE (v)** | WHILE YOU LOWER As you lower the pump, THE PUMP, MOVE IT guide it onto the ONTO THE MOUNTING mounting bracket. BRACKET. |
| **gush (v) — UNNAPROVED** | FLOW (n) IF YOU TURN THE If you turn the valve HANDLE TO "FULL," handle to FULL, water THERE WILL BE A will gush from the outlet. STRONG FLOW OF WATER FROM THE OUTLET. |

## Page 267 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **halt (v) — UNNAPROVED** | STOP (v) IF YOU HEAR AN If you hear an unusual UNUSUAL NOISE, noise, halt the STOP THE procedure. PROCEDURE. |
| **halve (v) — UNNAPROVED** | HALF (TN) MAKE SURE THAT THE Check that the deviation PITCH DECREASES TO in pitch is halved. HALF ITS VALUE. |
| **hamper (v) — UNNAPROVED** | PREVENT (v) STRONG WINDS CAN Strong winds can PREVENT THE hamper the correct CORRECT deployment of the DEPLOYMENT OF THE escape slides. ESCAPE SLIDES. |
| **handle (v) — UNNAPROVED** | MOVE (v) MOVE THE ACTUATOR Handle the actuator with WITH A HOIST. a hoist. |
| **TOUCH (v)** | DO NOT TOUCH THE Do not handle the PRINTED CIRCUIT printed circuit card. CARD. |
| **USE (v)** | BE CAREFUL WHEN Be careful when you YOU USE SOLVENTS. handle solvents. |
| **CAREFUL (adj)** | BE CAREFUL WITH Handle instruments with INSTRUMENTS. care. This word can be part of a safety sign (rule 8.6). |
| **hand-tight (adj) — UNNAPROVED** | TIGHTEN … WITH INSTALL THE FILTER Install the filter case YOUR HAND CASE AND TIGHTEN IT hand-tight. WITH YOUR HAND. |
| **hand-tighten (v) — UNNAPROVED** | TIGHTEN … WITH TIGHTEN THE SWIVEL Hand-tighten the swivel YOUR HAND NUT WITH YOUR nut. HAND. |
| **HANG (v)** | , To attach or to be HANG THE SHACKLE HANGS, attached to something ON THE HOIST. HUNG, above with no support HUNG from below LOWER THE PLATFORM ASSEMBLY UNTIL IT HANGS ON THE SUPPORT FRAME. |
| **happen (v) — UNNAPROVED** | OCCUR (v) IF AN ACCIDENT If an accident happens, OCCURS, GET get medical attention. MEDICAL AID. |
| **HARD (adj)** | Not easy to cut, not easy IF THE SURFACE IS (HARDER, to go into or through HARD, USE A CARBIDE HARDEST) DRILL. |

## Page 268 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **harden (v) — UNNAPROVED** | HARD (adj) LET THE ADHESIVE Let the adhesive harden. BECOME HARD. CURE (TV) LET THE BONDING Let the bonding material MATERIAL CURE. harden. Refer to rule 1.12. |
| **harm (v) — UNNAPROVED** | INJURY (n) BE CAREFUL WHEN Be careful when you cut YOU CUT LOCKWIRE. lockwire. It can harm IT CAN CAUSE INJURY your eyes. TO YOUR EYES. IRRITATION (TN) HYDRAULIC FLUID Hydraulic fluid can harm CAN CAUSE SKIN your skin. IRRITATION. Refer to rule 1.5. |
| **harmful (adj) — UNNAPROVED** | DANGEROUS (adj) SOLVENT FUMES ARE Solvent fumes are DANGEROUS. harmful to your health. |
| **INJURY (n)** | THIS ADHESIVE This adhesive compound COMPOUND CAN is harmful to your skin. CAUSE INJURY TO YOUR SKIN. |
| **harmonize (v) — UNNAPROVED** | AGREE (v) MAKE THE POSITIONS Harmonize the positions OF THE VALVES of the valves. AGREE. |
| **ALIGN (v)** | ALIGN THE Harmonize the centerline CENTERLINE ON THE on the flux valve. FLUX VALVE. |
| **haul (v) — UNNAPROVED** | TOW (v) BEFORE YOU START Haul the hydraulic cart THE ENGINE, TOW away from the aircraft THE HYDRAULIC CART before you start the AWAY FROM THE engine. AIRCRAFT. |
| **MOVE (v)** | BEFORE YOU START Haul the hydraulic cart THE ENGINE, MOVE away from the aircraft THE HYDRAULIC CART before you start the AWAY FROM THE engine. AIRCRAFT |
