# Page 285–288 of 434

> **Source:** ASD-STE100 Issue 9, January 2025
> **Pages:** 285–288 of 434

# Page 285 of 434

**Word Approved meaning/** **<u>(part of speech) ALTERNATIVES STE EXAMPLE</u>**

**<u>Non-STE example</u>**

Blank Page

# Page 286 of 434

| **Word**<br>**(part of speech)** | **Approved meaning/**<br>**ALTERNATIVES** | **STE EXAMPLE** | **Non-STE example** |
|---|---|---|---|
| **label (v) — UNNAPPROVED** | IDENTIFY (v)<br><br>LABEL (TN) | IDENTIFY THE<br>COMPONENT WITH A<br>CODE TO HELP YOU<br>INSTALL IT AGAIN<br>CORRECTLY.<br><br>PUT A LABEL ON THE<br>RELAY ASSEMBLY. | Label the component<br>with a code to help you<br>install it again correctly.<br><br>Label the relay<br>assembly. |
| **lack (n) — UNNAPPROVED** | NOT SUFFICIENT | DAMAGE CAN OCCUR<br>TO THE PUMP IF<br>THERE IS NOT<br>SUFFICIENT OIL IN<br>THE RESERVOIR. | Damage can occur<br>to the pump if there is a<br>lack of oil in the<br>reservoir. |
| **LAMINATED (adj)** | Made of laminations | THIS PANEL IS MADE<br>OF LAMINATED<br>CARBON FIBER. |  |
| **LAMINATION (n)** | Layers of one or more<br>materials bonded<br>together | IF THE LAMINATION IS<br>DAMAGED, REPLACE<br>THE PANEL. |  |
| **land (v) — UNNAPPROVED** | LANDING (TN) | AFTER A HEAVY<br>LANDING, DO THE<br>HEAVY LANDING<br>INSPECTION. | If the aircraft landed<br>heavily, do the Heavy<br>Landing Inspection. |
| **LARGE (adj)**<br>**(LARGER,**<br>**LARGEST)** | More than average in<br>dimension, quantity, or<br>capacity | CLEAN YOUR SKIN<br>WITH A LARGE<br>QUANTITY OF CLEAN<br>WATER. |  |
| **LAST (adj)** | That comes at the end | IMMEDIATELY AFTER<br>THE LAST FLIGHT OF<br>THE DAY, INSTALL ALL<br>COVERS. |  |
| **LAST (adv)** | After other persons or<br>things | FILL THE OUTER<br>TANKS LAST. |  |
| **last (v) — UNNAPPROVED** | CONTINUE (v) | THE SIGNALS<br>CONTINUE FOR<br>0.8 SECONDS. | The signals last<br>0.8 seconds. |
| **LATCH (v),**<br>**LATCHES,**<br>**LATCHED,**<br>**LATCHED** | To hold something in<br>position with a latching<br>device | MAKE SURE THAT<br>YOU LATCH THE<br>DOOR CORRECTLY.<br><br>MAKE SURE THAT THE<br>DOOR LATCHES<br>CORRECTLY. |  |

# Page 287 of 434

| **Word**<br>**(part of speech)** | **Approved meaning/**<br>**ALTERNATIVES** | **STE EXAMPLE** | **Non-STE example** |
|---|---|---|---|
| **later (adj) — UNNAPPROVED** | SUBSEQUENT (adj)<br><br>THEN (adv) | A SUBSEQUENT<br>REPAIR WILL BE FOR<br>THE NEW<br>CONFIGURATION.<br><br>DO THIS STEP FIRST.<br>THEN, DISCONNECT<br>THE CABLES. | A later repair will be for<br>the new configuration.<br><br>Do this step first. At a<br>later time, disconnect the<br>cables. |
| **later (adv) — UNNAPPROVED** | SUBSEQUENTLY (adv)<br><br>WHEN (conj)<br>If it is possible,<br>give the condition<br>or time.<br><br>AFTER (prep) | MAKE SURE THAT THE<br>TOOL IS<br>SUBSEQUENTLY<br>AVAILABLE FOR THE<br>INSTALLATION<br>PROCEDURE.<br><br>DO STEPS (3) THRU<br>(5). DO STEP (6) WHEN<br>THE AILERON<br>MOVEMENT STOPS.<br><br>THE BAR MOVES<br>DOWN AFTER 20<br>SECONDS. | Make sure that the tool<br>is available later for the<br>installation procedure.<br><br>Do steps (3) to (5). Do<br>step (6) later.<br><br>The bar moves down<br>later. |
| **LATERAL (adj)** | Related to or on the side | ADJUST THE LATERAL<br>LEVEL. |  |
| **LATERALLY (adv)** | In a lateral direction | PUSH THE UNIT OUT,<br>AND THEN MOVE IT<br>LATERALLY. |  |
| **lay (v) — UNNAPPROVED** | PUT (v) | PUT COVERS ON THE<br>FLOOR. | Lay covers on the floor. |
| **LAYER (n)** | A material applied to a<br>surface or put on, or<br>below, a second material | APPLY A THIN LAYER<br>OF SEALING<br>COMPOUND ON THE<br>BARE METAL. |  |
| **lead (v) — UNNAPPROVED** | PUT (v) | PUT THE TELEFLEX<br>CABLE THROUGH THE<br>BULKHEAD. | Lead the Teleflex cable<br>through the bulkhead. |
| **LEAK (n)** | A crack, gap or hole<br>which lets fluid or light<br>go into or come out of<br>something | EXAMINE THE SWIVEL<br>COUPLINGS FOR<br>LEAKS. |  |

# Page 288 of 434

| **Word**<br>**(part of speech)** | **Approved meaning/**<br>**ALTERNATIVES** | **STE EXAMPLE** | **Non-STE example** |
|---|---|---|---|
| **leak (v) — UNNAPPROVED** | LEAK (n) | IF THERE ARE LEAKS<br>IN THE SYSTEM,<br>REPAIR THEM. | If the system is leaking,<br>repair it. |
| **LEAKAGE (n)** | The quantity of material<br>that goes through a leak | MEASURE THE<br>LEAKAGE FROM THE<br>OUTLET PORT. |  |
| **least (adv) — UNNAPPROVED** | MINIMUM (adj) | REPAIR THE AREA<br>WITH THE MINIMUM<br>DAMAGE FIRST. | Repair the least<br>damaged area first. |
| **least (at least)**<br>**(adv)** | MINIMUM (adj)<br><br>MINIMUM (n) | THE MINIMUM TIME<br>BETWEEN CHECKS IS<br>TWO MINUTES.<br><br>DO STEPS 13 THRU 16<br>FOR A MINIMUM OF<br>THREE TIMES. | The time between<br>checks is at least two<br>minutes.<br><br>Do steps 13 thru 16 at<br>least three times. |
| **leave (v) — UNNAPPROVED** | KEEP (v)<br><br>LET …. STAY (v)<br><br>GO (v) | KEEP THE VENT<br>VALVES OPEN.<br><br>LET THE VENT<br>VALVES STAY OPEN.<br><br>IF FUEL SPILLS ON<br>THE GROUND,<br>IMMEDIATELY GO TO<br>A SAFE AREA. | Leave the vent valves<br>open.<br><br>Leave the vent valves<br>open.<br><br>If fuel spills on the<br>ground, immediately<br>leave the contaminated<br>area. |
| **LEFT (adj)** | On the west side when<br>you look north | INSTALL THE<br>CONTROL PANEL IN<br>THE LEFT CONSOLE. |  |
| **left-hand (adj) — UNNAPPROVED** | LEFT (adj) | SET THE LEFT<br>SWITCH TO "ON." | Set the left-hand switch<br>to ON. |
| **legible (adj) — UNNAPPROVED** | READ (v) | MAKE SURE THAT<br>YOU CAN READ THE<br>IDENTIFICATION<br>PLATES. | Make certain that the<br>identification plates are<br>legible. |
| **LENGTH (n)** | 1. The distance from<br>one end to the other<br>end<br><br>2. The longer or longest<br>of the three<br>dimensions of an<br>object | MEASURE THE<br>LENGTH OF THE JACK<br>RAM.<br><br>THE DIMENSIONS OF<br>THE UNIT ARE:<br>- LENGTH      300  mm<br>- WIDTH           90  mm<br>- THICKNESS  60  mm. |  |
