# Page 281–284 of 434

> **Source:** ASD-STE100 Issue 9, January 2025
> **Pages:** 281–284 of 434

# Page 281 of 434

| Word (part of speech) | Approved meaning/ALTERNATIVES | STE EXAMPLE | Non-STE example |
|---|---|---|---|
| inward (adj) — UNNAPPROVED | INNER (adj) | MEASURE THE INNER<br>DIAMETER OF THE<br>HOLE. | Measure the inward<br>diameter of the hole. |
| inward (adv) — UNNAPPROVED | IN (adv) | MOVE THE DOOR IN<br>AND REARWARD. | Move the door inward<br>and rearward. |
| IRREGULAR (adj) | Not regular | IF THE SIGNALS ARE<br>IRREGULAR, REPLACE<br>THE UNIT. |  |
| irregularity (n) — UNNAPPROVED | DAMAGE (n)<br><br>DEFECT (TN)<br><br>IRREGULAR (adj)<br><br>UNUSUAL (adj) | THERE MUST BE NO<br>DAMAGE TO THE<br>SURFACE FINISH.<br><br>THERE MUST BE NO<br>DEFECTS IN THE<br>SURFACE FINISH.<br><br>IF YOU GET<br>IRREGULAR RESULTS,<br>DO THE TEST AGAIN.<br><br>IF YOU GET UNUSUAL<br>RESULTS, DO THE<br>TEST AGAIN. | There must be no<br>irregularities in the<br>surface finish.<br><br>There must be no<br>irregularities in the<br>surface finish.<br><br>If you get irregularities in<br>the results, do the test<br>again.<br><br>If you get irregularities in<br>the results, do the test<br>again. |
| IRREGULARLY (adv) | Not regularly | IF THE UNIT RECEIVES<br>THE SIGNALS<br>IRREGULARLY,<br>REPLACE IT. |  |
| ISOLATE (v),<br>(Is,<br>(ISOLATED,<br>(ISOLATED | To prevent a supply or<br>connection to | ISOLATE THE<br>ELECTRICAL POWER<br>SUPPLY. |  |
| isolation (n) — UNNAPPROVED | ISOLATE (v) | ISOLATE SYSTEM<br>No. 1 TO DO THE<br>LEAKAGE CHECKS. | Isolation of system No. 1<br>is necessary to do the<br>leakage checks. |
| IT (pron) | 1. That refers to a thing<br>that was previously<br>mentioned<br><br>2. That refers to an<br>explicit or implicit<br>state of affairs or<br>circumstances | CAREFULLY MOVE<br>THE DEFLECTOR UNIT<br>DOWN UNTIL IT<br>ENGAGES.<br><br>IT IS IMPORTANT TO<br>DO THIS ADJUSTMENT<br>CORRECTLY. |  |
| ITEM (n) | A thing that is<br>determined or specified | LUBRICATE THESE<br>ITEMS WITH GREASE. |  |
| ITS (adj) | Belonging to a thing | REMOVE THE UNIT<br>AND ITS WIRING. |  |

# Page 282 of 434

| Word (part of speech) | Approved meaning/ALTERNATIVES | STE EXAMPLE | Non-STE example |
|---|---|---|---|
| jack (v) — UNNAPPROVED | JACK (TN) | DO NOT LIFT THE<br>AIRCRAFT ON JACKS<br>IF THE WIND SPEED IS<br>MORE THAN 20 MPH. | Do not jack the aircraft if<br>the wind speed exceeds<br>20 mph. |
| jam (v) — UNNAPPROVED | FREELY (adv) | MAKE SURE THAT THE<br>VALVE SPINDLE<br>MOVES FREELY. | Check that the valve<br>spindle does not bind or<br>jam. |
| job (n) — UNNAPPROVED | WORK (n)<br><br>TASK (n) | DO THIS WORK IN A<br>CLEAN AREA.<br><br>DO THIS TASK IN A<br>CLEAN AREA. | Do this job in a clean<br>area.<br><br>Do this job in a clean<br>area. |
| join (v) — UNNAPPROVED | BOND (v)<br><br>ATTACH (v)<br><br>CONNECT (v) | USE ADHESIVE No. 35<br>TO BOND METAL TO<br>METAL.<br><br>ATTACH SMOKE<br>DETECTOR 1 TO<br>SMOKE DETECTOR 2.<br><br>CONNECT THE HOSE<br>TO THE PIPE WITH A<br>CLIP. | Use adhesive No. 35 to<br>join metal to metal.<br><br>Join smoke detectors 1<br>and 2.<br><br>Join the hose to the pipe<br>with a clip. |
| JOINT (n) | The area at which two<br>surfaces or edges touch<br>or are attached | SEAL THE JOINT WITH<br>SEALING COMPOUND. |  |
| just (adv) — UNNAPPROVED | IMMEDIATELY (adv) | KEEP THE RING<br>IMMEDIATELY ABOVE<br>THE JACK COLLARS. | Keep the ring just above<br>the jack collars. |

# Page 283 of 434

Blank Page

# Page 284 of 434

| Word (part of speech) | Approved meaning/ALTERNATIVES | STE EXAMPLE | Non-STE example |
|---|---|---|---|
| KEEP (v),<br>(KEEPS,<br>(KEPT,<br>(KEPT | To continue to have or<br>hold | KEEP THE<br>COMPOUND IN A<br>CLOSED CONTAINER. |  |
| key (v) — UNNAPPROVED | REFER (v)<br><br>KEY (TN) | THE ILLUSTRATION<br>REFERS TO EACH<br>STEP.<br><br>INSTALL THE KEY<br>BETWEEN THE<br>PULLEY AND THE<br>SHAFT. | The illustration will be<br>keyed to each of the<br>steps.<br><br>The pulley must be<br>keyed to the shaft. |
| KILL (v),<br>(KILLS,<br>(KILLED,<br>(KILLED | To cause death | HIGH VOLTAGES CAN<br>KILL YOU. |  |
| kind (n) — UNNAPPROVED | TYPE (n) | YOU CAN USE TWO<br>TYPES OF SEALING<br>COMPOUND. | Two kinds of sealing<br>compound can be used. |
| kink (v) — UNNAPPROVED | KINK (TN) | DO NOT MAKE KINKS<br>IN THE CABLES. | Do not kink the cables. |
| knock (v) — UNNAPPROVED | HIT (v) | HIT THE CLAMP ON<br>THE RIGHT SIDE WITH<br>A HAMMER. | Knock the clamp on the<br>right side with a hammer. |
| KNOW (v),<br>(KNOWS,<br>(KNEW,<br>(KNOWN | To be sure of data, to<br>have data ready to use | IF YOU KNOW THE<br>CLEARANCE, YOU<br>CAN CALCULATE THE<br>THICKNESS OF THE<br>WASHER. |  |
