# Page 321–324 of 434

> **Source:** ASD-STE100 Issue 9, January 2025
> **Pages:** 321–324 of 434

# Page 321 of 434

| Word (part of speech) | Approved meaning/ALTERNATIVES | STE EXAMPLE | Non-STE example |
|---|---|---|---|
| **particular (adj) — UNNAPPROVED** | ONLY APPLICABLE<br>VERY (adv) | THIS PROCEDURE IS<br>ONLY APPLICABLE TO<br>TYPE A PARTS.<br>THIS STEP IS VERY<br>IMPORTANT. | This procedure is<br>particular to type A parts.<br>This step is of particular<br>importance. |
| **particularly (adv) — UNNAPPROVED** | VERY (adv) | THIS PRECAUTION IS<br>VERY IMPORTANT. | This precaution is<br>particularly important. |
| **partly (adv) — UNNAPPROVED** | NOT FULLY | IF THE VALVE DOES<br>NOT FULLY OPEN,<br>EXAMINE THE<br>POSITIONS OF THE<br>END STOPS ON THE<br>ACTUATOR. | If the valve opens only<br>partly, examine the<br>positions of the end<br>stops on the actuator. |
| **pass (v) — UNNAPPROVED** | GO (v)<br>THROUGH (prep)<br>GIVE (v) | MAKE SURE THAT THE<br>CABLE GOES ONTO<br>THE PULLEY.<br>PUT THE ANTENNA<br>CABLE THROUGH THE<br>TOP SLOTS.<br>GIVE ONE END OF<br>THE CABLE TO A<br>SECOND PERSON. | <br>Make sure that the cable<br>passes over the pulley.<br>Pass the antenna cable<br>through the top slots.<br>Pass one end of the<br>cable to another person. |
| **passage (n) — UNNAPPROVED** | FLOW (n)<br>HOLE (n)<br>OPENING (n) | THE FLOW OF FLUID<br>THROUGH THE VALVE<br>MUST BE<br>CONTINUOUS.<br>CAREFULLY PUT THE<br>TUBE THROUGH THE<br>HOLE.<br>CAREFULLY PUT THE<br>TUBE THROUGH THE<br>OPENING. | The passage of fluid<br>through the valve must<br>be continuous.<br>Carefully put the tube<br>through the passage.<br>Carefully put the tube<br>through the passage. |
| **past (prep) — UNNAPPROVED** | AROUND (prep)<br>THROUGH (prep) | IF YOU INSTALL THE<br>SEAL INCORRECTLY,<br>LEAKS CAN OCCUR<br>AROUND THE VALVE.<br>IF YOU INSTALL THE<br>SEAL INCORRECTLY,<br>THE FLUID WILL GO<br>THROUGH IT. | If you install the seal<br>incorrectly, leaks can<br>occur past the valve.<br>An incorrect installation<br>of the seal will let fluid go<br>past it. |
| **PASTE (n)** | A wet, flexible mixture or<br>compound | MIX THE MATERIALS<br>UNTIL THEY MAKE A<br>SOLID PASTE. |  |

# Page 322 of 434

| Word (part of speech) | Approved meaning/ALTERNATIVES | STE EXAMPLE | Non-STE example |
|---|---|---|---|
| **PATCH (n)** | A piece of material that<br>you use to repair a<br>surface or hole | BOND THE PATCH TO<br>THE TUBE WITH<br>ADHESIVE. |  |
| **penetrate (v) — UNNAPPROVED** | GO THROUGH<br>GO INTO | IF THE SCRATCH<br>DOES NOT GO<br>THROUGH THE<br>PROTECTIVE LAYER,<br>THE UNIT IS<br>SERVICEABLE.<br>MAKE SURE THAT THE<br>HYDRAULIC FLUID DOES NOT GO INTO<br>THE RECEPTACLES. | If the scratch does not<br>penetrate the protective<br>layer, the unit is<br>serviceable.<br>Make sure that the<br>hydraulic fluid does not<br>penetrate the<br>receptacles. |
| **people (n) — UNNAPPROVED** | PERSON (n)<br>PERSONNEL (n)<br>To select the correct<br>alternative, refer to the approved<br>meanings of<br>PERSON (n) and<br>PERSONNEL (n). | KEEP ALL PERSONS OUT OF THE WORK AREA.<br>TELL YOUR<br>PERSONNEL ABOUT<br>THESE NEW<br>REGULATIONS. | Keep all people out of<br>the work area.<br>Tell your people about<br>these new regulations. |
| **per (prep) — UNNAPPROVED** | FOR EACH<br>REFER (v) | DO NOT USE MORE THAN TWO WASHERS FOR EACH BOLT.<br>DO THE LEAK TEST:<br>REFER TO<br>PARAGRAPH 7.0. | Do not use more than<br>two washers per bolt.<br>Do the leak test as per<br>paragraph 7.0. |
| **perforated (adj) — UNNAPPROVED** | HOLE (n) | MAKE SURE THAT THERE ARE NO HOLES IN THE MEMBRANE. | Make sure that the<br>membrane is not<br>perforated. |
| **perform (v) — UNNAPPROVED** | DO (v)<br>You can use a more accurate verb.<br>MEASURE (v) | DO THE LEAK TEST.<br>MEASURE THE VOLTAGE BETWEEN PINS A AND B. | Perform the leak test.<br>Perform the voltage<br>measurement between<br>pins A and B. |

# Page 323 of 434

| Word (part of speech) | Approved meaning/ALTERNATIVES | STE EXAMPLE | Non-STE example |
|---|---|---|---|
| **PERFORMANCE**<br>**(n)** | The ability of a part, a<br>mechanism, or system to<br>do its necessary function<br>when you compare it<br>with a standard or<br>specification<br>For other meanings, use:<br>DO (v) | THESE ADJUSTMENTS<br>WILL INCREASE THE<br>PERFORMANCE OF<br>THE ENGINE.<br>DO THE TEST. THEN, GO TO PARAGRAPH C. | After performance of the<br>test, go to paragraph C. |
| **PERIOD (n)** | A quantity of time | THE EMERGENCY<br>LOCATOR<br>TRANSMITTER HAS A<br>STANDBY PERIOD OF<br>30 SECONDS. |  |
| **periodically (adv) — UNNAPPROVED** | INTERVAL (n)<br>Give the value. | EXAMINE THE<br>CONDITION OF THE<br>HOSES AND SEALS AT<br>INTERVALS OF TWO<br>YEARS. | Examine the condition of<br>hoses and seals<br>periodically. |
| **PERMANENT (adj)** | Without a limit in time | MAKE SURE THAT THE<br>PERMANENT<br>INSTALLATION OF THE<br>SYSTEM IS SAFE. |  |
| **PERMANENTLY**<br>**(adv)** | In a permanent manner | THE "NO SMOKING"<br>SIGNS WILL STAY ON<br>PERMANENTLY. |  |
| **permissible (adj) — UNNAPPROVED** | PERMITTED (adj) | EQUIVALENT<br>MATERIALS ARE ALSO<br>PERMITTED. | Equivalent materials are<br>also permissible. |
| **permit (v) — UNNAPPROVED** | LET (v) | DO NOT LET THE<br>FLUID TOUCH YOU. | Do not permit the fluid to<br>touch you. |
| **PERMITTED (adj)** | Allowed | A MAXIMUM OF TWO<br>WASHERS IS<br>PERMITTED FOR<br>EACH BOLT. |  |
| **PERPENDICULAR**<br>**(adj)** | At a 90 degree angle to<br>a given line or plane | MAKE SURE THAT THE<br>TOOL AND FASTENER ARE PERPENDICULAR<br>TO THE WORK<br>SURFACE. |  |

# Page 324 of 434

| Word (part of speech) | Approved meaning/ALTERNATIVES | STE EXAMPLE | Non-STE example |
|---|---|---|---|
| **persist (v) — UNNAPPROVED** | CONTINUE (v) | IF THE FAULT MESSAGE CONTINUES, PUSH<br>THE AUDIO CANCEL<br>SWITCH ON THE TEST<br>PANEL. | If the fault message<br>persists, push the<br>AUDIO CANCEL switch on the test panel. |
| **persistent (adj) — UNNAPPROVED** | CONTINUOUS (adj) | IF YOU HEAR CONTINUOUS<br>BACKGROUND NOISE,<br>FIND THE CAUSE. | If you hear persistent<br>background noise, find<br>the cause. |
| **PERSON (n)** | A human being | WHEN YOU DO WORK IN ISOLATED<br>LOCATIONS, MAKE<br>SURE THAT THERE IS<br>ALWAYS A PERSON<br>NEAR YOU. |  |
| **PERSONNEL (n)** | Persons employed in a<br>group or organization | TELL YOUR<br>PERSONNEL ABOUT<br>THESE NEW<br>REGULATIONS. |  |
| **pertinent (adj) — UNNAPPROVED** | APPLICABLE (adj) | MAKE SURE THAT<br>YOU HAVE ALL THE<br>APPLICABLE<br>DOCUMENTS. | Make sure that you have<br>all the pertinent<br>documents. |
| **picket (v) — UNNAPPROVED** | MOOR (v) | IF STRONG WINDS<br>OCCUR, MOOR THE BR>VEHICLE. | Picket the vehicle in<br>strong winds. |
| **PIECE (n)** | A quantity or segment of<br>a whole that you can use<br>on its own, or that can<br>operate as an individual<br>item | <br>REMOVE ALL PIECES<br>OF THE BROKEN<br>SEAL. |  |
| **pierced (adj) — UNNAPPROVED** | HOLE (n) | MAKE SURE THAT THERE ARE NO<br>HOLES IN THE BR>MEMBRANE. | Make sure that the<br>membrane is not pierced. |
| **placard (v) — UNNAPPROVED** | PUT (v)<br>(A PLACARD [TN]) | BEFORE YOU START THE TEST, PUT A<br>PLACARD ON THE<br> CONTROLS. | Placard the controls<br>before you start the test. |
| **place (n) — UNNAPPROVED** | POSITION (n)<br>AREA (n) | MAKE SURE THAT ALL<br>COVERS ARE IN THEIR<br>POSITION.<br>REPAIR THE BR>DAMAGED AREAS. | Ensure that covers are in<br>place.<br>Repair the damaged<br>places. |
