# Page 225–228 of 434

> **Source:** ASD-STE100 Issue 9, January 2025
> **Pages:** 225–228 of 434

# Page 225 of 434

| **Word**<br>**(part of speech)** | **Approved meaning/**<br>**ALTERNATIVES** | **STE EXAMPLE** | **Non-STE example** |
|---|---|---|---|
| **ENTRY (n)** | A record of an<br>occurrence | MAKE AN ENTRY IN<br>THE LOG CARD. | |
| **EQUAL (adj)** | The same dimension,<br>quality, quantity, or<br>number | MAKE SURE THAT<br>THERE IS AN EQUAL<br>DISTANCE BETWEEN<br>THE HOLES. | |
| **equal (v) — UNNAPPROVED** | SAME (adj)<br>EQUAL (adj) | DIMENSION "X" MUST<br>BE THE SAME AS<br>DIMENSION "Z."<br>DIMENSION "X" MUST<br>BE EQUAL TO<br>DIMENSION "Y." | Dimension X must equal<br>dimension Z.<br>Dimension X must equal<br>dimension Y. |
| **EQUALLY (adv)** | The same dimension,<br>quality, quantity, or<br>number | ADJUST THE<br>TURNBUCKLES<br>EQUALLY. | |
| **equip (v) — UNNAPPROVED** | INSTALL (v) | INSTALL THE<br>SHUTOFF VALVES ON<br>EACH HP MANIFOLD. | Equip each HP manifold<br>with shutoff valves. |
| **EQUIPMENT (n)** | The objects or tools<br>used for operation and<br>maintenance | REMOVE ALL THE<br>EQUIPMENT FROM<br>THE WORK AREA. | |
| **equipped (adj) — UNNAPPROVED** | HAVE (v) | BE CAREFUL WHEN<br>YOU MOVE JET PIPES<br>OR EXHAUST CONES<br>THAT HAVE<br>INSULATING<br>BLANKETS. | Be careful when<br>handling jet pipes or<br>exhaust cones equipped<br>with insulating blankets. |
| **EQUIVALENT (adj)** | Has the same<br>properties, functions, or<br>values | MATERIALS<br>(REF. No. 2) AND<br>(REF. No. 18) ARE<br>EQUIVALENT. | |
| **EQUIVALENT (n)** | Something that has the<br>same properties,<br>functions, or values | USE CLEANING<br>COMPOUND ARDROX<br>6025, OR AN<br>EQUIVALENT. | |
| **ERASE (v),**<br>**ERASES,**<br>**ERASED,**<br>**ERASED** | To remove data from a<br>medium | ERASE THE TAPE. | |

# Page 226 of 434

| **Word**<br>**(part of speech)** | **Approved meaning/**<br>**ALTERNATIVES** | **STE EXAMPLE** | **Non-STE example** |
|---|---|---|---|
| **erect (v) — UNNAPPROVED** | ASSEMBLE (v)<br>BECOME STABLE | BEFORE YOU LIFT THE<br>GEARBOX, ASSEMBLE<br>THE MOVABLE HOIST.<br>LET THE VERTICAL<br>GYRO BECOME<br>STABLE. | Erect the movable hoist<br>before lifting the<br>gearbox.<br>Give the vertical gyro<br>time to erect. |
| **erratic (adj) — UNNAPPROVED** | IRREGULAR (adj) | THE OPERATION OF<br>THE COMPASS IS<br>IRREGULAR. | The compass is erratic. |
| **ERROR (n)** | The difference from that<br>which is correct or<br>accurate | IF THE ERROR IS<br>MORE THAN 3 DEG.,<br>CALIBRATE THE<br>COMPASS. | |
| **escape (v) — UNNAPPROVED** | DEFLATE (v)<br>RELEASE (v) | DEFLATE THE TIRE.<br>RELEASE ALL THE<br>NITROGEN. | Let the air escape from<br>the tire.<br>Allow all the nitrogen to<br>escape. |
| **establish (v) — UNNAPPROVED** | MAKE SURE (v) | IN THE STEP THAT<br>FOLLOWS, MAKE<br>SURE THAT THE FUEL<br>PUMP OPERATES<br>CORRECTLY. | In the following step,<br>establish the correct<br>functioning of the fuel<br>pump. |
| **ESTIMATE (n)** | A calculated,<br>approximate result | MAKE AN ESTIMATE<br>OF THE NECESSARY<br>QUANTITY OF PAINT. | |
| **estimate (v) — UNNAPPROVED** | ESTIMATE (n) | MAKE AN ESTIMATE<br>OF THE QUANTITY OF<br>CLEANING FLUID THAT<br>IS NECESSARY. | Estimate the amount of<br>cleaning fluid that is<br>necessary. |
| **evaluate (v) — UNNAPPROVED** | EXAMINE (v)<br>ANALYSIS (TN) | EXAMINE THE<br>DAMAGE AFTER AN<br>ACCIDENT.<br>MAKE AN ANALYSIS<br>OF THE TEST<br>RESULTS. | Evaluate the damage<br>after an accident.<br>Evaluate the test results. |

# Page 227 of 434

| **Word**<br>**(part of speech)** | **Approved meaning/**<br>**ALTERNATIVES** | **STE EXAMPLE** | **Non-STE example** |
|---|---|---|---|
| **evaluation (n) — UNNAPPROVED** | EXAMINE (v)<br>ANALYSIS (TN) | EXAMINE THE<br>DAMAGE.<br>MAKE AN ANALYSIS<br>OF THE TEST<br>RESULTS. | Do an evaluation of the<br>damage.<br>Do an evaluation of the<br>test results. |
| **evaporate (v) — UNNAPPROVED** | DRY (v) | LET THE COMPOUND<br>DRY. | Allow the solvent to<br>evaporate from the<br>compound. |
| **even (adj) — UNNAPPROVED** | SMOOTH (adj)<br>SAME (adj)<br>FLAT (adj)<br>FLUSH (adj)<br>LEVEL (adj) | A GUIDE ROD IS<br>ATTACHED TO THE<br>METAL BELLOWS<br>DISC FOR A SMOOTH<br>MOVEMENT OF THE<br>BELLOWS.<br>APPLY THE SAME<br>LOAD ON THE TWO<br>BRAKES.<br>MAKE SURE THAT<br>THE SURFACE IS<br>FLAT.<br>MAKE SURE THAT<br>THE FASTENER<br>HEADS ARE FLUSH<br>WITH THE SKIN.<br>MAKE SURE THAT<br>THE MARK ON THE<br>BOLT IS LEVEL WITH<br>THE MARK ON THE<br>HANDLE. | A guide rod is attached<br>to the metal bellows disc<br>for an even movement of<br>the bellows.<br>Braking must be even on<br>the two brakes.<br>Ensure the surface is<br>even.<br>Make sure that the<br>fastener heads are even<br>with the skin.<br>Make sure that the mark<br>on the bolt is even with<br>the mark on the handle. |
| **evenly (adv) — UNNAPPROVED** | GRADUALLY (adv)<br>EQUALLY (adv) | INCREASE THE<br>TEMPERATURE<br>GRADUALLY.<br>APPLY THE LOAD<br>EQUALLY ON THE<br>AREA. | Increase the<br>temperature evenly.<br>Apply the load evenly on<br>the area. |
| **event (n) — UNNAPPROVED** | IF (conj) | IF THE PRESSURE<br>DECREASES<br>SUDDENLY, CLOSE<br>THE VALVE. | In the event of a sudden<br>dropping of pressure,<br>close the valve. |
| **eventually (adv) — UNNAPPROVED** | SOME TIME | IF THE CABLE RUBS,<br>IT WILL BREAK AFTER<br>SOME TIME. | If the cable chafes, it will<br>eventually break. |

# Page 228 of 434

| **Word**<br>**(part of speech)** | **Approved meaning/**<br>**ALTERNATIVES** | **STE EXAMPLE** | **Non-STE example** |
|---|---|---|---|
| **every (adj) — UNNAPPROVED** | ALL (adj)<br>EACH (adj)<br>INTERVAL (n) | REMOVE ALL SAFETY<br>PINS BEFORE FLIGHT.<br>SET THE BTRY<br>SWITCH TO "ON"<br>EACH TIME.<br>DO AN INSPECTION<br>AT INTERVALS OF<br>20 000 FLIGHT<br>HOURS. | Every safety pin must be<br>removed before flight.<br>It is necessary to set the<br>BTRY switch to ON<br>every time.<br>Do an inspection every<br>20 000 flight hours. |
| **evidence (n) — UNNAPPROVED** | INDICATION (n)<br>SIGN (n) | IF THERE IS AN<br>INDICATION OF A<br>LEAK, REPLACE THE<br>VALVE.<br>ONE SIGN OF A LEAK<br>OF HOT AIR FROM A<br>JOINT IS THAT THE<br>TEMPERATURE<br>INDICATION<br>DECREASES. | If there is evidence of a<br>leak, replace the valve.<br>Evidence of a leak of hot<br>air from a joint is that the<br>temperature reading<br>drops. |
| **evidence (v) — UNNAPPROVED** | SHOW (v)<br>FIND (v) | IF THE TEST SHOWS<br>NO FAULT, CONTINUE<br>THE PROCEDURE.<br>IF YOU DO NOT FIND<br>DAMAGE DURING THE<br>INSPECTION<br>PROCEDURE,<br>ASSEMBLE THE UNIT. | If no fault is evidenced<br>by the test, continue the<br>procedure.<br>If the inspection does<br>not evidence any<br>damage, assemble the<br>unit. |
| **evident (adj) — UNNAPPROVED** | FIND (v) | IF YOU DO NOT FIND<br>DAMAGE, CONTINUE<br>THE INSPECTION. | If no damage is evident,<br>continue the inspection. |
| **exact (adj) — UNNAPPROVED** | ACCURATE (adj)<br>CORRECT (adj) | IF THE INDICATION IS<br>NOT ACCURATE, DO<br>THE TEST AGAIN.<br>IF THE INDICATION IS<br>NOT CORRECT, DO<br>THE TEST AGAIN. | If the indication is not<br>exact, do the test again.<br>If the indication is not<br>exact, do the test again. |
