<!-- section: DICT_G-P | pages: 281-284 | verified: true -->

# Page 281 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

|| Word (POS) | Meaning & Examples |
||------------|-------------------|
|| **incomplete (adj) — UNNAPROVED** | NOT FULL IF THE ACTUATOR If the actuator travel is TRAVEL IS NOT FULL, incomplete, readjust the ADJUST THE RODS rods. AGAIN. NOT COMPLETED IF THE ADJUSTMENT If the adjustment is IS NOT COMPLETED, incomplete, the values THE VALUES SHOWN shown on the indicator ON THE INDICATOR will be incorrect. WILL BE INCORRECT. |
|| **ALL (adj)** | IF YOU DO NOT HAVE If the results are ALL THE RESULTS, DO incomplete, do the test THE TEST AGAIN. again. |
|| **incorporate (v) — UNNAPROVED** | INCLUDE (v) ALL MODELS INCLUDE All models incorporate a A MICROPROCESSOR microprocessor control CONTROL UNIT. unit. |
|| **HAVE (v)** | SOME RELAYS HAVE A Some relays incorporate POTENTIOMETER. a potentiometer. |
|| **incorporation (n) — UNNAPROVED** | INCLUDE (v) THE MANUFACTURER Incorporation of a INCLUDED A SECOND second diode increased DIODE TO INCREASE the reliability of the THE RELIABILITY OF motor. THE MOTOR. |
|| **INCORRECT (adj)** | Not correct IF THE TRIM TAB ADJUSTMENT IS INCORRECT, DO STEPS 7 THRU 10. INCORRECTLY In an incorrect manner IF YOU SEE THE RED (adv) MARK, THE PART IS INSTALLED INCORRECTLY. |

# Page 282 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

|| Word (POS) | Meaning & Examples |
||------------|-------------------|
|| **increase (n) — UNNAPROVED** | INCREASE (v) THE TEMPERATURE There must be an MUST INCREASE. increase in temperature. |
|| **INCREASE (v)** | , To make or become INCREASE THE VANE INCREASES, larger or higher in value ANGLE TO INCREASED, 90 DEGREES. INCREASED MAKE SURE THAT THE TEMPERATURE INCREASES TO 30 °C. |
|| **INCREMENT (n)** | One of a sequence of ADJUST THE STOP regular operations done BOLT IN INCREMENTS one after the other, to OF 5 mm. increase or decrease an adjustable quantity |
|| **incur (v) — UNNAPROVED** | CAUSE (v) REMOVAL OF THE Removal of the unit UNIT BEFORE before 24 hours can 24 HOURS CAN CAUSE incur damage. DAMAGE. |
|| **independent (adj) — UNNAPROVED** | INDEPENDENTLY (adv) THIS UNIT OPERATES The operation of this unit INDEPENDENTLY. is independent. INDEPENDENTLY Without a relation with THE EMERGENCY (adv) SYSTEM IS CONTROLLED INDEPENDENTLY. |
|| **indicate (v) — UNNAPROVED** | SHOW (v) THE POINTER SHOWS The pointer indicates ZERO FEET. zero feet. |
|| **IDENTIFY (v)** | A 406 MHz DIGITAL A 406 MHz digital signal SIGNAL IDENTIFIES indicates the emergency THE EMERGENCY locator transmitter and LOCATOR its location. TRANSMITTER AND ITS LOCATION. |
|| **SPECIFIED (adj)** | IF TOLERANCES ARE If tolerances are not NOT SPECIFIED, indicated, refer to REFER TO GENERAL general tolerance TOLERANCE VALUES. values. |
|| **INDICATION (n)** | Something that is shown MAKE SURE THAT THE INDICATION IS CORRECT. |
|| **induce (v) — UNNAPROVED** | CAUSE (v) SCRATCHES IN THE Scratches in the WINDSCREEN CAN windscreen may induce CAUSE CRACKS. cracks. |

# Page 283 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

|| Word (POS) | Meaning & Examples |
||------------|-------------------|
|| **ineffective (adj) — UNNAPROVED** | UNSERVICEABLE (adj) IF THE PUMP IS If the pump is ineffective, UNSERVICEABLE, replace it. REPLACE IT. UNSATISFACTORY IF THE OPERATION OF If the operation of the (adj) THE PUMP IS pump is ineffective, UNSATISFACTORY, replace it. REPLACE IT. NOT OPERATE IF THE PUMP DOES If the pump is ineffective, NOT OPERATE replace it. CORRECTLY, REPLACE IT. |
|| **inflammable (adj) — UNNAPROVED** | FLAMMABLE (adj) SOLVENT IS VERY Solvent is highly FLAMMABLE. inflammable. |
|| **INFLATE (v)** | , To make or become INFLATE THE TIRES INFLATES, larger as a result of WITH NITROGEN. INFLATED, pressurization by a gas INFLATED OPERATION OF THE HANDLE RELEASES THE GAS, AND THE SLIDE-RAFT INFLATES. |
|| **inform (v) — UNNAPROVED** | TELL (v) TELL THE Inform the manufacturer MANUFACTURER about the problem. ABOUT THE PROBLEM. |
|| **INFORMATION (n)** | Data collected and made THIS MANUAL available for a specified CONTAINS function INFORMATION ABOUT MAINTENANCE PROCEDURES. |
|| **ingest (v) — UNNAPROVED** | SWALLOW (v) IF YOU SWALLOW If you ingest hydraulic HYDRAULIC FLUID, fluid, get medical aid GET MEDICAL AID immediately. IMMEDIATELY. |
|| **ingress (n) — UNNAPROVED** | GO INTO IF WATER GOES INTO Water ingress will THE COMPONENT, damage the component. DAMAGE WILL OCCUR. |

# Page 284 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

|| Word (POS) | Meaning & Examples |
||------------|-------------------|
|| **inhale (v) — UNNAPROVED** | BREATHE (v) DO NOT BREATHE Do not inhale the solvent THE SOLVENT FUMES. fumes. |
|| **inhibit (v) — UNNAPROVED** | PREVENT (v) ALODINE PREVENTS Alodine inhibits CORROSION. corrosion. |
|| **INITIAL (adj)** | That is related to the MOVE THE LEVER start BACK TO ITS INITIAL POSITION. |
|| **INITIALLY (adv)** | At the start INITIALLY, THE SPEED INCREASES TO 3000 RPM. |
|| **initiate (v) — UNNAPROVED** | START (v) START THE TEST AT Initiate the test at 2000 RPM. 2000 rpm. |
|| **inject (v) — UNNAPROVED** | PUT (v) PUT OIL INTO THE Inject oil into the gearbox GEARBOX WITH A with a syringe. SYRINGE. |
|| **injection (n) — UNNAPROVED** | PUT (v) PUT THE CORROSION The injection of the PREVENTIVE OIL INTO corrosion preventive oil THE PUMP WITH A into the pump must be SYRINGE. done with a syringe. |
|| **injure (v) — UNNAPROVED** | INJURY (n) MAKE SURE THAT THE Make sure that the end END OF THE SAFETY of the safety wire will not WIRE WILL NOT injure persons. CAUSE INJURY TO PERSONS. |
|| **INJURY (n)** | Damage to a person BEND THE ENDS OF THE LOCKING WIRE TO PREVENT INJURY. |
|| **INNER (adj)** | Nearer to the center of THE INNER SURFACE an object OF THE PART IS BLACK. |
|| **inoperative (adj) — UNNAPROVED** | OFF (adj) BEFORE YOU DRAIN Before you drain the THE FUEL, MAKE fuel, make sure that the SURE THAT THE system is inoperative. SYSTEM IS OFF. NOT OPERATE MAKE SURE THAT THE Make sure that the DEMISTING SYSTEM demisting system is DOES NOT OPERATE. inoperative. |
|| **INPUT (n)** | The data, power, or THE UNIT COMPARES energy put into THE INPUTS FROM equipment or a system THE TWO SENSORS TO THE COMPUTER. |
