# Page 329 of 434

**Page 2-1-P9**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
||---|---|---|---|
||**PREPARE (v),**<br>**PREPARES,**<br>**PREPARED,**<br>**PREPARED**|To make or become<br>ready|PREPARE THE TUBE<br>FOR THE LEAK TEST.|
||||PREPARE FOR THE<br>ELECTRICAL BONDING<br>PROCEDURE.|
||**prescribed (adj) — UNNAPPROVED**|SPECIFIED (adj)|FILL THE CONTAINER<br>WITH THE SPECIFIED<br>COOLANT FLUID.|Fill the container with the<br>prescribed coolant fluid.|
||**presence (n) — UNNAPPROVED**|BE (v)|THIS INSPECTION IS<br>NECESSARY WHEN<br>THERE ARE DEFECTS.|This inspection is<br>necessary in the<br>presence of defects.|
||**present (adj) — UNNAPPROVED**|BE (v)|IF THERE IS A<br>VOLTAGE AT PIN C OF<br>CONNECTOR F7, THE<br>UNIT IS<br>UNSERVICEABLE.|If a voltage is present at<br>pin C of connector F7,<br>the unit is faulty.|
||**present (v) — UNNAPPROVED**|GIVE (v)|THIS SECTION GIVES<br>THE APPLICABLE<br>TORQUE VALUES.|The applicable torque<br>values are presented in<br>this section.|
|||SHOW (v)|THE TABLE THAT<br>FOLLOWS SHOWS<br>THE RESULTS OF THE<br>SURVEY.|The results of the survey<br>are presented in the<br>following table.|
||**preserve (v) — UNNAPPROVED**|PRESERVATION (TN)|THIS PROCEDURE IS<br>FOR THE<br>PRESERVATION OF<br>STEEL CABLES.|This procedure will<br>preserve the steel cables.|
||**preset (v) — UNNAPPROVED**|SET (v)|SET THE TENSION<br>INDICATOR TO ZERO.|Preset the tension<br>indicator to zero.|
||**press (v) — UNNAPPROVED**|PUSH (v)|PUSH AND HOLD THE<br>TEST BUTTON.|Press and hold the TEST<br>button.|
||**PRESSURIZATION**<br>**(n)**|The procedure that<br>supplies or increases<br>the pressure|CONTINUE THE<br>PRESSURIZATION<br>FOR 10 MINUTES.|
||**PRESSURIZE (v),**<br>**PRESSURIZES,**<br>**PRESSURIZED,**<br>**PRESSURIZED**|To supply pressure|PRESSURIZE THE<br>CHAMBER TO 150 psi.|

# Page 330 of 434

**Page 2-1-P10**

**Part 2 - Dictionary**

**Issue 9 2025-01-15**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
||---|---|---|---|
||**PREVENT (v),**<br>**PREVENTS,**<br>**PREVENTED,**<br>**PREVENTED**|To make sure that<br>something does not<br>occur|TO PREVENT DAMAGE<br>TO THE ENGINE,<br>IMMEDIATELY INSTALL<br>PROTECTIVE COVERS<br>ON ALL OPENINGS.|
||**prevent (from) (v)**|LET (v)|DO NOT LET THE<br>DOOR OPEN.|Prevent the door from<br>opening.|
||**preventive (adj) — UNNAPPROVED**|PREVENT (v)|THIS COATING<br>PREVENTS<br>CORROSION.|This coating is a<br>preventive measure for<br>corrosion.|
||**PREVIOUS (adj)**|That goes before in an<br>unspecified time or<br>sequence|IF YOU SELECTED<br>"YES" IN A PREVIOUS<br>STEP, GO TO<br>PARAGRAPH 7.5.|
|||Be accurate.<br>Use LAST (adj)<br>for the event that<br>occurs<br>immediately<br>before in time or<br>sequence.|DO THE LAST<br>INSPECTION AGAIN.|Do the previous<br>inspection again.|
||**PREVIOUSLY (adv)**|Before, earlier, in the<br>past|THIS SOFTWARE<br>FINDS TERMS FROM<br>PREVIOUSLY<br>TRANSLATED FILES.|
||**primarily (adv) — UNNAPPROVED**|PRIMARY (adj)|THE PRIMARY<br>FUNCTION OF THE<br>HYDRAULIC SYSTEM<br>IS TO SUPPLY THE<br>PRESSURE TO<br>OPERATE THE FLIGHT<br>CONTROLS.|The hydraulic system<br>primarily supplies the<br>pressure to operate the<br>flight controls.|
||**PRIMARY (adj)**|First in importance|THE PRIMARY<br>FUNCTION OF THE<br>POWER UNIT IS TO<br>SUPPLY ELECTRICAL<br>POWER.|
||**prime (v) — UNNAPPROVED**|FILL (v)|FILL THE FILLER HOSE<br>WITH WATER.|Prime the filler hose with<br>water.|

|||PUT (v)|PUT FUEL IN THE<br>FUEL PUMP.|Prime the fuel pump.

# Page 331 of 434

**Page 2-1-P11**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
||---|---|---|---|
||**principal (adj) — UNNAPPROVED**|PRIMARY (adj)|THE PRIMARY<br>FUNCTION OF THE<br>SYSTEM IS TO SUPPLY<br>ELECTRICAL POWER<br>TO THE CONTROL<br>PANEL.|The principal function of<br>the system is to supply<br>electrical power to the<br>control panel .|
||**prior to (prep) — UNNAPPROVED**|BEFORE (conj)|BEFORE YOU<br>DISCONNECT THE<br>HOSES, DRAIN THE<br>SYSTEM.|Drain the system prior to<br>disconnecting the<br>hoses.|
||**priority (n) — UNNAPPROVED**|IMPORTANT (adj)|THIS PROCEDURE IS<br>VERY IMPORTANT.|This procedure has high<br>priority.|
||**|**BEFORE (prep)|BEFORE YOU FILL THE<br>OUTER TANK, FILL THE<br>INNER TANK.|The inner tank filling<br>procedure has priority<br>over the outer tank filling<br>procedure.|
||**|FIRST (adv)|DURING THE<br>PROCEDURE THAT<br>FOLLOWS, REPAIR THE<br>UPPER FLANGE FIRST.|
|During the following<br>repair procedure, the<br>upper flange has priority.|
||**probability (n) — UNNAPPROVED**|RISK (n)|TO DECREASE THE<br>RISK OF FIRE, OBEY<br>THE SAFETY<br>PRECAUTIONS.|Obey the safety<br>precautions to decrease<br>the probability of fire.|
||**probable (adj) — UNNAPPROVED**|VERY POSSIBLE|IF YOU DO NOT<br>SAFETY THE DOOR, IT<br>IS VERY POSSIBLE<br>THAT STRONG WINDS<br>WILL CAUSE DAMAGE<br>TO THE STRUCTURE.|If you do not safety the<br>door, damage to the<br>structure due to strong<br>winds is probable.|
||**|RISK (n)|IF YOU DO NOT<br>SAFETY THE DOOR,<br>THERE IS A RISK THAT<br>STRONG WINDS WILL<br>CAUSE DAMAGE TO<br>THE STRUCTURE.|If you do not safety the<br>door, damage to the<br>structure due to strong<br>winds is probable.|
||**probe (v) — UNNAPPROVED**|FIND (v)<br>(WITH A PROBE [TN])|FIND THE BLOCKAGE<br>IN THE TUBE WITH AN<br>APPLICABLE PROBE.|Probe the tube to find<br>the blockage.|
||**PROBLEM (n)**|Something that is difficult<br>and for which you must<br>find the correct answer|<br>IF YOU FIND A<br>PROBLEM DURING THE<br>TEST, REFER TO THE<br>FAULT ISOLATION<br>TABLE.|

# Page 332 of 434

**Page 2-1-P12**

**Part 2 - Dictionary**

**Issue 9 2025-01-15**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
||---|---|---|---|
||**PROCEDURE (n)**|Steps that are in a<br>sequence|THIS SECTION GIVES<br>THE PROCEDURE TO<br>DISASSEMBLE THE<br>COMPONENT FULLY.|
||**proceed (v) — UNNAPPROVED**|CONTINUE (v)|CONTINUE WITH THE<br>ELECTRICAL TEST.|Proceed with the<br>electrical test.|
||**process (in the**<br>**process of ) (prep)**|DURING (prep)|DURING THIS REPAIR,<br>APPLY SUFFICIENT<br>HEAT TO THE UNIT.|Apply sufficient heat to<br>the unit in the process of<br>doing this repair.|
||**|WHILE (conj)|WHILE YOU DO THIS<br>REPAIR, APPLY<br>SUFFICIENT HEAT TO<br>THE UNIT.|Apply sufficient heat to<br>the unit in the process of<br>doing this repair.|
||**process (n) — UNNAPPROVED**|PROCEDURE (n)|THESE TWO<br>ASSEMBLY<br>PROCEDURES ARE<br>ALMOST THE SAME.|These two assembly<br>processes are almost<br>the same.|
||**|This word is a<br>technical noun<br>when it means a<br>sequence of<br>changes that<br>occur and cause<br>a result.|CORROSION IS AN<br>ELECTROLYTIC<br>PROCESS.|
||**process (v) — UNNAPPROVED**|DO (v) THE …<br>PROCEDURE (n)|PUT THE PARTS IN AN<br>ELECTROLYTIC BATH.<br>THEN, DO THE<br>ELECTROPLATING<br>PROCEDURE.|Process the parts in an<br>electrolytic bath.|
||**produce (v) — UNNAPPROVED**|CAUSE (v)|ELECTRICAL<br>EQUIPMENT CAN<br>CAUSE<br>INTERFERENCE IN<br>COMMUNICATION.|Electrical equipment can<br>produce interference in<br>communication.|
||**|GIVE (v)|A DILUTED SOLUTION<br>WILL NOT GIVE YOU<br>THE CORRECT<BR>RESULTS.|A diluted solution does<br>not produce the correct<br>results.|
||**|MAKE (v)|WHEN THE LEVER<br>ENGAGES, IT MAKES A<br>CLICK|The lever produces a<br>click when engaged.|

||**|SUPPLY (v)|THE POWER UNIT<br>SUPPLIES THE<br>SYSTEM WITH A<br>VOLTAGE OF 28 V DC.|The power unit produces<br>a voltage of 28 V DC.
