# Page 397–400 of 434

> **Source:** ASD-STE100 Issue 9, January 2025
> **Pages:** 397–400 of 434

# Page 397 of 434

| **Word**<br>**(part of speech)** | **Approved meaning/**<br>**ALTERNATIVES** | **STE EXAMPLE** | **Non-STE example** |
|---|---|---|---|
| **TOGETHER (adv)** | In one group or position<br>For other<br>meanings, use: | USE TAPE TO ATTACH<br>THE CABLES<br>TOGETHER. |  |
| **AT THE SAME TIME** | DISASSEMBLE THE<br>BYPASS VALVE AND<br>THE DUMP VALVE AT<br>THE SAME TIME. | Disassemble the bypass<br>valve and the dump<br>valve together. |  |
| **TOLERANCE (n)** | A permitted difference<br>from a standard | THE TOLERANCE IS<br>PLUS OR MINUS<br>0.2 mm. |  |
| **TOO (adv)** | More than is necessary<br>or correct | MAKE SURE THAT THE<br>TEMPERATURE IS<br>NOT TOO HIGH. |  |
| **TOOL (n)** | An object used to make<br>or do something | REMOVE ALL TOOLS<br>AND EQUIPMENT. |  |
| **TOP (adj)** | That is uppermost | A NUMBER IN THE<br>TOP LEFT CORNER OF<br>THE DISPLAY REFERS<br>TO A RELATED PAGE. |  |
| **TOP (n)** | The uppermost position | THE VERTICAL<br>STABILIZER IS<br>INSTALLED ON THE<br>TOP OF THE<br>FUSELAGE TAIL<br>SECTION. |  |
| **top off (v) — UNNAPPROVED** | FILL (v)<br>ADD (v) | FILL THE HYDRAULIC<br>SYSTEM AS<br>NECESSARY.<br>ADD FLUID TO THE<br>HYDRAULIC<br>RESERVOIR AS<br>NECESSARY. | Top off the hydraulic<br>system as necessary.<br>Top off the hydraulic<br>reservoir as necessary. |
| **TORQUE (v),**<br>**TORQUES,**<br>**TORQUED,**<br>**TORQUED** | To tighten to a specified<br>torque | TORQUE THE PLUG<br>TO 6 Nm. |  |
| **TOTAL (adj)** | All of | THE TOTAL QUANTITY<br>OF FUEL IN THE<br>CENTER TANK IS<br>5000 lb. |  |

# Page 398 of 434

| **Word**<br>**(part of speech)** | **Approved meaning/**<br>**ALTERNATIVES** | **STE EXAMPLE** | **Non-STE example** |
|---|---|---|---|
| **TOTAL (n)** | The full quantity | ADD THE VALUES.<br>THE TOTAL MUST NOT<br>BE MORE THAN<br>15 mm. |  |
| **TOUCH (v),**<br>**TOUCHES,**<br>**TOUCHED,**<br>**TOUCHED** | To be in contact | MAKE SURE THAT THE<br>LOCK NUT TOUCHES<br>THE SPRING. |  |
| **TOW (v),**<br>**TOWS,**<br>**TOWED,**<br>**TOWED** | To pull something along | BEFORE YOU TOW<br>THE VEHICLE BACK<br>TO ITS INITIAL<br>POSITION, COMPLETE<br>THE PROCEDURE |  |
| **toward (prep) — UNNAPPROVED** | TO (prep)<br>DIRECTION (n) | THE ARROW MUST<br>POINT TO THE REAR.<br>MANUALLY PUSH THE<br>RAM AIR TURBINE IN<br>THE DIRECTION OF<br>THE RETRACTED<br>POSITION. | The arrow must point<br>toward the rear.<br>Manually push the Ram<br>Air Turbine toward the<br>retracted position. |
| **toxic (adj) — UNNAPPROVED** | POISONOUS (adj) | THIS COMPOUND IS<br>POISONOUS. | This compound is toxic. |
| **trace (n) — UNNAPPROVED** | SIGN (n) | EXAMINE THE AREA<br>AROUND THE DRAIN<br>HOLES FOR SIGNS OF<br>CORROSION. | Check the area<br>surrounding the drain<br>holes for traces of<br>corrosion. |
| **trace (v) — UNNAPPROVED** | FIND (v) | FIND THE BROKEN<br>WIRE. | Trace the broken wire. |
| **track (v) — UNNAPPROVED** | MONITOR (v) | MONITOR THE<br>TEMPERATURE. | Track the temperature. |
| **trained (adj) — UNNAPPROVED** | APPROVED (adj) | ONLY APPROVED<br>PERSONNEL CAN<br>OPERATE THE<br>BRAKES. | Only trained personnel<br>can operate the brakes. |

# Page 399 of 434

| **Word**<br>**(part of speech)** | **Approved meaning/**<br>**ALTERNATIVES** | **STE EXAMPLE** | **Non-STE example** |
|---|---|---|---|
| **transfer (n) — UNNAPPROVED** | MOVEMENT (n)<br>SUPPLY (n) | MAKE SURE THAT THE<br>RATE OF MOVEMENT<br>OF FUEL FROM THE<br>WING TANKS TO THE<br>CENTER TANK IS<br>EQUAL.<br>MAKE SURE THAT THE<br>RATE OF SUPPLY OF<br>FUEL FROM THE WING<br>TANKS TO THE<br>CENTER TANK IS<br>EQUAL. | <br>Make sure the rate of<br>fuel transfer from the<br>wing tanks to the center<br>tank is equal.<br> <br>Make sure the rate of<br>fuel transfer from the<br>wing tanks to the center<br>tank is equal. |
| **transfer (v) — UNNAPPROVED** | MOVE (v)<br>INSTALL (v) | MOVE THE<br>COUPLINGS TO THE<br>NEW UNIT.<br>INSTALL THE<br>COUPLINGS ON THE<br>NEW UNIT. | The couplings must be<br>transferred to the new<br>unit.<br>Transfer the couplings to<br>the new unit. |
| **transition (n) — UNNAPPROVED** | CHANGE (n) | THE CHANGE FROM<br>FULL-RATE<br>OPERATION TO<br>HALF-RATE<br>OPERATION MUST<br>OCCUR IMMEDIATELY. | The transition from full-<br>rate operation to half-<br>rate operation must<br>occur immediately. |
| **TRANSMIT (v),**<br>**TRANSMITS,**<br>**TRANSMITTED,**<br>**TRANSMITTED** | To send energy or a<br>signal | MAKE SURE THAT THE<br>TRANSPONDER<br>TRANSMITS THE<br>SIGNAL CORRECTLY. |  |
| **TRANSPARENT**<br>**(adj)** | Easy to see through | PUT A TRANSPARENT<br>SHEET OF PLASTIC<br>ON THE SURFACE. |  |
| **transport (v) — UNNAPPROVED** | SEND (v) | SEND THE PART TO<br>THE OVERHAUL<br>SHOP. | Transport the part to the<br>overhaul shop. |
| **trapped (adj) — UNNAPPROVED** | CAUGHT (adj) | MAKE SURE THAT THE<br>CABLE IS NOT<br>CAUGHT. | <br>Make sure that the cable<br>is not trapped. |
| **TRAVEL (n)** | The movement of an<br>item | MAKE SURE THAT THE<br>RANGE OF TRAVEL OF<br>THE CONTROL<br>SURFACES IS CLEAR. | <br> |

# Page 400 of 434

| **Word**<br>**(part of speech)** | **Approved meaning/**<br>**ALTERNATIVES** | **STE EXAMPLE** | **Non-STE example** |
|---|---|---|---|
| **travel (v) — UNNAPPROVED** | GO (v)<br>MOVE (v) | THE TURNBUCKLE<br>GOES THROUGH A<br>HOLE IN THE<br>BULKHEAD.<br>THE LEVER MOVES<br>THROUGH A 30-DEG.<br>ARC. | The turnbuckle travels<br>through a hole in the<br>bulkhead.<br>The lever travels through<br>a 30-deg. arc. |
| **treat (v) — UNNAPPROVED** | APPLY (v)<br>TOUCH (v) | APPLY WAX TO THE<br>SURFACE.<br>BE CAREFUL WHEN<br>YOU TOUCH PRINTED<br>CIRCUIT BOARDS. | Treat the surface with<br>wax.<br>Be careful when you<br>treat printed circuit<br>boards. |
| **trigger (v) — UNNAPPROVED** | CAUSE (v)<br>START (v) | HEAT CAUSES THE<br>PRESSURE TO<br>INCREASE.<br>THIS SIGNAL STARTS<br>THE OPERATION OF<br>THE TEST SET. | Heat triggers a pressure<br>increase.<br>This signal triggers test<br>set operation. |
| **trim (v) — UNNAPPROVED** | CUT (v) | CUT THE PATCH TO<br>THE CORRECT<br>DIMENSION. | Trim the patch to fit. |
| **trip (v) — UNNAPPROVED** | OPEN (v)<br>RELEASE (v)<br>CAUSE TO FALL | OPEN THE CIRCUIT<br>BREAKER.<br>THE HOLD-ON SWITCH<br>RELEASES.<br>AN IRREGULAR<br>SURFACE CAN CAUSE<br>YOU TO FALL. | Trip the circuit breaker.<br><br>Hold-on switch trips.<br>You can trip and fall on<br>an irregular surface. |
| **troubleshoot (v) — UNNAPPROVED** | TROUBLESHOOTING<br>(TN) | DO THE<br>TROUBLESHOOTING<br>PROCEDURE ON THE<br>VHF NAVIGATION<br>SYSTEM. | Troubleshoot the VHF<br>navigation system. |
| **true (adj) — UNNAPPROVED** | CORRECT (adj)<br>AGREE (v) | MAKE SURE THAT THE<br>VALUE SHOWN ON<br>THE INDICATOR IS<br>CORRECT.<br>MAKE SURE THAT THE<br>INDICATION ON THE<br>GAUGE AGREES WITH<br>THE QUANTITY OF<br>FUEL THAT IS IN THE<br>TANK. | Make sure that the<br>indicator reading is true.<br>Make sure that the<br>gauge shows the true<br>quantity of fuel that is in<br>the tank. |
