# Page 345–348 of 434

> **Source:** ASD-STE100 Issue 9, January 2025
> **Pages:** 345–348 of 434

# Page 345 of 434

| Word (part of speech) | Approved meaning/ALTERNATIVES | STE EXAMPLE | Non-STE example |
|---|---|---|---|
| **RECYCLE (v),**<br>**RECYCLES,**<br>**RECYCLED,**<br>**RECYCLED** | To put a used material<br>through a process to<br>make it possible to use it<br>or its components again<br>For other<br>meanings, use: CYCLE (n) | MAKE SURE THAT<br>YOU RECYCLE THE<br>REMOVED<br>INSULATION<br>MATERIAL.<br>DO ONE MORE TEST<br>CYCLE OF THE<br>COMPONENT. | Recycle the component<br>through a test. |
| **reduce (v) — UNNAPPROVED** | DECREASE (v) | SLOWLY DECREASE<br>THE SPEED. | Slowly reduce the<br>speed. |
| **REFER (v),**<br>**REFERS,**<br>**REFERRED,**<br>**REFERRED** | 1.<br>To tell a person<br>where to find<br>information<br>2.<br>To give information | REFER TO CHAPTER<br>28 FOR THE<br>INSTALLATION<br>PROCEDURE.<br>BEFORE YOU DO THIS<br>PROCEDURE,<br>ENGAGE THE RAMP<br>SERVICE DOOR<br>SAFETY CONNECTOR<br>PIN (THE PIN THAT:<br>HOLDS THE RAMP<br>SERVICE DOOR,<br>REFER TO IN THIS<br>PROCEDURE AS THE<br>“SAFETY CONNECTOR<br>PIN”). |  |
| **reference (n) — UNNAPPROVED** | REFER (v) | REFER TO<br>CHAPTER 20 FOR THE<br>STANDARD TORQUE<br>VALUES. | Reference is made to<br>Chapter 20 for the<br>standard torque values. |
| **referenced (adj) — UNNAPPROVED** | SHOW (v) | MAKE SURE THAT THE<br>GRAPH SHOWS THIS<br>POINT. | Make sure that this point<br>is referenced on the<br>graph. |
| **refill (v) — UNNAPPROVED** | FILL (v) | FILL THE CONTAINER<br>AGAIN. | Refill the container. |
| **refit (v) — UNNAPPROVED** | INSTALL (v) | INSTALL THE LINKAGE<br>AGAIN. | Refit the linkage. |
| REPAIR (v) | ON THE SUBMARINE,<br>REPAIR ALL DAMAGE<br>AND REPLACE ALL<br>WORN PARTS. | Refit the submarine. |  |

# Page 346 of 434

| Word (part of speech) | Approved meaning/ALTERNATIVES | STE EXAMPLE | Non-STE example |
|---|---|---|---|
| **reflect (v) — UNNAPPROVED** | REFLECTION (n) | THE RETICLE IMAGE<br>MAKES A REFLECTION<br>ON THE BOTTOM<br>SURFACE OF THE<br>GLASS. | The reticle image<br>reflects on the bottom<br>surface of the glass. |
| **REFLECTION (n)** | Something that occurs<br>when energy comes<br>against a surface which<br>sends it back | A CLEAN SURFACE<br>GIVES A BETTER<br>REFLECTION. |  |
| **REFUEL (v),**<br>**REFUELS,**<br>**REFUELED,**<br>**REFUELED** | To supply with fuel | REFUEL THE VEHICLE. |  |
| **register (v) — UNNAPPROVED** | SHOW (v) | ADJUST THE “SET +40”<br>CONTROL UNTIL THE<br>POINTER SHOWS +40. | Adjust the “SET +40”<br>control until the pointer<br>registers +40. |
| **regrease (v) — UNNAPPROVED** | APPLY (v)<br>MORE (adj) | APPLY GREASE TO<br>THE ROD AGAIN.<br>PUT MORE GREASE<br>ON THE JOINT UNTIL<br>YOU CAN MOVE IT. | Regrease the rod.<br>Regrease the joint until<br>you can move it. |
| **REGULAR (adj)** | At specified or equal<br>intervals | THE COMPUTER<br>GIVES REGULAR<br>INPUTS TO THE<br>CONTROL SYSTEM. |  |
| **REGULARLY (adv)** | In a regular manner | IF THE FAILURE<br>OCCURS REGULARLY,<br>DO A SYSTEM TEST. |  |
| **regulate (v) — UNNAPPROVED** | CONTROL (v)<br>ADJUST (v) | CONTROL THE<br>ELECTRICAL<br>CURRENT.<br>ADJUST THE TIRE<br>PRESSURE AS<br>NECESSARY. | Regulate the electrical<br>current.<br>Regulate the tire<br>pressure as necessary. |

# Page 347 of 434

| Word (part of speech) | Approved meaning/ALTERNATIVES | STE EXAMPLE | Non-STE example |
|---|---|---|---|
| **regulation (n) — UNNAPPROVED** | ADJUSTMENT (n)<br>CONTROL (n)<br>CONTROL (v) | THE TEMPERATURE<br>ADJUSTMENT IS<br>AUTOMATIC.<br>THE TEMPERATURE<br>CONTROL IS<br>AUTOMATIC.<br>A SENSOR CONTROLS<br>THE TEMPERATURE IN<br>THE COMPARTMENT. | The regulation of<br>temperature is<br>automatic.<br>The regulation of<br>temperature is<br>automatic.<br>The regulation of<br>temperature in the<br>compartment is effected<br>by a sensor. |
| **reinflate (v) — UNNAPPROVED** | INFLATE (v) | INFLATE THE TIRE<br>AGAIN. | Reinflate the tire. |
| **reinforce (v) — UNNAPPROVED** | MAKE … STRONGER | DOUBLERS MAKE THE<br>JOINT STRONGER. | Doublers reinforce the<br>joint. |
| **reinstall (v) — UNNAPPROVED** | INSTALL (v) | AFTER YOU ADJUST<br>THE UNIT, INSTALL<br>THE COVER AGAIN. | Reinstall the cover after<br>you adjust the unit. |
| **reinstallation (n) — UNNAPPROVED** | INSTALLATION (n) | ONLY APPROVED<br>PERSONNEL Can DO<br>THE INSTALLATION<br>PROCEDURE. | This reinstallation must<br>be performed by<br>qualified personnel. |
| **REJECT (v),**<br>**REJECTS,**<br>**REJECTED,**<br>**REJECTED** | To make a decision that<br>something is<br>unsatisfactory | REJECT THE PARTS<br>THAT ARE DAMAGED. |  |
| **rejection (n) — UNNAPPROVED** | REJECT (v) | IF THE TEST IS NOT<br>SATISFACTORY,<br>REJECT THE<br>COMPONENT. | Rejection is mandatory if<br>the test proves the<br>component to be<br>defective. |
| **relate (v) — UNNAPPROVED** | RELATED (adj) | THE PROCEDURES<br>ARE RELATED TO THE<br>SYSTEM TEST. | The procedures relate to<br>the system test. |
| **RELATED (adj)** | That has a relation | CLEAN THE BALLS OF<br>THE ELECTRICAL<br>LATCH AND ITS<br>RELATED SOCKETS. |  |
| **RELATION (n)** | The connection between<br>two or more things<br>caused by their<br>functions, values, or<br>conditions | THE RELATION<br>BETWEEN THE TWO<br>CONTROL SYSTEMS<br>KEEPS THE AIRCRAFT<br>STABLE. |  |

# Page 348 of 434

| Word (part of speech) | Approved meaning/ALTERNATIVES | STE EXAMPLE | Non-STE example |
|---|---|---|---|
| **relay (v) — UNNAPPROVED** | SEND (v) | SEND THE<br>INFORMATION TO THE<br>ENGINEERING<br>DEPARTMENT. | Relay the information to<br>the engineering<br>department. |
| **RELEASE (v),**<br>**RELEASES,**<br>**RELEASED,**<br>**RELEASED** | To make free, to let go | RELEASE THE<br>INSTRUMENT PANEL<br>TO GET ACCESS TO<br>THE CONNECTIONS. |  |
| **relevant (adj) — UNNAPPROVED** | RELATED (adj)<br>THEIR (adj)<br>ITS (adj) | REMOVE THE ROD<br>END FROM THE<br>RELATED PIVOT.<br>INSTALL THE BOLTS<br>IN THEIR HOLES.<br>INSTALL THE<br>COMPUTER IN ITS<br>RACK. | Withdraw the rod end<br>from the relevant pivot.<br>Install the bolts in the<br>relevant holes.<br>Install the computer in<br>the relevant rack. |
| **relieve (v) — UNNAPPROVED** | RELEASE (v) | RELEASE THE<br>TENSION IN THE<br>CABLE. | Relieve the tension in<br>the cable. |
| **remain (v) — UNNAPPROVED** | STAY (v) | THE FLAGS MUST<br>STAY OUT OF VIEW. | The flags must remain<br>out of view. |
| **REMAINING (adj)** | That continues to stay | REMOVE THE<br>REMAINING SEALANT<br>WITH SOLVENT. |  |
| **remnant (n) — UNNAPPROVED** | REMAINING (adj) | REMOVE THE<br>REMAINING SEALANT<br>FROM THE FLOOR<br>COVERING. | Remove sealant<br>remnants from the floor<br>covering. |
| **removable (adj) — UNNAPPROVED** | REMOVE (v) | FIND THE PART OF<br>THE BARREL THAT<br>YOU CAN REMOVE. | Find the removable part<br>of the barrel. |
| **REMOVAL (n)** | A procedure which<br>removes an object | THE SUPERVISOR<br>MUST GIVE THE<br>APPLICABLE<br>PROCEDURE FOR<br>CORROSION<br>REMOVAL. |  |
| **REMOVE (v),**<br>**REMOVES,**<br>**REMOVED,**<br>**REMOVED** | To take or move<br>something away from its<br>initial position | REMOVE THE<br>INDICATOR FROM THE<br>PANEL. |  |
| **render (v) — UNNAPPROVED** | MAKE (v) | MAKE THE SYSTEM<br>ELECTRICALLY SAFE. | Render the system<br>electrically safe. |
